{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Series 700"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Series 700","index":0,"n_rows":179,"n_cols":4,"rows_kept":179,"cut":false,"hidden":false,"merged":[]}
["ITEM","DESCRIPTION","UNIT","RATE"]
["","Series 700 PAVEMENTS (Scope Paragraph 18.6.1)"]
["","Repairs and Patching"]
["","Local Repairs not exceeding 5 number Local Repairs per Task;"]
["1","In carriageways.","kg"]
["2","In footways.","kg"]
["","Local Repairs exceeding 5 but not exceeding 20 number Local Repairs per Task;"]
["3","In carriageways.","kg"]
["4","In footways.","kg"]
["","Local Repairs exceeding 20 number Local Repairs per Task;"]
["5","In carriageways.","kg"]
["6","In footways.","kg"]
["","Hand Lay Patching"]
["","Patching; Hand lay; not exceeding 10 square metres of patching per Task;"]
["","Individual patch area not exceeding 1 square metre; in carriageways;"]
["7","Material ref: WC1 or WC2; layer not exceeding 50mm thick","m2"]
["8","Material ref: WC1 or WC2; layer not exceeding 50mm thick laid over material refs BC1 or BC3 layer not exceeding 100mm thick; combined thickness not exceeding 150mm.","m2"]
["9","Material ref: WC1 or WC2; layer not exceeding 50mm thick laid over material refs BC1 or BC3 layer not exceeding 100mm thick laid over material refs: BA1 or BA3 layer not exceeding 200mm thick; combined thickness not exceeding 350mm.","m2"]
["","Individual patch area not exceeding 5 square metres; in footways and paved areas;"]
["10","Material ref: PWC1 or FWC1; layer not exceeding 25mm thick","m2"]
["11","Material ref: PWC1 or FWC1; layer not exceeding 25mm thick laid over material refs PBC1 or FBC1 layer not exceeding 75mm thick; combined thickness not exceeding 100mm.","m2"]
["","Individual patch area exceeding 5 square metres but not exceeding 10 square metres; in footways and paved areas;"]
["12","Material ref: PWC1 or FWC1; layer not exceeding 25mm thick","m2"]
["13","Material ref: PWC1 or FWC1; layer not exceeding 25mm thick laid over material refs PBC1 or FBC1 layer not exceeding 75mm thick; combined thickness not exceeding 100mm.","m2"]
["","Patching; Hand lay; exceeding 10 square metres but not exceeding 20 square metres of patching per Task;"]
["","Individual patch area not exceeding 1 square metre; in carriageways;"]
["14","Material ref: WC1 or WC2; layer not exceeding 50mm thick","m2"]
["15","Material ref: WC1 or WC2; layer not exceeding 50mm thick laid over material refs BC1 or BC3 layer not exceeding 100mm thick; combined thickness not exceeding 150mm.","m2"]
["16","Material ref: WC1 or WC2; layer not exceeding 50mm thick laid over material refs BC1 or BC3 layer not exceeding 100mm thick laid over material refs: BA1 or BA3 layer not exceeding 200mm thick; combined thickness not exceeding 350mm.","m2"]
["","Individual patch area not exceeding 5 square metres; in footways and paved areas;"]
["17","Material ref: PWC1 or FWC1; layer not exceeding 25mm thick","m2"]
["18","Material ref: PWC1 or FWC1; layer not exceeding 25mm thick laid over material refs PBC1 or FBC1 layer not exceeding 75mm thick; combined thickness not exceeding 100mm.","m2"]
["","Individual patch area exceeding 5 square metres but not exceeding 10 square metres; in footways and paved areas;"]
["19","Material ref: PWC1 or FWC1; layer not exceeding 25mm thick","m2"]
["20","Material ref: PWC1 or FWC1; layer not exceeding 25mm thick laid over material refs PBC1 or FBC1 layer not exceeding 75mm thick; combined thickness not exceeding 100mm.","m2"]
["","Individual patch area exceeding 10 square metres but not exceeding 15 square metres; in footways and paved areas;"]
["21","Material ref: PWC1 or FWC1; layer not exceeding 25mm thick","m2"]
["22","Material ref: PWC1 or FWC1; layer not exceeding 25mm thick laid over material refs PBC1 or FBC1 layer not exceeding 75mm thick; combined thickness not exceeding 100mm.","m2"]
["","Individual patch area exceeding 15 square metres but not exceeding 20 square metres; in footways and paved areas;"]
["23","Material ref: PWC1 or FWC1; layer not exceeding 25mm thick","m2"]
["24","Material ref: PWC1 or FWC1; layer not exceeding 25mm thick laid over material refs PBC1 or FBC1 layer not exceeding 75mm thick; combined thickness not exceeding 100mm.","m2"]
["","Patching; Hand lay; exceeding 20 square metres but not exceeding 50 square metres of patching per Task;"]
["","Individual patch area not exceeding 1 square metre; in carriageways;"]
["25","Material ref: WC1 or WC2; layer not exceeding 50mm thick","m2"]
["26","Material ref: WC1 or WC2; layer not exceeding 50mm thick laid over material refs BC1 or BC3 layer not exceeding 100mm thick; combined thickness not exceeding 150mm.","m2"]
["27","Material ref: WC1 or WC2; layer not exceeding 50mm thick laid over material refs BC1 or BC3 layer not exceeding 100mm thick laid over material refs: BA1 or BA3 layer not exceeding 200mm thick; combined thickness not exceeding 350mm.","m2"]
["","Individual patch area not exceeding 5 square metres; in footways and paved areas;"]
["28","Material ref: PWC1 or FWC1; layer not exceeding 25mm thick","m2"]
["29","Material ref: PWC1 or FWC1; layer not exceeding 25mm thick laid over material refs PBC1 or FBC1 layer not exceeding 75mm thick; combined thickness not exceeding 100mm.","m2"]
["","Individual patch area exceeding 5 square metres but not exceeding 10 square metres; in footways and paved areas;"]
["30","Material ref: PWC1 or FWC1; layer not exceeding 25mm thick","m2"]
["31","Material ref: PWC1 or FWC1; layer not exceeding 25mm thick laid over material refs PBC1 or FBC1 layer not exceeding 75mm thick; combined thickness not exceeding 100mm.","m2"]
["","Individual patch area exceeding 10 square metres but not exceeding 15 square metres; in footways and paved areas;"]
["32","Material ref: PWC1 or FWC1; layer not exceeding 25mm thick","m2"]
["33","Material ref: PWC1 or FWC1; layer not exceeding 25mm thick laid over material refs PBC1 or FBC1 layer not exceeding 75mm thick; combined thickness not exceeding 100mm.","m2"]
["","Individual patch area exceeding 15 square metres but not exceeding 20 square metres; in footways and paved areas;"]
["34","Material ref: PWC1 or FWC1; layer not exceeding 25mm thick","m2"]
["35","Material ref: PWC1 or FWC1; layer not exceeding 25mm thick laid over material refs PBC1 or FBC1 layer not exceeding 75mm thick; combined thickness not exceeding 100mm.","m2"]
["","Individual patch area exceeding 20 square metres but not exceeding 50 square metres; in footways and paved areas;"]
["36","Material ref: PWC1 or FWC1; layer not exceeding 25mm thick","m2"]
["37","Material ref: PWC1 or FWC1; layer not exceeding 25mm thick laid over material refs PBC1 or FBC1 layer not exceeding 75mm thick; combined thickness not exceeding 100mm.","m2"]
["","Patching; Hand lay; exceeding 50 square metres of patching per Task;"]
["","Individual patch area not exceeding 1 square metre; in carriageways;"]
["38","Material ref: WC1 or WC2; layer not exceeding 50mm thick","m2"]
["39","Material ref: WC1 or WC2; layer not exceeding 50mm thick laid over material refs BC1 or BC3 layer not exceeding 100mm thick; combined thickness not exceeding 150mm.","m2"]
["40","Material ref: WC1 or WC2; layer not exceeding 50mm thick laid over material refs BC1 or BC3 layer not exceeding 100mm thick laid over material refs: BA1 or BA3 layer not exceeding 200mm thick; combined thickness not exceeding 350mm.","m2"]
["","Individual patch area not exceeding 5 square metres; in footways and paved areas;"]
["41","Material ref: PWC1 or FWC1; layer not exceeding 25mm thick","m2"]
["42","Material ref: PWC1 or FWC1; layer not exceeding 25mm thick laid over material refs PBC1 or FBC1 layer not exceeding 75mm thick; combined thickness not exceeding 100mm.","m2"]
["","Individual patch area exceeding 5 square metres but not exceeding 10 square metres; in footways and paved areas;"]
["43","Material ref: PWC1 or FWC1; layer not exceeding 25mm thick","m2"]
["44","Material ref: PWC1 or FWC1; layer not exceeding 25mm thick laid over material refs PBC1 or FBC1 layer not exceeding 75mm thick; combined thickness not exceeding 100mm.","m2"]
["","Individual patch area exceeding 10 square metres but not exceeding 15 square metres; in footways and paved areas;"]
["45","Material ref: PWC1 or FWC1; layer not exceeding 25mm thick","m2"]
["46","Material ref: PWC1 or FWC1; layer not exceeding 25mm thick laid over material refs PBC1 or FBC1 layer not exceeding 75mm thick; combined thickness not exceeding 100mm.","m2"]
["","Individual patch area exceeding 15 square metres but not exceeding 20 square metres; in footways and paved areas;"]
["47","Material ref: PWC1 or FWC1; layer not exceeding 25mm thick","m2"]
["48","Material ref: PWC1 or FWC1; layer not exceeding 25mm thick laid over material refs PBC1 or FBC1 layer not exceeding 75mm thick; combined thickness not exceeding 100mm.","m2"]
["","Individual patch area exceeding 20 square metres but not exceeding 50 square metres; in footways and paved areas;"]
["49","Material ref: PWC1 or FWC1; layer not exceeding 25mm thick","m2"]
["50","Material ref: PWC1 or FWC1; layer not exceeding 25mm thick laid over material refs PBC1 or FBC1 layer not exceeding 75mm thick; combined thickness not exceeding 100mm.","m2"]
["","Individual patch area exceeding 50 square metres; in footways and paved areas;"]
["51","Material ref: PWC1 or FWC1; layer not exceeding 25mm thick","m2"]
["52","Material ref: PWC1 or FWC1; layer not exceeding 25mm thick laid over material refs PBC1 or FBC1 layer not exceeding 75mm thick; combined thickness not exceeding 100mm.","m2"]
["","Patching; Machine lay; exceeding 10 square metres but not exceeding 20 square metres of patching per Task;"]
["","Individual patch area not exceeding 5 square metres; in carriageways;"]
["53","Material ref: WC1 or WC2; layer not exceeding 50mm thick","m2"]
["54","Material refs: WC1 or WC2; layer not exceeding 50mm thick laid over material refs BC1 or BC3 layer not exceeding 100mm thick; combined thickness not exceeding 150mm.","m2"]
["55","Material refs: WC1 or WC2; layer not exceeding 50mm thick laid over material refs BC1 or BC3 layer not exceeding 100mm thick laid over material refs: BA1 or BA3 layer not exceeding 200mm thick; combined thickness not exceeding 350mm.","m2"]
["","Individual patch area exceeding 5 square metres but not exceeding 10 square metres; in carriageways;"]
["56","Material ref: WC1 or WC2; layer not exceeding 50mm thick","m2"]
["57","Material refs: WC1 or WC2; layer not exceeding 50mm thick laid over material refs BC1 or BC3 layer not exceeding 100mm thick; combined thickness not exceeding 150mm.","m2"]
["58","Material refs: WC1 or WC2; layer not exceeding 50mm thick laid over material refs BC1 or BC3 layer not exceeding 100mm thick laid over material refs: BA1 or BA3 layer not exceeding 200mm thick; combined thickness not exceeding 350mm.","m2"]
["59","Material ref: WC5; layer not exceeding 50mm thick","m2"]
["60","Material refs: WC5; layer not exceeding 50mm thick laid over material refs BC1 or BC3 layer not exceeding 100mm thick; combined thickness not exceeding 150mm.","m2"]
["61","Material refs: WC5; layer not exceeding 50mm thick laid over material refs BC1 or BC3 layer not exceeding 100mm thick laid over material refs:  BA1 or BA3 layer not exceeding 200mm thick; combined thickness not exceeding 350mm.","m2"]
["62","Material ref: WC6; layer not exceeding 50mm thick","m2"]
["63","Material refs: WC6; layer not exceeding 50mm thick laid over material refs BC1 or BC3 layer not exceeding 100mm thick; combined thickness not exceeding 150mm.","m2"]
["64","Material refs: WC6; layer not exceeding 50mm thick laid over material refs BC1 or BC3 layer not exceeding 100mm thick laid over material refs:  BA1 or BA3 layer not exceeding 200mm thick; combined thickness not exceeding 350mm.","m2"]
["65","Material ref: WC8; layer not exceeding 50mm thick","m2"]
["66","Material refs: WC8; layer not exceeding 50mm thick laid over material refs BC1 or BC3 layer not exceeding 100mm thick; combined thickness not exceeding 150mm.","m2"]
["67","Material refs: WC8; layer not exceeding 50mm thick laid over material refs BC1 or BC3 layer not exceeding 100mm thick laid over material refs:  BA1 or BA3 layer not exceeding 200mm thick; combined thickness not exceeding 350mm.","m2"]
["","Individual patch area exceeding 10 square metres but not exceeding 15 square metres; in carriageways;"]
["68","Material ref: WC1 or WC2; layer not exceeding 50mm thick","m2"]
["69","Material refs: WC1 or WC2; layer not exceeding 50mm thick laid over material refs BC1 or BC3 layer not exceeding 100mm thick; combined thickness not exceeding 150mm.","m2"]
["70","Material refs: WC1 or WC2; layer not exceeding 50mm thick laid over material refs BC1 or BC3 layer not exceeding 100mm thick laid over material refs: BA1 or BA3 layer not exceeding 200mm thick; combined thickness not exceeding 350mm.","m2"]
["71","Material ref: WC5; layer not exceeding 50mm thick","m2"]
["72","Material refs: WC5; layer not exceeding 50mm thick laid over material refs BC1 or BC3 layer not exceeding 100mm thick; combined thickness not exceeding 150mm.","m2"]
["73","Material refs: WC5; layer not exceeding 50mm thick laid over material refs BC1 or BC3 layer not exceeding 100mm thick laid over material refs:  BA1 or BA3 layer not exceeding 200mm thick; combined thickness not exceeding 350mm.","m2"]
["74","Material ref: WC6; layer not exceeding 50mm thick","m2"]
["75","Material refs: WC6; layer not exceeding 50mm thick laid over material refs BC1 or BC3 layer not exceeding 100mm thick; combined thickness not exceeding 150mm.","m2"]
["76","Material refs: WC6; layer not exceeding 50mm thick laid over material refs BC1 or BC3 layer not exceeding 100mm thick laid over material refs:  BA1 or BA3 layer not exceeding 200mm thick; combined thickness not exceeding 350mm.","m2"]
["77","Material ref: WC8; layer not exceeding 50mm thick","m2"]
["78","Material refs: WC8; layer not exceeding 50mm thick laid over material refs BC1 or BC3 layer not exceeding 100mm thick; combined thickness not exceeding 150mm.","m2"]
["79","Material refs: WC8; layer not exceeding 50mm thick laid over material refs BC1 or BC3 layer not exceeding 100mm thick laid over material refs:  BA1 or BA3 layer not exceeding 200mm thick; combined thickness not exceeding 350mm.","m2"]
["","Individual patch area exceeding 15 square metres but not exceeding 20 square metres; in carriageways;"]
["80","Material ref: WC1 or WC2; layer not exceeding 50mm thick","m2"]
["81","Material refs: WC1 or WC2; layer not exceeding 50mm thick laid over material refs BC1 or BC3 layer not exceeding 100mm thick; combined thickness not exceeding 150mm.","m2"]
["82","Material refs: WC1 or WC2; layer not exceeding 50mm thick laid over material refs BC1 or BC3 layer not exceeding 100mm thick laid over material refs: BA1 or BA3 layer not exceeding 200mm thick; combined thickness not exceeding 350mm.","m2"]
["83","Material ref: WC5; layer not exceeding 50mm thick","m2"]
["84","Material refs: WC5; layer not exceeding 50mm thick laid over material refs BC1 or BC3 layer not exceeding 100mm thick; combined thickness not exceeding 150mm.","m2"]
["85","Material refs: WC5; layer not exceeding 50mm thick laid over material refs BC1 or BC3 layer not exceeding 100mm thick laid over material refs:  BA1 or BA3 layer not exceeding 200mm thick; combined thickness not exceeding 350mm.","m2"]
["86","Material ref: WC6; layer not exceeding 50mm thick","m2"]
["87","Material refs: WC6; layer not exceeding 50mm thick laid over material refs BC1 or BC3 layer not exceeding 100mm thick; combined thickness not exceeding 150mm.","m2"]
["88","Material refs: WC6; layer not exceeding 50mm thick laid over material refs BC1 or BC3 layer not exceeding 100mm thick laid over material refs:  BA1 or BA3 layer not exceeding 200mm thick; combined thickness not exceeding 350mm.","m2"]
["89","Material ref: WC8; layer not exceeding 50mm thick","m2"]
["90","Material refs: WC8; layer not exceeding 50mm thick laid over material refs BC1 or BC3 layer not exceeding 100mm thick; combined thickness not exceeding 150mm.","m2"]
["91","Material refs: WC8; layer not exceeding 50mm thick laid over material refs BC1 or BC3 layer not exceeding 100mm thick laid over material refs:  BA1 or BA3 layer not exceeding 200mm thick; combined thickness not exceeding 350mm.","m2"]
["","Patching; Machine lay; exceeding 20 square metres but not exceeding 50 square metres of patching per Task;"]
["","Individual patch area not exceeding 5 square metres; in carriageways;"]
["92","Material ref: WC1 or WC2; layer not exceeding 50mm thick","m2"]
["93","Material refs: WC1 or WC2; layer not exceeding 50mm thick laid over material refs BC1 or BC3 layer not exceeding 100mm thick; combined thickness not exceeding 150mm.","m2"]
["94","Material refs: WC1 or WC2; layer not exceeding 50mm thick laid over material refs BC1 or BC3 layer not exceeding 100mm thick laid over material refs: BA1 or BA3 layer not exceeding 200mm thick; combined thickness not exceeding 350mm.","m2"]
["","Individual patch area exceeding 5 square metres but not exceeding 10 square metres; in carriageways;"]
["95","Material ref: WC1 or WC2; layer not exceeding 50mm thick","m2"]
["96","Material refs: WC1 or WC2; layer not exceeding 50mm thick laid over material refs BC1 or BC3 layer not exceeding 100mm thick; combined thickness not exceeding 150mm.","m2"]
["97","Material refs: WC1 or WC2; layer not exceeding 50mm thick laid over material refs BC1 or BC3 layer not exceeding 100mm thick laid over material refs: BA1 or BA3 layer not exceeding 200mm thick; combined thickness not exceeding 350mm.","m2"]
["","Individual patch area exceeding 10 square metres but not exceeding 15 square metres; in carriageways;"]
["98","Material ref: WC1 or WC2; layer not exceeding 50mm thick","m2"]
["99","Material refs: WC1 or WC2; layer not exceeding 50mm thick laid over material refs BC1 or BC3 layer not exceeding 100mm thick; combined thickness not exceeding 150mm.","m2"]
["100","Material refs: WC1 or WC2; layer not exceeding 50mm thick laid over material refs BC1 or BC3 layer not exceeding 100mm thick laid over material refs: BA1 or BA3 layer not exceeding 200mm thick; combined thickness not exceeding 350mm.","m2"]
["","Individual patch area exceeding 15 square metres but not exceeding 20 square metres; in carriageways;"]
["101","Material ref: WC1 or WC2; layer not exceeding 50mm thick","m2"]
["102","Material refs: WC1 or WC2; layer not exceeding 50mm thick laid over material refs BC1 or BC3 layer not exceeding 100mm thick; combined thickness not exceeding 150mm.","m2"]
["103","Material refs: WC1 or WC2; layer not exceeding 50mm thick laid over material refs BC1 or BC3 layer not exceeding 100mm thick laid over material refs: BA1 or BA3 layer not exceeding 200mm thick; combined thickness not exceeding 350mm.","m2"]
["","Individual patch area exceeding 20 square metres but not exceeding 50 square metres; in carriageways;"]
["104","Material ref: WC1 or WC2; layer not exceeding 50mm thick","m2"]
["105","Material refs: WC1 or WC2; layer not exceeding 50mm thick laid over material refs BC1 or BC3 layer not exceeding 100mm thick; combined thickness not exceeding 150mm.","m2"]
["106","Material refs: WC1 or WC2; layer not exceeding 50mm thick laid over material refs BC1 or BC3 layer not exceeding 100mm thick laid over material refs: BA1 or BA3 layer not exceeding 200mm thick; combined thickness not exceeding 350mm.","m2"]
["","Patching; Machine lay; exceeding 50 square metres of patching per Task;"]
["","Individual patch area not exceeding 5 square metres; in carriageways;"]
["107","Material ref: WC1 or WC2; layer not exceeding 50mm thick","m2"]
["108","Material refs: WC1 or WC2; layer not exceeding 50mm thick laid over material refs BC1 or BC3 layer not exceeding 100mm thick; combined thickness not exceeding 150mm.","m2"]
["109","Material refs: WC1 or WC2; layer not exceeding 50mm thick laid over material refs BC1 or BC3 layer not exceeding 100mm thick laid over material refs: BA1 or BA3 layer not exceeding 200mm thick; combined thickness not exceeding 350mm.","m2"]
["","Individual patch area exceeding 5 square metres but not exceeding 10 square metres; in carriageways;"]
["110","Material ref: WC1 or WC2; layer not exceeding 50mm thick","m2"]
["111","Material refs: WC1 or WC2; layer not exceeding 50mm thick laid over material refs BC1 or BC3 layer not exceeding 100mm thick; combined thickness not exceeding 150mm.","m2"]
["112","Material refs: WC1 or WC2; layer not exceeding 50mm thick laid over material refs BC1 or BC3 layer not exceeding 100mm thick laid over material refs: BA1 or BA3 layer not exceeding 200mm thick; combined thickness not exceeding 350mm.","m2"]
["","Individual patch area exceeding 10 square metres but not exceeding 15 square metres; in carriageways;"]
["113","Material ref: WC1 or WC2; layer not exceeding 50mm thick","m2"]
["114","Material refs: WC1 or WC2; layer not exceeding 50mm thick laid over material refs BC1 or BC3 layer not exceeding 100mm thick; combined thickness not exceeding 150mm.","m2"]
["115","Material refs: WC1 or WC2; layer not exceeding 50mm thick laid over material refs BC1 or BC3 layer not exceeding 100mm thick laid over material refs: BA1 or BA3 layer not exceeding 200mm thick; combined thickness not exceeding 350mm.","m2"]
["","Individual patch area exceeding 15 square metres but not exceeding 20 square metres; in carriageways;"]
["116","Material ref: WC1 or WC2; layer not exceeding 50mm thick","m2"]
["117","Material refs: WC1 or WC2; layer not exceeding 50mm thick laid over material refs BC1 or BC3 layer not exceeding 100mm thick; combined thickness not exceeding 150mm.","m2"]
["118","Material refs: WC1 or WC2; layer not exceeding 50mm thick laid over material refs BC1 or BC3 layer not exceeding 100mm thick laid over material refs: BA1 or BA3 layer not exceeding 200mm thick; combined thickness not exceeding 350mm.","m2"]
["","Individual patch area exceeding 20 square metres but not exceeding 50 square metres; in carriageways;"]
["119","Material ref: WC1 or WC2; layer not exceeding 50mm thick","m2"]
["120","Material refs: WC1 or WC2; layer not exceeding 50mm thick laid over material refs BC1 or BC3 layer not exceeding 100mm thick; combined thickness not exceeding 150mm.","m2"]
["121","Material refs: WC1 or WC2; layer not exceeding 50mm thick laid over material refs BC1 or BC3 layer not exceeding 100mm thick laid over material refs: BA1 or BA3 layer not exceeding 200mm thick; combined thickness not exceeding 350mm.","m2"]
["","Individual patch area exceeding  50 square metres; in carriageways;"]
["122","Material ref: WC1 or WC2; layer not exceeding 50mm thick","m2"]
["123","Material refs: WC1 or WC2; layer not exceeding 50mm thick laid over material refs BC1 or BC3 layer not exceeding 100mm thick; combined thickness not exceeding 150mm.","m2"]
["124","Material refs: WC1 or WC2; layer not exceeding 50mm thick laid over material refs BC1 or BC3 layer not exceeding 100mm thick laid over material refs: BA1 or BA3 layer not exceeding 200mm thick; combined thickness not exceeding 350mm.","m2"]
[]
[null,"Note: Above rates are based on Mon to Fri 0700-1900hrs"]
[]
[null,"Out of Hours Uplift for Night Working (Mon to Fri 1900-0700hrs)","%"]
[null,"Out of Hours Uplift for Weekend Working (0700hrs on Sat to 0700 on Mon)","%"]