Clarifications to Bidder’s Questions:

Section 38 Whixall Manor Drain Diversion Completion

|  |  |  |
| --- | --- | --- |
| 1 | Annex 2 shows a “New crossing point” on the map, but it is not referred to elsewhere in the documentation. | Annex 2 map shows a New crossing point. This is no longer required. This is why it is not referred to on any of the other documentation or Annexes. |
| 2 | This was about the levels for the 10m turn into the Whixall Main drain at the western end of the Diversion. “Is there any room for manoeuvre on the Diversion ditch line toward where the diversion will re-join the Whixall Moss Main Drain? There was concern that the 10m radial bend would go up hill into section 38, this would need significantly more excavation than if it dropped a few metres north of the fence line then turned. “  I have consulted with the Designer who said “I don’t have a problem with re-positioning the outlet from the Diversion. We were just keeping it out of the peat.” | At the western end of the Diversion, where it enters the Whixall Moss Main Drain, a 10m curve is specified, so the two flows of water will join seamlessly (Annex 4). The Drain must be cut “in the dry” leaving 5m to minimise sedimentation and pollution downstream. However, the Diversion can be moved a few meters north and then curved into the Main Drain to avoid cutting too deeply into the southern ridge, as long as the levels in the Diversion work. |