GLOBAL WAR GALLERY

**NATIONAL ARMY MUSEUM**

**Graphics Specification and Graphics Schedule**

Produced by

**STUDIOHB Ltd**

**FEBRUARY 2022**

**PRELIMS:**

Graphic production generic specification

To be read with Preliminaries/General Conditions and the Pricing Document.

### **A General Requirements**

1. The specification outlines the Designers' intentions. The Designers are happy to be advised of cost savings made as a result of changes to the production methods provided that these do not compromise the integrity of the design and the durability of the finishes.
2. The Graphics Contractor should indicate in the Pricing Document the cost of all Graphic Production and Installation (unless otherwise stated).
3. It is suggested that where the Contractor for graphic application supplies panels they will be delivered to the Graphic Contractor at the cost of the Contractor. Completed panels will be returned to the Contractor or to site at the cost of the Graphic Contractor.
4. The Graphic contractor shall be responsible for ensuring that all items are packaged and stored in accordance with any special requirements for particular materials. The Graphic contractor will be responsible for the general packaging and safe storage of all items so that the items will be adequately protected against damage in both storage and transit.
5. The Graphic contractor shall anticipate the possible sources of damage to these works and to existing works and shall take active and positive prospective measures to the satisfaction of the Designer. Protective devices shall protect the works against damage arising from weather conditions, construction, other contractors, warping, distortion, abrasion, sunlight, humidity or other conditions that could have an adverse effect on the works.
6. Graphics indicated on the Drawings contained in the documentation and in the samples provided, show design intent and give the overall aesthetic that is required. Final sizes may vary.
7. The Graphic contractor shall be required to supply samples of each product for approval by the designer. A duplicate of the approved product shall be retained by the Client for future reference in event of any contractual dispute regarding the material or finished quality of products supplied under the con- tract.
8. Samples need to be provided of all colours for all substrates. All colour references will refer to the PANTONE COLOUR MATCHING SYSTEM and need to be matched as closely as possible and to the satisfaction of the designer.
9. Prior to the production the Graphic contractor will submit to the designer a sample of each type of digital output and printing at relevant size, which are relevant to those products, which the Graphic contractor will be contracted to supply:

Foamex lettering, Title lettering, Story panels, section panels, captions

1. All products and materials described in the specification shall be covered by a full performance guaranteed for a hard wearing permanent exhibition. The guarantee period shall commence from the date of completion of the contract.
2. Visual elements including the materials – self coloured and applied colour and graphics shall not show symptoms of colour fade, degradation, embrittlement or substrate interaction as a result of ageing and/or exposure to daylight, artificial light, climatic and local environmental conditions such that the colours change beyond the material manufacturer’s expected tolerances within the minimum life expectancy period.
3. The Graphic contractor shall be responsible for ensuring that all colour-finishing materials are compatible with the material and/or substrate to which they are applied. Compatibility includes all aspects of colour finish in respect of ageing, colour fastness, light reflectiveness and physical and chemical properties such as the performance when applied shall at least be equal to the performance standards quoted by the manufacturer of the colour finishing material.
4. All sizes shown are for pricing only and are to a certain extent indicative areas and quantities of graphics in any location may be exchanged on a like for like basis during the Artwork process
5. The exact sizes quantities and types of the graphics required following ongoing detailed graphic design will vary. The contractor and graphic subcontractor are to expect such variation and provide alternatives on a pro rata basis.

### **B Graphic Production**

1. The quality of work and the materials used in production must be of the highest standards and conform to relevant British Standards. All materials must be used in accordance either their manufacturers' instructions to ensure maximum durability.
2. It is the responsibility of the Graphics Contractor to ensure that all surfaces are suitable for stencil and paint treatment and should provide any necessary preparatory work prior to application of graphics.
3. Where self-adhesive vinyl is specified, material of a high quality is required. A vinyl should be of a durable nature, preferably with a 10-year life span. A colour chart and samples form the vinyl ranges to be used together with associated technical support information should be supplied to the client for approval.
4. All fixing details to be as per construction specification.
5. Acrylic and Plexiglas are the same material.
6. All vinyl films, including their adhesive must be compatible with the material and/or substrate to which they are applied. Compatibility includes all aspects of colour in respect of ageing, colourfastness, light reflectants and physical and chemical properties.
7. Scanned photographs and illustrations must be high resolution.
8. Screen inks and stencilled printed on exposed surfaces are to be twin pack epoxy inks compatible with the material on to which they are being printed. Where necessary a sample will be provided by the Graphic contractor for approval of the graphic treatment by the Contract Administrator. Inks should be matched to a "Pantone Colour Matching System" reference.
9. All powder coating, spray painting, stenciling and silk-screening is to be carried out fully in accordance with the manufacturers recommendation for each particular combination of substrate material/surface, surface preparation and paint or print process and paint or paint medium.
10. Overall panel areas have been supplied - these are to be divided into standard widths.
11. All substrates used in panel production (e.g. Foamex, MDF) are to be fire rated to a minimum Class 1.
12. All MDF/ply panels are to be counter balanced to prevent ‘bowing’.
13. All Foamex and MDF graphics not under glass sheet panels should be matt wrap heatsealed unless specified. Allow for split bonding/battening through- out.
14. All visible MDF edges should be painted black unless otherwise indicated.
15. All toughened glass to be subjected to "heat- soak" process.

### **SPECIFICATION NAM GLOBAL WAR**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Outline Description** | **Panel code** | **Panel size & Mounting (w x h)** | **Method of production** | **Cost** | **Notes** |
| **ENTRANCE** |  |  |  |  |  |
| ENTRANCE WALL | GW.E.1.1.G1 | 1872mm (w) x 2380mm (h)  Allow 100mm bleed | DTM to graphic soundproof stretched fabric. Allow for applied elements such as fire safety sign and sponsorship panel |  | Material spec to be confirmed by NAM and to match existing acoustic specification. |
| GALLERY TITLE | GW.T&E.1.1.G1 | 794mm (w) x 2392mm (h) | DTM to 3M matt self adhesive vinyl. Apply to sanded, smoothed and sealed MDF panel. |  | MDF supplied by main contractor |
| **ELEVATION 1**  TRADE AND EMPIRE |  |  |  |  |  |
| Horizontal text panel | GW.T&E.2.1.G1 | 1419mm (w) x 497mm (h) | DTM to 3M matt self adhesive vinyl. Apply to sanded, smoothed and sealed MDF panel. See 3D drawing for fixing details. |  | MDF supplied by main contractor |
| Section text panel top | GW.T&E.2.2.G1a | 494mm (w) x 1594mm (h) | DTM to 3M matt self adhesive vinyl. Apply to sanded, smoothed and sealed MDF panel. See 3D drawing for fixing details. |  | MDF supplied by main contractor |
| Section image panel | GW.T&E.2.2.G1b | 494mm (w) x 795mm (h) | DTM to 3M matt self adhesive vinyl. Apply to sanded, smoothed and sealed MDF panel. See 3D drawing for fixing details. |  | MDF supplied by main contractor |
| Section quote vinyl | GW.T&E.2.2.G2 | To cover approx area: 1466mm (w) x 200mm (h) | DTM in 1no colour on to 3M matt self adhesive vinyl. Laser cut letter and apply on site to 1no painted MDF panel. |  |  |
| Section text panel top | GW.T&E.2.3.G1a | 494mm (w) x 1594mm (h) | DTM to 3M matt self adhesive vinyl. Apply to sanded, smoothed and sealed MDF panel. See 3D drawing for fixing details. |  | MDF supplied by main contractor |
| Section image panel | GW.T&E.2.3.G1b | 494mm (w) x 795mm (h) | DTM to 3M matt self adhesive vinyl. Apply to sanded, smoothed and sealed MDF panel. See 3D drawing for fixing details. |  | MDF supplied by main contractor |
| Section quote vinyl | GW.T&E.2.3.G2 | To cover approx area: 1466mm (w) x 200mm (h) | DTM in 1no colour on to 3M matt self adhesive vinyl. Laser cut letter and apply on site to 1no painted MDF panel. |  |  |
| **ELEVATION 2** |  |  |  |  |  |
| Section quote vinyl | GW.T&E.2.3.G3&4 | To cover approx area: 1466mm (w) x 200mm (h) | DTM in 1no colour on to 3M matt self adhesive vinyl. Laser cut letter and apply on site to 1no painted MDF panel. |  |  |
| Section quote vinyl | GW.GCR.5.1.G1&2 | To cover approx area: 1466mm (w) x 200mm (h) | DTM in 1no colour on to 3M matt self adhesive vinyl. Laser cut letter and apply on site to 1no painted MDF panel. |  |  |
| **ELEVATION 3**  TRADE AND EMPIRE cont. |  |  |  |  |  |
| Section text panel top | GW.T&E.2.4.G1a | 494mm (w) x 1596mm (h) | DTM to 3M matt self adhesive vinyl. Apply to sanded, smoothed and sealed MDF panel. See 3D drawing for fixing details. |  | MDF supplied by main contractor |
| Section image panel | GW.T&E.2.4.G1b | 494mm (w) x 795mm (h) | DTM to 3M matt self adhesive vinyl. Apply to sanded, smoothed and sealed MDF panel. See 3D drawing for fixing details. |  | MDF supplied by main contractor |
| Section quote vinyl | GW.T&E.2.4.G2 | To cover approx area: 1466mm (w) x 200mm (h) | DTM in 1no colour on to 3M matt self adhesive vinyl. Laser cut letter and apply on site to 1no painted MDF panel. |  |  |
| Section text panel top | GW.T&E.2.5.G1a | 494mm (w) x 1596mm (h) | DTM to 3M matt self adhesive vinyl. Apply to sanded, smoothed and sealed MDF panel. See 3D drawing for fixing details. |  | MDF supplied by main contractor |
| Section image panel | GW.T&E.2.5.G1b | 494mm (w) x 795mm (h) | DTM to 3M matt self adhesive vinyl. Apply to sanded, smoothed and sealed MDF panel. See 3D drawing for fixing details. |  | MDF supplied by main contractor |
| Section quote vinyl | GW.T&E.2.5.G2 | To cover approx area: 1466mm (w) x 200mm (h) | DTM in 1no colour on to 3M matt self adhesive vinyl. Laser cut letter and apply on site to 1no painted MDF panel. |  |  |
| **CASE 4**  VINYL TEXT AND IMAGE | GW.T&E.2.6.G1 | 395mm (w) x 1630mm (h) (allow bleed of 20mm) | DTM to 3M matt self adhesive vinyl wrap to 5mm foamed panel. |  |  |
| **ELEVATION 4** |  |  |  |  |  |
| Section text panel top | GW.T&E.2.7.G1a | 494mm (w) x 1596mm (h) | DTM to 3M matt self adhesive vinyl. Apply to sanded, smoothed and sealed MDF panel. See 3D drawing for fixing details. |  | MDF supplied by main contractor |
| Section image panel | GW.T&E.2.5.G1b | 494mm (w) x 795mm (h) | DTM to 3M matt self adhesive vinyl. Apply to sanded, smoothed and sealed MDF panel. See 3D drawing for fixing details. |  | MDF supplied by main contractor |
| LIGHTBOX 1 | GW.T&E.2.8.G1 | 494mm (w) x 2394mm (h) | Supply 1no duratrans mount to rear face of 10mm clear acrylic. |  | See 3d drawing of Lightbox for fixing detail |
| LIGHTBOX 2 | GW.T&E.2.9.G1 | 494mm (w) x 2394mm (h) | Supply 1no duratrans mount to rear face of 10mm clear acrylic. |  | See 3d drawing of Lightbox for fixing detail |
| Section quote vinyl | GW.T&E.2.9.G2 | To cover approx area: 500mm (w) x 400mm (h) | DTM in 1no colour on to 3M matt self adhesive vinyl. Laser cut letter and apply on site to 1no painted MDF panel. |  |  |
| LIGHTBOX 3 | GW.T&E.2.11.G1 | 494mm (w) x 2394mm (h) | Supply 1no duratrans mount to rear face of 10mm clear acrylic. |  | See 3d drawing of Lightbox for fixing detail |
| Section quote vinyl | GW.T&E.2.11.G2 | To cover approx area: 1466mm (w) x 200mm (h) | DTM in 1no colour on to 3M matt self adhesive vinyl. Laser cut letter and apply on site to 1no painted MDF panel. |  |  |
| LIGHTBOX 4 | GW.T&E.2.12.G1 | 494mm (w) x 2394mm (h) | Supply 1no duratrans mount to rear face of 10mm clear acrylic. |  | See 3d drawing of Lightbox for fixing detail |
| **ELEVATION 5**  **OCEANIA** |  |  |  |  |  |
| Section text panel top | GW.T&E.2.10.G1a | 494mm (w) x 1596mm (h) | DTM to 3M matt self adhesive vinyl. Apply to sanded, smoothed and sealed MDF panel. See 3D drawing for fixing details. |  | MDF supplied by main contractor |
| Section image panel | GW.T&E.2.10.G1b | 494mm (w) x 795mm (h) | DTM to 3M matt self adhesive vinyl. Apply to sanded, smoothed and sealed MDF panel. See 3D drawing for fixing details. |  | MDF supplied by main contractor |
| Section quote vinyl | GW.T&E.2.10.G2 | To cover approx area: 1466mm (w) x 200mm (h) | DTM in 1no colour on to 3M matt self adhesive vinyl. Laser cut letter and apply on site to 1no painted MDF panel. |  |  |
| **ELEVATION 6**  **DEFENCE OF EMPIRE** |  |  |  |  |  |
| Column panel | GW.DOE.3.1.G1a&b | 542mm (w) x 2397mm (h) | DTM to 2no 3M matt self adhesive vinyl. Wrap to 2no sanded, smoothed and sealed 18mm MDF panel. See 3D drawing for fixing details. |  | Refer to 3D drawing package for fixing details |
| Section text panel top | GW.EA&ME.3.2.G1a | 494mm (w) x 1596mm (h) | DTM to 3M matt self adhesive vinyl. Apply to sanded, smoothed and sealed MDF panel. See 3D drawing for fixing details. |  | MDF supplied by main contractor |
| Section image panel | GW.EA&ME.3.2.G1b | 494mm (w) x 795mm (h) | DTM to 3M matt self adhesive vinyl. Apply to sanded, smoothed and sealed MDF panel. See 3D drawing for fixing details. |  | MDF supplied by main contractor |
| Section quote vinyl | GW.EA&ME.3.2.G2 | To cover approx area: 1300mm (w) x 200mm (h) | DTM in 1no colour on to 3M matt self adhesive vinyl. Laser cut letter and apply on site to 1no painted MDF panel. |  |  |
| Section text panel top | GW.EA&ME.3.3.G1a | 494mm (w) x 1596mm (h) | DTM to 3M matt self adhesive vinyl. Apply to sanded, smoothed and sealed MDF panel. See 3D drawing for fixing details. |  | MDF supplied by main contractor |
| Section image panel | GW.EA&ME.3.3.G1b | 494mm (w) x 795mm (h) | DTM to 3M matt self adhesive vinyl. Apply to sanded, smoothed and sealed MDF panel. See 3D drawing for fixing details. |  | MDF supplied by main contractor |
| Section quote vinyl | GW.EA&ME.3.3.G2 | To cover approx area: 1300mm (w) x 200mm (h) | DTM in 1no colour on to 3M matt self adhesive vinyl. Laser cut letter and apply on site to 1no painted MDF panel. |  |  |
| **ELEVATION 7**  **DEFENCE OF EMPIRE** |  |  |  |  |  |
| Section text panel top | GW.EA&ME.3.4.G1a | 393mm (w) x 1048mm (h) | DTM to 3M matt self adhesive vinyl. Apply to sanded, smoothed and sealed MDF panel. See 3D drawing for fixing details. |  | MDF supplied by main contractor |
| Section image panel | GW.EA&ME.3.4.G1b | 1143mm (w) x 640mm (h) | DTM to 3M matt self adhesive vinyl. Apply to sanded, smoothed and sealed MDF panel. See 3D drawing for fixing details. |  | MDF supplied by main contractor |
| Section quote vinyl | GW.EA&ME.3.4.G2 | To cover approx area: 1100mm (w) x 400mm (h) | DTM in 1no colour on to 3M matt self adhesive vinyl. Laser cut letter and apply on site to 1no painted MDF panel. |  |  |
| Section text panel top | GW.EA&ME.4.1.G1a | 494mm (w) x 1596mm (h) | DTM to 3M matt self adhesive vinyl. Apply to sanded, smoothed and sealed MDF panel. See 3D drawing for fixing details. |  | MDF supplied by main contractor |
| Section image panel | GW.WFE.4.1.G1b | 494mm (w) x 795mm (h) | DTM to 3M matt self adhesive vinyl. Apply to sanded, smoothed and sealed MDF panel. See 3D drawing for fixing details. |  | MDF supplied by main contractor |
| **ELEVATION 8**  **WITHDRAWAL FROM EMPIRE** |  |  |  |  |  |
| Section quote vinyl | GW.WFE.4.1.G2+3 | To cover approx area: 1466mm (w) x 400mm (h) | DTM in 1no colour on to 3M matt self adhesive vinyl. Laser cut letter and apply on site to 1no painted MDF panel. |  |  |
| Section text panel top | GW.GCR.5.1.G1a | 494mm (w) x 1596mm (h) | DTM to 3M matt self adhesive vinyl. Apply to sanded, smoothed and sealed MDF panel. See 3D drawing for fixing details. |  | MDF supplied by main contractor |
| Section image panel | GW.GCR.5.1.G1b | 494mm (w) x 795mm (h) | DTM to 3M matt self adhesive vinyl. Apply to sanded, smoothed and sealed MDF panel. See 3D drawing for fixing details. |  | MDF supplied by main contractor |
| Section quote vinyl | GW.GCR.5.1.G2+3 | To cover approx area: 1466mm (w) x 400mm (h) | DTM in 1no colour on to 3M matt self adhesive vinyl. Laser cut letter and apply on site to 1no painted MDF panel. |  |  |
| **CASE ASSET PRINTS** |  |  |  |  |  |
| Case 1 photographic print | GW.CSP1.G1 | 169mm (w) x 119mm (h) | Supply no full colour image print onto photographic matt paper. Mount to 2mm black core foamex. |  | 1969.07-17-01 |
| Case 6 photographic print | GW.CSP6.G1-3 | 2no: 169mm (w) x 119mm (h)  1no: 340mm (w) x 305mm (h) | Supply 3no full colour image print onto photographic matt paper. Mount to 2mm black core foamex. |  | Newly-arrived Indian troops with the Malta garrison, Florian Parade, June 1878  NAM. 1957-04-30-77 Neg. 110083  Soldiers from 123rd Outram’s Rifles on board the Royal Indian Marine steamer ‘Hardinge’ bound for Jask, 1910  NAM. 2014-08-7-71 Neg. 1154390 (crop out border) |
| Case 7 photographic print | GW.CSP7.G1-2 | 139mm (w) x 104mm (h)  412mm (w) x 253mm (h) | Supply 2no full colour image print onto photographic matt paper. Mount to 2mm black core foamex. |  | **British South Africa Company**’**s Police, Pioneer Column, Mashonaland, 1890**  NAM. 1982-06-103-2 Neg.125261 |
| Case 10 photographic print | GW.CSP10.G1-2 | 139mm (w) x 173mm (h)  139mm (w) x 104mm (h) | Supply 2no full colour image print onto photographic matt paper. Mount to 2mm black core foamex. |  | Waziri and Mahsud warriors, *c*1919  NAM. 1989-03-28-2 Neg. 119465  NAM. 1965-10-220-25 Neg. 98812 |
| Case 11 photographic print | GW.CSP11.G1-3 | 189mm (w) x 188mm (h)  269mm (w) x 183mm (h)  678mm (w) x 479mm (h) | Supply 3no full colour image print onto photographic matt paper. Mount to 2mm black core foamex. |  | Photographs of a field telegrapher and a six-inch naval gun mounted on a railway truck at Modder River, 1899  NAM. 1998-01-135-51 Neg. 92783  NAM. 1986-08-49-140 Neg. 84854  NAM. 1971-04-41  (Neg to be supplied by NAM) |
| Case 12 photographic print | GW.CSP12.G1-5 | 80mm (w) x 66mm (h)  80mm (w) x 50mm (h) 94mm (w) x 97mm (h) 290mm (w) x 165mm (h)  400mm (w) x 306mm (h) | Supply 4no full colour image print onto photographic matt paper. Mount to 2mm black core foamex. |  | **German colonial soldiers and the Nigeria Regiment Artillery, West Africa Frontier Force, 1914**  NAM. 1987-05-8-3 Neg.111806  NAM. 1987-05-8-1 Neg. 111804  South Africans outside a desert blockhouse, 1915  NAM. 1972-08-67-2-130 Neg. 110733  Indian Army troops marching into Baghdad, 11 March 1917  NAM. 1965-10-221-85 Neg. 1017230  Postcard lithograph  NAM. 1960.09.35.2 |
| Case 13 photographic print | GW.CSP13.G1-2 | 250mm (w) x 170mm (h)  311mm (w) x 225mm (h) | Supply 2no full colour image print onto photographic matt paper. Mount to 2mm black core foamex. |  | 1999.04.29  2003.04.235 |
| Case 15 photographic print | GW.CSP15.G1-4 | 196mm (w) x 230mm (h)  145mm (w) x 212mm (h)  227mm (w) x 214mm (h) 175mm (w) x 213mm (h) | Supply 4no full colour image print onto photographic matt paper. Mount to 2mm black core foamex. |  | 1994-02.28  1955.05.871  2009.01.29  2016.10.23 |
| Case 16 photographic print | GW.CSP16.G1-3 | 252mm (w) x 173mm (h)  140mm (w) x 210mm (h)  375mm (w) x 176mm (h) | Supply 3no full colour image print onto photographic matt paper. Mount to 2mm black core foamex. |  | Rebels captured by the Queen's Own Highlanders at the Brunei oil town of Seria, 1962  NAM. 2004-12-33-3 Neg. 1009011  2003.11.15.4  1988.12.41.9 |
| Case 19 photographic print | GW.CSP19.G1-3 | 254mm (w) x 203mm (h)  254mm (w) x 203mm (h)  254mm (w) x 203mm (h) | Supply 3no full colour image print onto photographic matt paper. Mount to 2mm black core foamex. |  | A soldier of The Rifles checks motorists’ temperatures at a checkpoint in Freetown, Sierra Leone, 2015  NAM. 2017-07-5-226 Neg. 228530  Royal Engineers clearing hurricane debris on Grand Turk Island, 2017  NAM. 2017-10-33-43 Neg. 236674    British Army medics work with their Kenyan counterparts to assist villagers during Exercise Askari Storm, 2016  NAM. 2017-08-6-32 Neg. 229378 |
| WALL REPROGRAPHICS | GW.3 / ELEVATION  GW. 6 / ELEVATION  GW.7 / ELEVATION  GW.7 / ELEVATION  GW.8 / ELEVATION | 263mm (w) x 173mm (h)  355mm (w) x 254mm (h)  258mm (w) x 351mm (h)  255mm (w) x 354mm (h)  358mm (w) x 260mm (h)  358mm (w) x 260mm (h)  224mm (w) x 224mm (h)  224mm (w) x 224mm (h)  358mm (w) x 259mm (h)  358mm (w) x 259mm (h)  252mm (w) x 167mm (h) | Supply 11no full colour image print onto photographic matt paper. DO NOT TRIM. |  | 1971.02.-33.515.7  1985.11.36.25  2005.09.60.15  2005.08.63  2007.04.43-4  2007-12-6-110  1992-11-145-22  1992.08-65-86  1996.06.157  1999.11.8.75  2003-03-597-1 |
| **CASE 1-19 TITLES** |  |  |  |  |  |
| CASE VINYL TITLES | GW.CST.G1-24 | To cover approx area:  14no 500mm x 155mm  10no 400mm x 100mm | Output total number 24no dusted crystal laser cut vinyl. Apply on site to interior of showcase glass. |  | SAMPLE TO BE SUPPLIED AND TESTED ON SITE FOR LEGIBILITY |
| **OBJECT LABELS** |  |  |  |  |  |
| Wall mounted object labels | GW.WL.G1-53 | 150mm (w) x 210mm (h) | DTM to GF Smith Colour plan (uncoated) Vellum White 540gsm card. Mount to supplied angled label holder |  | Label holders supplied by NAM. |
| Plinth labels | GW.PL.G1-44 | **Case 1**  870mm (w) x 233mm (h)  **Case 2**  196mm (w) x 1500mm (h)  **Case 3**  640mm (w) x 233mm (h)  **Case 5**  1400mm (w) x 233mm (h)  **Case 6**  1400mm (w) x 233mm (h)  **Case 7**  1400mm (w) x 233mm (h)  **Case 8**  250mm (w) x 500mm (h)  **Case 9**  740mm (w) x 233mm (h)  160mm (w) x 450mm (h)  **Case 10**  Front plinth A  550mm (w) x 233mm (h)  End plinth A  180mm (w) x 233mm (h)  Front plinth B  630mm (w) x 233mm (h)  Front plinth C  932mm (w) x 233mm (h)  Front plinth D  538mm (w) x 233mm (h)  Front plinth E  580mm (w) x 233mm (h)  End plinth E  137mm (w) x 233mm (h)  Front plinth F  962mm (w) x 233mm (h)  Front plinth G  560mm (w) x 233mm (h)  Front plinth H  679mm (w) x 233mm (h)  Rod support  200mm (w) x 160mm (h)  End of plinth A elevation 1  180mm (w) x 233mm (h) | DTM to GF Smith Colour plan (uncoated) Vellum White 540gsm card. Mount to angled table holder  **Case 2 & 8**  DTM to clear vinyl. Backed up with solid colour or dusted crystal  For Rod fixing double mount card  **Case 9**  Rod fixing on smaller label |  | Refer to 3D drawing package for plinth sizes and label fixing details  Refer to 3d drawing package for the **rod type** label fixing details |
|  |  | **Case 11**  Front plinth A  482mm (w) x 233mm (h)  End plinth A  180mm (w) x 233mm (h)  Front plinth B  950mm (w) x 233mm (h)  Front plinth C  580mm (w) x 233mm (h)  Front plinth D  580mm (w) x 233mm (h)  End plinth E  261mm (w) x 233mm (h)  Front plinth F  580mm (w) x 233mm (h)  Fixed to support rods for object 1999-10-33-1  160mm (w) x 160mm (h)  Fixed to support rods for object 1964-12-39-1  160mm (w) x 160mm (h)  **Case 12**  Rod support  563mm (w) x 233mm (h)  Front plinth A  315mm (w) x 160mm (h)  Front plinth B  628mm (w) x 233mm (h)  Rod support  160mm (w) x 233mm (h)  Front plinth C  587mm (w) x 233mm (h)  Rod support  562mm (w) x 233mm (h)  End Rod support  300mm (w) x 160mm (h)  Front plinth D  1100mm (w) x 233mm (h)  Rod support  180mm (w) x 430mm (h)  **Case 13**  Front plinth  1900mm (w) x 233mm (h) | DTM to GF Smith Colour plan (uncoated) Vellum White 540gsm card. Mount to angled table holder  For Rod fixing double mount card |  |  |
|  |  | Rod 160mm (w) x 450mm (h)  Rod 160mm (w) x 450mm (h)  **Case 14**  Front plinth  973mm (w) x 233mm (h)  **Case 15**  Front plinth  1900mm (w)x 233mm (h)  **Case 16**  150 (w) x 282 (h) mounted on case base  500 x 50 wall mounted  500 x 230 mounted on case base  150 x 640 wall mounted  **Case 17**  Front plinth  920mm (w)x 233mm (h)  **Case 18A**  Front plinth  935mm (w)x 233mm (h)  **Case 18B**  Front plinth  982mm (w)x 233mm (h)  **Case 18C**  Front plinth  935mm (w)x 233mm (h)  **Case 19**  Front plinth  920mm (w)x 233mm (h) | DTM to GF Smith Colour plan (uncoated) Vellum White 540gsm card. Mount to angled table holder  For Rod fixing double mount card |  |  |
| FLOOR GRAPHIC | GW.F.G1 | 2000mm (w)x2000mm (h) | Supply 1no DTM full colour to adhesive floor vinyl |  | Existing floor finish is concrete. Adhesive to be approved by client |
| **SAMPLES** |  |  |  |  |  |
| COLOR SAMPLES FOR PAINT MATCHING |  |  | DTM on to 3M matt self adhesive vinyl. |  |  |
| FABRIC PANEL FOR ENTRANCE AREA |  | 1000mm (w) x 1000mm (h) | DTM to graphic wallpaper stretched fabric. Allow for applied elements such as fire safety sign and sponsorship panel |  |  |
| LIGHTBOX DURATRANS |  | 1000mm (w) x 1000mm (h) | Full colour durations showing all 4no area colours to test colour match and legibility of type |  |  |
| VINYL FOR MOUNTED TO MDF PANEL |  | 1000mm (w) x 1000mm (h) | DTM in 1no colour on to 3M matt self adhesive vinyl. |  | TO INCLUDE PART OF IMAGE FOR COLOUR MATCHING |
| VINYL FOR quotes |  | 500mm (w) x 200mm (h) | DTM in 1no colour on to 3M matt self adhesive vinyl. Laser cut letter and apply on site to 1no painted MDF panel. |  |  |
| DUSTED CRYSTAL TITLE CASE TITLES |  | 500mm (w) x 200mm (h) | Laser cut dusted crystal laser cut vinyl. Apply on site to interior of showcase glass. |  | SAMPLE TO BE TESTED ON SITE WITH LIGHTING |
| LABEL SAMPLES AT 1.1 TO INCLUDE ALL COLOURS |  | 8no 150mm (w) x 210mm (h)  8no 973mm (w) x 233mm (h) | DTM to GF Smith Colour plan (uncoated) Vellum White 540gsm card. Mount to angled table holder |  |  |
| FLOOR GRAPHIC |  | 500mm (w) x 200mm (h) | Supply 1no DTM full colour to adhesive floor vinyl |  | ADHESIVE TO TO  APPROVED BY CLIENT |
|  |  |  |  |  |  |