**Appendix 3**

**Wet pour Specification for Tender**

Specification Generally a thickness of 15mm and above to be installed on to a sound bitumen or concrete area whereas a minimum of 40mm should be installed onto a subbase type material.