BRIEF TECHNICAL DESCRIPTIONS – TOYOTA LAND CRUISERS:-

|  |
| --- |
| **44 x TOYOTA LAND CRUISER 78 SERIES - HZJ78L-RJMRS** |
| All 44 vehicles should be plain white (external colour);Left hand drive, 4x4;Seats: 13 Seater. No. of doors: 3 (with central locking); Diesel engine, (Petrol V8 model not permitted);Transmission 5 speed, Manual;Engine: Model 1HZ - 4164cc, Diesel (Fuel tank capacity litres – 90L + 90L), 6 cylinders, BHP: 129, KW: 96, Cooling (Water), electrics 12 Volts with air conditioning included;Brakes: Front: Disc, Rear: Drum;All wheel rims are steel, inclusive of two spare wheels - Mud tyres (NO ALLOYS);Vehicles to be fitted with bullbars, winches, long jacks and roof rack with four jerry can holders;Warranty must be provided on the vehicles;Vehicles must be compliant with road regulations in South Sudan, suitable for the local terrain/environment, climate and the engine must be capable of operating with the quality of diesel fuel available within this country.  |