**TENDER SUMMARY SHEET**

|  |  |  |
| --- | --- | --- |
|  | **Specification** | **Price** |
| **1.** | **Required** |  |
| 1.1 | For Roof A & Roof B required work is clean and remove all debris of the gutters before the roof takes place. | £.0.00 |
| 1.2 | Roof A – Fully remove and re-line gutters with a rolled-on membrane which is then fixed to the abutment under the flashing. This is done with combination of mechanical fixings and hot air welds. The system would include the insertion of liners into the rainwater outlets are heat welded into place. (400m Indicative Measurements) | £.0.00 |
|  | Roof B – Fully remove and re-line gutters with a rolled-on membrane which is then fixed to the abutment under the flashing. This is done with combination of mechanical fixings and hot air welds. The system would include the insertion of liners into the rainwater outlets are heat welded into place.  As part of this work to Roof B application of the membrane you will be required to lift the coping stones in order to allow the new gutter lining. (200m Indicative Measurements) |  |
| 1.3 | For Roof B a steel flashing should be used to cover the edges of the new gutter lining. | £.0.00 |
| 1.4 | Replace all the spouts on Roof A & B. | £.0.00 |
| 1.5 | There is parapet between two sections of the single storey roof. This serves no practical purpose and is contributing to water ingress. It is proposed this should be reduced. | £.0.00 |
| 1..6 | The current Safe Access system is inappropriate for the single storey building on JS B1 therefore the contractor will be appointed to complete design and install for a compliant safe access system. | £.0.00 |
| **2** | **Desired** |  |
| 2.1 | On Roof A the hip ridges, water seeps through due to the insulation being decayed or lost in some areas. The flashings need to be lifted and the fillers need to be replaced and the flashings re-instated. | £.0.00 |
| 2.1 | Cut edge corrosion repair undertaken | £.0.00 |
| **3.** | **Access** |  |
| 3.1 | Access to undertaken the works for Two Storey Building | £.0.00 |
| 3.2 | Access to undertaken the works for Single Storey Building | £.0.00 |
| 4. | Site Compound |  |
| 4.1 | Site Compound incl. cabin, any require herras fencing etc | £.0.00 |