Saxmundham Town Council – Memorial field Project

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Item | Description | Quantity | Cost |  |
| 1 | Set up site | Item |  |  |
| 1a | Spray off future planted area | 270m2 |  |  |
| 1b |  |  |  |  |
| 2 | Rotivate soil depth 150-300mm | 270m2 |  |  |
| 3 | Excavate pathway and circle; approx depth 150-300mm | 107m2 |  | 40m3 |
| 3a | Provide and lay Terram T1000 geo-textile to pathways | 107m2 |  |  |
| 4 | Import type 1 fill to centre circle; approx depth 200mm | 45m2 |  |  |
| 5 | Import type 1 Fill to paths; approx depth 200mm | 62m2 |  |  |
| 5a | Spread / compact type 1 | 107m2 |  |  |
| 6 | Lay 2x 100mm duct to centre circle | 13m |  |  |
| 7 | Lay corten steel path edgings; 3mm thk x 150mm | 135.5m |  |  |
| 8 | Lay circular corten steel path edging ; 1.0m dia | 1no |  |  |
| 9 | Lay bound gravel to pathways; 100mm depth | 59.5m2 |  | Allow e/o for resin bound gravel as option |
| 10 | Lay bound gravel to centre circle; 100mm depth | 45m2 |  |  |
| 11 | Form bund using arising from paths | 40m3 |  |  |
| 12 |  planting; as per landscape planting schedule | item |  |  |
| 13 | Excavate foundation for circular bench x2 | 1.5m3 |  |  |
| 14 | Place concrete for foundation for circular benches | 1.5m3 |  |  |
| 15 | Build circular benches ; see detail drg | Item |  | Design / appearance to be finalised |
| 16 | Excavate foundation for memorial plinth | 0.5m3 |  |  |
| 17 | Build memorial ; see detail drg | Item  |  |  |
| 18 | Resite and lay original memorial stone | item |  |  |
| 19 | Erect Notice /Information boards  | 2no |  | Free issue |
| 20 | Erect new field and pedestrian gates. Design by others | Item |  |  |
| 21 | Erect Burleigh estate steel fencing to entrance area | 16m |  |  |
| 22 | Erect Burleigh estate steel fencing to roadway  | 34m |  |  |
| 23 | Lay corten path edging to 50% of circle dia. 7.5m rad. | Item |  |  |
| 24 | Excavate area adjacwent existing gate/drive; 150-300mm depth | 30m2 |  |  |
| 25 | Fill area with type 1; approx. 200mm depth | 30m2 |  |  |
| 26 | Fill area with bound gravel, 100mm depth | 30m2 |  |  |
|  |  |  |  |  |
|  | TOTAL |  | £ |  |
|  |  |  |  |  |
|  |  |  |  |  |