**All weather path for Bull Meadow**

To install 1000 linear metres of 1200mm wide all weather path with tanalised timber edging using 22mm thick boards, excavated to a depth of 120mm, lined with Terram  T1000 geotextile membrane with 100mm of compacted type one stone with a 50mm capping layer of self-binding gravel.

Any spoil created should be added to the bunds in Bull Meadow.

This price should include any grading works that are required to ensure that the gradient of the path does not exceed 1:12 for wheelchair use.

The path is to go within the perimeter of Bull Meadow in Fernhill Heath and will be circular so that users can enter via the pedestrian entrance and walk around the meadow and leave at the entry point. Exact location is not fixed but please see attached map for approximate pathway location. Pathway is noted as all-weather pathway on the map.

Works are to be completed by the end of Spring 2023.

Any questions please contact

Clare Shinner

clerk@northclainesparishcouncil.gov.uk