**QUOTATION AND SPECIFICATION**

**General**

All works from formation to finished surface will be carried out by our Lasertru Levelling System for guaranteed accuracy throughout the construction.

**Access**

It is assumed that full access for plant and material deliveries will be available up to the site of the working area.

**Preparation**

The existing surface will be cleaned, holes will be drilled at 450mm centres and filled with clean shingle. The edge will be cut back (where required) to allow the new surface to finish flush with the existing edgings. The whole area will then be sprayed with bitumen emulsion to bind the new surface to the old.

**Weed Treatment**

 An appropriate herbicide will be applied at rates recommended by the manufacturer to destroy as far as possible any remaining weed roots or seedlings.

**Nets Posts & Fittings**

One pair of our super match quality 75mm square tennis posts will be provided with heavy duty ground sockets securely set in concrete with a centre band ground anchor also set in concrete. A tournament quality net will be supplied complete with a centre band adjuster

**Clarify 1 or 2 sets of posts and netts ?**

 **Surfacing**

 Surfacing comprises of a layer of specially formulated porous bitumen macadam screeded to accurate levels, rolled and cross rolled to give a smooth playing surface. The total depth of Macadam will be 35mm consolidated. The surface will be laid to accurate levels by our special Laser true screeding process.

**Painting**

After an appropriate interval, (4/6 weeks) the surface will be coloured with two coats of acrylic paint by our special high-pressure spraying process. Non slip White lines for Tennis x2 will be painted on. Paint is available in a range of colours including standard red and standard green, 2 tone green or a combination to meet your requirements.

 **Site clearance/Reinstatement**

 Upon completion the site will be cleared of all surplus materials, tools, and rubbish and left tidy. Whilst care will be taken to minimise disruption and disturbance no further allowance has been made for landscaping and or reinstatement of the working area or access way.

**All for the sum of £32,560.00 plus VAT**

**Option ‘A’**

**Fence**

Take down the existing chain-link fence and the existing timber boards. The existing posts will be cleaned, then painted with red oxide primmer followed green topcoat paint. Supply and install new chain -link fencing fixed to the existing posts. 3 Mesh Panels will be installed with new posts behind both basketball/ football goals.

**All for the sum of £11,520.00 plus VAT**

**Clarify cost if boarding and chain link fence were removed by ourselves**

 **Option ‘B’**

Take down the existing chain-link fence, timber boards and all of the existing posts. Supply and install new 3m high green mesh panel fencing system, with 1x 1.2m wide gate.

**All for the sum of £24,320.00 plus VAT**

**Clarify cost if boarding, chain link fence and posts were removed by ourselves**

**Extra’s**

Socketed basketball goals

 All for the sum of £1,250.00 plus VAT Per end

**Only one basket ball goal will be required at this present time ?**

Free standing Football Goals £650 plus VAT (pair)

**Ive looked around and these seem a fair price, but are free standing a good idea ? (kids will move them about (what other options are there) ?**

Socketed Netball posts £480 plus VAT (pair)

**Do we need a pair at this moment in time? Can another be added at a later date?**

Extra lines Netball £360 plus VAT per set

**I assume this price of £360 is for if we had 2 netball hoops and would be half the cost if only 1 netball hoop was installed ?**

Football lines £360 plus VAT per set

**I don’t see any problems with this**

Basketball lines with keys £520 plus VAT per set

**I assume this price of £520 is if we had 2 basketball hoops installed and would it be half the cost if only 1 basketball hoop was installed**