{"text_format":"1","workbook":"xlsx","n_sheets":6,"sheets":["COVER","CY1100","CY11O1","CY1140","CY1142","CY2623"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":2,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"COVER","index":0,"n_rows":13,"n_cols":7,"rows_kept":13,"cut":false,"hidden":false,"merged":[[9,3,9,9]]}
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,"BFCCB/1372 DEFFORM 47 ANNEX C"]
[]
[]
[null,null,null,null,null,null,"TECHNICAL EVALUATION MATRIX"]

{"sheet":"CY1100","index":1,"n_rows":71,"n_cols":5,"rows_kept":71,"cut":false,"hidden":false,"merged":[[6,0,6,4]]}
["BFC WHITE FLEET VEHICLE TECHNICAL ASSESSMENT DATA - CY1100 - TRUCK UTILITY CREW CAB 4X4"]
[]
["Supplier:"]
["Vehicle Tendered:"]
["Date:"]
[]
["Tenderers to provide proof that they can meet the requirement by providing copies of the vehicle specification, brochure, warranty details and any other supporting evidence. "]
[]
["General Conditions","Pass","Fail","Parameter ","Response & Comments"]
["Vehicle meets all applicable EU Community specifications and type approvals",null,null,"none"]
["Vehicle has a minimum 4* Euro NCAP rating",null,null,"state rating"]
["Vehicle Certificate of Conformity available",null,null,"none"]
["Vehicle meets all applicable Republic of Cyprus Transport Regulations",null,null,"none"]
["Vehicle can operate in all Republic of Cyprus environmental conditions",null,null,"none"]
["Minimum 3 year, 100, 000km full parts and labour warranty",null,null,"provide full warranty details as per specification"]
["Vehicle Configuration","Pass","Fail","Parameter ","Response & Comments"]
["4-door crew cab with 4x4 drive",null,null,"Vehicle Certificate"]
["Seats for 4 passengers plus driver",null,null,"Vehicle Certificate"]
["All doors lockable with central locking",null,null,"Vehicle Certificate"]
["Fitted with a laminated windscreen",null,null,"Vehicle Certificate"]
["Separate cargo compartment",null,null,"Vehicle Certificate"]
["Cargo compartment plastic liner fitted",null,null,"include details"]
["Cargo compartment internal length minimum 1400mm",null,null,"state length"]
["Cargo compartment internal height minimum 400mm",null,null,"state height"]
["Cargo compartment internal width minimum 1500mm",null,null,"state width"]
["Cargo compartment tailgate bottom hinged folding flat to floor",null,null,"none"]
["Towing hitch with combined 50mm ball and pintle fitted",null,null,"none"]
["Trailer electrical socket and associated wiring fitted (to EU Standard 12N)",null,null,"none"]
["Costs included for specific paint finishes",null,null,"include costs in tender "]
["Vehicle Weights","Pass","Fail","Parameter ","Response & Comments"]
["Payload minimum of 1000 kg",null,null,"state load"]
["Capable of towing 2000kg braked trailer",null,null,"state tow wt"]
["Vehicle Power Train","Pass","Fail","Parameter ","Response & Comments"]
["Diesel engine drive with minimum power of 105 kW",null,null,"state max kW"]
["Minimum 5-speed manual gearbox",null,null,"state number"]
["Engine filled with anti-freeze suitable for Cyprus conditions",null,null,"none"]
["Fitted with steel wheels",null,null,"none"]
["Fitted with steel braced radial tyres",null,null,"none"]
["Performance","Pass","Fail","Parameter ","Response & Comments"]
["Acceleration from zero to 100 kph in 15.0 seconds or less",null,null,"state time"]
["Emission standards conform to EURO 6 requirements",null,null,"none"]
["CO² emissions (combined figure) as low as possible below 190 gm/km",null,null,"state gm/km"]
["Diesel fuel tank capacity minimum 60 ltr",null,null,"state ltr"]
["Systems","Pass","Fail","Parameter ","Response & Comments"]
["Fitted with power assisted steering",null,null,"none"]
["Fitted with heavy duty sealed for life battery",null,null,"none"]
["Fitted with high level rear brake lights",null,null,"none"]
["Fitted with a minimum of one rear high intensity fog light.",null,null,"none"]
["Fitted with nearside, offside and interior rear view mirrors",null,null,"none"]
["Brake system with ABS",null,null,"none"]
["Interior Safety","Pass","Fail","Parameter ","Response & Comments"]
["Fitted with driver and front passenger airbags",null,null,"none"]
["Fitted with front and rear seat head rests (rear centre not essential)",null,null,"none"]
["Fitted with lap & diagonal inertia reel seat belts (rear centre static lap OK)",null,null,"none"]
["Interior Systems","Pass","Fail","Parameter ","Response & Comments"]
["Drivers seat adjustable for height, rake & reach",null,null,"none"]
["Fitted with steering wheel column position adjustment ",null,null,"none"]
["Fitted with a heater/demister system capable of  providing 25°C interior",null,null,"none"]
["Fitted with an air-conditioning system capable of providing 25°C interior",null,null,"none"]
["Fitted with radio / CD player with minimum VHF(FM) & MW(AM) reception",null,null,"none"]
["Breakdown Equipment","Pass","Fail","Parameter ","Response & Comments"]
["Fitted with a full size spare wheel and tyre",null,null,"none"]
["Provided with a jack and jack handle capable of lifting fully loaded vehicle",null,null,"none"]
["Provided with a wheel brace capable of unscrewing wheel nuts",null,null,"none"]
["Provided with two warning triangles",null,null,"none"]
["Registration & Delivery","Pass","Fail","Parameter ","Response & Comments"]
["Vehicle to be registered by supplier in Republic of Cyprus",null,null,"none"]
["Vehicle to be fitted with Republic of Cyprus number plates",null,null,"none"]
["Vehicle to be delivered into BFC Vehicle Depot at RAF Akrotiri",null,null,"none"]
["Vehicle to be delivered in ready to use condition",null,null,"none"]
["Please provide a delivery timescale from start of contract.",null,null,"state timescale for delivery"]

{"sheet":"CY11O1","index":2,"n_rows":74,"n_cols":5,"rows_kept":74,"cut":false,"hidden":false,"merged":[[7,0,7,4]]}
["BFC WHITE FLEET VEHICLE TECHNICAL ASSESSMENT DATA - CY1101 - TRUCK UTILITY CREW CAB 4X4 "]
[null,"WITH CARGO BODY HARD TOP"]
[]
["Supplier:"]
["Vehicle Tendered:"]
["Date:"]
[]
["Tenderers to provide proof that they can meet the requirement by providing copies of the vehicle specification, brochure, warranty details and any other supporting evidence. "]
[]
["General Conditions","Pass","Fail","Parameter ","Response & Comments"]
["Vehicle meets all applicable EU Community specifications and type approvals",null,null,"none"]
["Vehicle has a minimum 4* Euro NCAP rating",null,null,"state rating"]
["Vehicle Certificate of Conformity available",null,null,"none"]
["Vehicle meets all applicable Republic of Cyprus Transport Regulations",null,null,"none"]
["Vehicle can operate in all Republic of Cyprus environmental conditions",null,null,"none"]
["Minimum 3 year, 100, 000km full parts and labour warranty",null,null,"provide full warranty details as per specification"]
["Vehicle Configuration","Pass","Fail","Parameter ","Response & Comments"]
["4-door crew cab with 4x4 drive",null,null,"none"]
["Seats for 4 passengers plus driver",null,null,"none"]
["All doors lockable with central locking",null,null,"none"]
["Fitted with a laminated windscreen",null,null,"none"]
["Separate cargo compartment",null,null,"none"]
["Cargo compartment plastic liner fitted",null,null,"include details"]
["Cargo compartment internal length minimum 1400mm",null,null,"state width"]
["Cargo compartment internal height minimum 400mm",null,null,"state length"]
["Cargo compartment internal width minimum 1500mm",null,null,"state height"]
["Cargo compartment tailgate bottom hinged folding flat to floor",null,null,"none"]
["Cargo compartment hard top fitted securely to vehicle body",null,null,"include details"]
["Cargo compartment hard top with lockable top-hinged lift-back rear door",null,null,"include details"]
["Towing hitch with combined 50mm ball and pintle fitted",null,null,"none"]
["Trailer electrical socket and associated wiring fitted (to EU Standard 12N)",null,null,"none"]
["Costs included for specific paint finishes",null,null,"include costs in tender "]
["Vehicle Weights","Pass","Fail","Parameter ","Response & Comments"]
["Payload minimum of 1000 kg",null,null,"state load"]
["Capable of towing 2000kg braked trailer",null,null,"state tow wt"]
["Vehicle Power Train","Pass","Fail","Parameter ","Response & Comments"]
["Diesel engine drive with minimum power of 105 kW",null,null,"state max kW"]
["Minimum 5-speed manual gearbox",null,null,"state number"]
["Engine filled with anti-freeze suitable for Cyprus conditions",null,null,"none"]
["Fitted with steel wheels",null,null,"none"]
["Fitted with steel braced radial tyres",null,null,"none"]
["Performance","Pass","Fail","Parameter ","Response & Comments"]
["Acceleration of zero to 100 kph by 15.0 seconds or less",null,null,"state time"]
["Emission standards conform to EURO 6 requirements",null,null,"none"]
["CO² emissions (combined figure) as low as possible below 190 gm/km",null,null,"state gm/km"]
["Diesel fuel tank capacity minimum 60 ltr",null,null,"state ltr"]
["Systems","Pass","Fail","Parameter ","Response & Comments"]
["Fitted with power assisted steering",null,null,"none"]
["Fitted with heavy duty sealed for life battery",null,null,"none"]
["Fitted with high level rear brake lights",null,null,"none"]
["Fitted with a minimum of one rear high intensity fog light.",null,null,"none"]
["Fitted with nearside, offside and interior rear view mirrors",null,null,"none"]
["Brake system with ABS",null,null,"none"]
["Interior Safety","Pass","Fail","Parameter ","Response & Comments"]
["Fitted with driver and front passenger airbags",null,null,"none"]
["Fitted with front and rear seat head rests (rear centre not essential)",null,null,"none"]
["Fitted with lap & diagonal inertia reel seat belts (rear centre static lap OK)",null,null,"none"]
["Interior Systems","Pass","Fail","Parameter ","Response & Comments"]
["Drivers seat adjustable for height, rake & reach",null,null,"none"]
["Fitted with steering wheel column position adjustment ",null,null,"none"]
["Fitted with a heater/demister system capable of  providing 25°C interior",null,null,"none"]
["Fitted with an air-conditioning system capable of providing 25°C interior",null,null,"none"]
["Fitted with radio / CD player with minimum VHF(FM) & MW(AM) reception",null,null,"none"]
["Breakdown Equipment","Pass","Fail","Parameter ","Response & Comments"]
["Fitted with a full size spare wheel and tyre",null,null,"none"]
["Provided with a jack and jack handle capable of lifting fully loaded vehicle",null,null,"none"]
["Provided with a wheel brace capable of unscrewing wheel nuts",null,null,"none"]
["Provided with two warning triangles",null,null,"none"]
["Registration & Delivery","Pass","Fail","Parameter ","Response & Comments"]
["Vehicle to be registered by supplier in Republic of Cyprus",null,null,"none"]
["Vehicle to be fitted with Republic of Cyprus number plates",null,null,"none"]
["Vehicle to be delivered into BFC Vehicle Depot at RAF Akrotiri",null,null,"none"]
["Vehicle to be delivered in ready to use condition",null,null,"none"]
["Please provide a delivery timescale from start of contract.",null,null,"state timescale for delivery"]

{"sheet":"CY1140","index":3,"n_rows":67,"n_cols":5,"rows_kept":67,"cut":false,"hidden":false,"merged":[[6,0,6,4]]}
["BFC WHITE FLEET VEHICLE TECHNICAL ASSESSMENT DATA - CY1140 - CAR UTILITY HATCHBACK 4X2"]
[]
["Supplier:"]
["Vehicle Tendered:"]
["Date:"]
[]
["Tenderers to provide proof that they can meet the requirement by providing copies of the vehicle specification, brochure, warranty details and any other supporting evidence. "]
[]
["General Conditions","Pass","Fail","Parameter ","Response & Comments"]
["Vehicle meets all applicable EU Community specifications and type approvals",null,null,"none"]
["Vehicle has a minimum 5* Euro NCAP rating",null,null,"state rating"]
["Vehicle Certificate of Conformity available",null,null,"none"]
["Vehicle meets all applicable Republic of Cyprus Transport Regulations",null,null,"none"]
["Vehicle can operate in all Republic of Cyprus environmental conditions",null,null,"none"]
["Minimum 3 year, 100, 000km full parts and labour warranty",null,null,"provide full warranty details as per specification"]
["Vehicle Configuration","Pass","Fail ","Parameter ","Response & Comments"]
["Medium sized 5-door hatchback with top hinged rear door",null,null,"none"]
["Seats for 4 passengers plus driver",null,null,"none"]
["All doors lockable with central locking",null,null,"none"]
["Fitted with a laminated windscreen",null,null,"none"]
["Rear seat able to fold in separate sections flat with rear load floor",null,null,"none"]
["Rear load area volume minimum 0.35m³ with rear seats in place",null,null,"state volume"]
["Rear load area volume minimum 1.20m³ with rear seat fully folded",null,null,"state volume"]
["Rear door sill height minimal above cargo floor level",null,null,"state height"]
["Costs included for specific paint finishes",null,null,"include costs in tender "]
["Vehicle Weights","Pass","Fail ","Parameter ","Response & Comments"]
["Payload minimum of 450 kg",null,null,"state load"]
["Vehicle Power Train","Pass","Fail ","Parameter ","Response & Comments"]
["Diesel engine drive with minimum power of 65kW",null,null,"state max kW"]
["Minimum 5 forward speed manual gearbox",null,null,"state number"]
["Engine filled with anti-freeze suitable for Cyprus conditions",null,null,"none"]
["Fitted with steel wheels",null,null,"none"]
["Fitted with steel braced radial tyres",null,null,"none"]
["Performance","Pass","Fail ","Parameter ","Response & Comments"]
["Acceleration time from zero to 100 kph by 14.0 seconds or less",null,null,"state time"]
["Emission standards conform to EURO 6 requirements",null,null,"none"]
["CO² emissions (combined figure) as low as possible below 115 gm/km",null,null,"state gm/km"]
["Diesel fuel tank capacity minimum 50 ltr",null,null,"state ltr"]
["Systems","Pass","Fail ","Parameter ","Response & Comments"]
["Fitted with power assisted steering",null,null,"none"]
["Fitted with heavy duty sealed for life battery",null,null,"none"]
["Fitted with high level rear brake lights",null,null,"none"]
["Fitted with a minimum of one rear high intensity fog light.",null,null,"none"]
["Fitted with nearside, offside and interior rear view mirrors",null,null,"none"]
["Fitted with rear windscreen wash and wiper systems",null,null,"none"]
["Brake system with ABS",null,null,"none"]
["Interior Safety","Pass","Fail ","Parameter ","Response & Comments"]
["Fitted with driver and front passenger airbags",null,null,"none"]
["Fitted with front and rear seat head rests (rear centre not essential)",null,null,"none"]
["Fitted with lap & diagonal inertia reel seat belts (rear centre static lap OK)",null,null,"none"]
["Interior Systems","Pass","Fail ","Parameter ","Response & Comments"]
["Drivers seat adjustable for height, rake & reach",null,null,"none"]
["Fitted with steering wheel column position adjustment ",null,null,"none"]
["Fitted with a heater/demister system capable of providing 25°C interior",null,null,"none"]
["Fitted with an air-conditioning system capable of providing 25°C interior",null,null,"none"]
["Fitted with radio / CD player with minimum VHF(FM) & MW(AM) reception",null,null,"none"]
["Breakdown Equipment","Pass","Fail ","Parameter ","Response & Comments"]
["Fitted with a full size or space saver spare wheel and tyre",null,null,"state type"]
["Provided with a jack and jack handle capable of lifting fully loaded vehicle",null,null,"none"]
["Provided with a wheel brace capable of unscrewing wheel nuts",null,null,"none"]
["Provided with two warning triangles",null,null,"none"]
["Registration & Delivery","Pass","Fail ","Parameter ","Response & Comments"]
["Vehicle to be registered by supplier in Republic of Cyprus",null,null,"none"]
["Vehicle to be fitted with Republic of Cyprus number plates",null,null,"none"]
["Vehicle to be delivered into BFC Vehicle Depot at RAF Akrotiri",null,null,"none"]
["Vehicle to be delivered in ready to use condition",null,null,"none"]
["Please provide a delivery timescale from start of contract.",null,null,"state timescale for delivery"]

{"sheet":"CY1142","index":4,"n_rows":66,"n_cols":5,"rows_kept":66,"cut":false,"hidden":false,"merged":[[6,0,6,4]]}
["BFC WHITE FLEET VEHICLE TECHNICAL ASSESSMENT DATA - CY1142 - CAR UTILITY ESTATE 4X2"]
[]
["Supplier:"]
["Vehicle Tendered:"]
["Date:"]
[]
["Tenderers to provide proof that they can meet the requirement by providing copies of the vehicle specification, brochure, warranty details and any other supporting evidence. "]
[]
["General Conditions","Pass","Fail","Parameter ","Response & Comments"]
["Vehicle meets all applicable current EU specifications and type approvals",null,null,"none"]
["Vehicle has a minimum 5* Euro NCAP rating",null,null,"state rating"]
["Vehicle Certificate of Conformity available",null,null,"none"]
["Vehicle meets all applicable Republic of Cyprus Transport Regulations",null,null,"none"]
["Vehicle can operate in all Republic of Cyprus environmental conditions",null,null,"none"]
["Minimum 3 year, 100, 000km full parts and labour warranty",null,null,"provide full warranty details as per specification"]
["Vehicle Configuration","Pass","Fail","Parameter ","Response & Comments"]
["Medium sized 5-door hatchback with top hinged rear door",null,null,"none"]
["Seats for 4 passengers plus driver",null,null,"none"]
["All doors lockable with central locking",null,null,"none"]
["Fitted with a laminated windscreen",null,null,"none"]
["Rear seat able to fold in separate sections flat with rear load floor",null,null,"none"]
["Rear load area volume minumum 0.45m³ with rear seats in place",null,null,"state volume"]
["Rear load area volume minumum 1.50m³ with rear seat fully folded",null,null,"state volume"]
["Costs included for specific paint finishes",null,null,"include costs in tender "]
["Vehicle Weights","Pass","Fail","Parameter ","Response & Comments"]
["Payload minimum of 475 kg",null,null,"state load"]
["Vehicle Power Train","Pass","Fail","Parameter ","Response & Comments"]
["Diesel engine drive with minimum power of 65kW",null,null,"state max kW"]
["Minimum 5 forward speed manual gearbox",null,null,"state number"]
["Engine filled with anti-freeze suitable for Cyprus conditions",null,null,"none"]
["Fitted with steel wheels",null,null,"none"]
["Fitted with steel braced radial tyres",null,null,"none"]
["Performance","Pass","Fail","Parameter ","Response & Comments"]
["Acceleration time from zero to 100 kph in 15.0 seconds or less",null,null,"state time"]
["Emission standards conform to EURO 6 requirements",null,null,"none"]
["CO² emissions (combined figure) as low as possible below 115 gm/km",null,null,"state gm/km"]
["Diesel fuel tank capacity minimum 50 ltr",null,null,"state ltr"]
["Systems","Pass","Fail","Parameter ","Response & Comments"]
["Fitted with power assisted steering",null,null,"none"]
["Fitted with heavy duty sealed for life battery",null,null,"none"]
["Fitted with high level rear brake lights",null,null,"none"]
["Fitted with a minimum of one rear high intensity fog light.",null,null,"none"]
["Fitted with nearside, offside and interior rear view mirrors",null,null,"none"]
["Fitted with rear windscreen wash and wiper systems",null,null,"none"]
["Brake system with ABS",null,null,"none"]
["Interior Safety","Pass","Fail","Parameter ","Response & Comments"]
["Fitted with driver and front passenger airbags",null,null,"none"]
["Fitted with front and rear seat head rests (rear centre not essential)",null,null,"none"]
["Fitted with lap & diagonal inertia reel seat belts (rear centre static lap OK)",null,null,"none"]
["Interior Systems","Pass","Fail","Parameter ","Response & Comments"]
["Drivers seat adjustable for height, rake & reach",null,null,"none"]
["Fitted with steering wheel column position adjustment ",null,null,"none"]
["Fitted with a heater/demister system capable of providing 25°C interior",null,null,"none"]
["Fitted with an air-conditioning system capable of providing 25°C interior",null,null,"none"]
["Fitted with radio / CD player with minimum VHF(FM) & MW(AM) reception",null,null,"none"]
["Breakdown Equipment","Pass","Fail","Parameter ","Response & Comments"]
["Fitted with a full size or space saver spare wheel and tyre",null,null,"state type"]
["Provided with a jack and jack handle capable of lifting fully loaded vehicle",null,null,"none"]
["Provided with a wheel brace capable of unscrewing wheel nuts",null,null,"none"]
["Provided with two warning triangles",null,null,"none"]
["Registration & Delivery","Pass","Fail","Parameter ","Response & Comments"]
["Vehicle to be registered by supplier in Republic of Cyprus",null,null,"none"]
["Vehicle to be fitted with Republic of Cyprus number plates",null,null,"none"]
["Vehicle to be delivered into BFC Vehicle Depot at RAF Akrotiri",null,null,"none"]
["Vehicle to be delivered in ready to use condition",null,null,"none"]
["Please provide a delivery timescale from start of contract.",null,null,"state timescale for delivery"]

{"sheet":"CY2623","index":5,"n_rows":87,"n_cols":5,"rows_kept":87,"cut":false,"hidden":false,"merged":[[6,0,6,4]]}
["BFC WHITE FLEET VEHICLE TECHNICAL ASSESSMENT DATA - CY2623 - VAN SMALL 1 TONNE 4X2 WITH DOUBLE SIDE DOORS"]
[]
["Supplier:"]
["Vehicle Tendered:"]
["Date:"]
[]
["Tenderers to provide proof that they can meet the requirement by providing copies of the vehicle specification, brochure, warranty details and any other supporting evidence. "]
[]
["General Conditions","Pass","Fail","Parameter ","Response & Comments"]
["Vehicle meets all applicable current EU specifications and type approvals",null,null,"none"]
["Vehicle has a minimum 4* Euro NCAP rating",null,null,"state rating"]
["Vehicle Certificate of Conformity available",null,null,"none"]
["Vehicle meets all applicable Republic of Cyprus Transport Regulations",null,null,"none"]
["Vehicle can operate in all Republic of Cyprus environmental conditions",null,null,"none"]
["Minimum 3 year, 100, 000km full parts and labour warranty",null,null,"provide full warranty details as per specification"]
["Vehicle Configuration","Pass","Fail","Parameter ","Response & Comments"]
["Short wheelbase low-roof panel van",null,null,"none"]
["Unladen overall height between 1.90m and 2.10m ",null,null,"state height"]
["Overall length between 4.70m and 5.40m ",null,null,"state length"]
["Overall width between 1.80m and 2.00m",null,null,"state width"]
["Wheelbase between 2.90m and 3.50m",null,null,"state length"]
["Turning circle kerb to kerb no greater than 13.0m",null,null,"state length"]
["Seats for driver and one passenger only",null,null,"none"]
["All doors lockable with central locking",null,null,"none"]
["Fitted with a laminated windscreen",null,null,"none"]
["Costs included for specific paint finishes",null,null,"include costs in tender "]
["Cargo Compartment ","Pass","Fail","Parameter ","Response & Comments"]
["Unglazed sliding door on both nearside and offside",null,null,"none"]
["Unglazed vertically split rear doors",null,null,"none"]
["Load length at floor level minimum 2,200mm",null,null,"state length"]
["Load height within range 1,350mm to 1,450mm",null,null,"state height"]
["Overall load width minimum 1,600mm",null,null,"state width"]
["Load width between wheel arches minimum 1,200mm",null,null,"state width"]
["Load deck height from ground level less than 650mm",null,null,"state height"]
["Total load volume within the range 5.0m3 to 6.0 m3.",null,null,"state volume"]
["Rear door aperture height minimum 1,250mm",null,null,"state height"]
["Rear door aperture width minimum 1,250mm",null,null,"state width"]
["Side door aperture height minimum 1,250mm",null,null,"state height"]
["Side door aperture width minimum 900mm",null,null,"state width"]
["Solid metal bulkhead between cargo compartment and cab",null,null,"none"]
["Non-slip flooring in full cargo compartment area",null,null,"none"]
["Protective liner to at least half height of the cargo compartment walls.\n\n",null,null,"none"]
["Minimum 6 cargo restraint loops",null,null,"state number"]
["Cargo Compartment interior lighting",null,null,"none"]
["Vehicle Weights","Pass","Fail","Parameter ","Response & Comments"]
["GVM no greater than 3,200 kg",null,null,"state GVM"]
["Payload minimum of 1150 kg",null,null,"state load"]
["Vehicle Power Train","Pass","Fail","Parameter ","Response & Comments"]
["Diesel engine drive with minimum power of 80 kW",null,null,"state max kW"]
["Minimum 5-speed manual gearbox",null,null,"state number"]
["Engine filled with anti-freeze suitable for Cyprus conditions",null,null,"none"]
["Fitted with steel wheels",null,null,"none"]
["Fitted with steel braced radial tyres",null,null,"none"]
["Performance","Pass","Fail","Parameter ","Response & Comments"]
["Emission standards conform to EURO 6 requirements",null,null,"none"]
["CO² emissions (combined figure) as low as possible below 180 gm/km",null,null,"state gm/km"]
["Diesel fuel tank capacity minimum 70 ltr",null,null,"state ltr"]
["Systems","Pass","Fail","Parameter ","Response & Comments"]
["Fitted with power assisted steering",null,null,"none"]
["Fitted with heavy duty sealed for life battery",null,null,"none"]
["Fitted with a high level rear brake light",null,null,"none"]
["Fitted with a minimum of one rear high intensity fog light.",null,null,"none"]
["Fitted with nearside, offside and interior rear view mirrors",null,null,"none"]
["Brake system with ABS",null,null,"none"]
["Interior Safety","Pass","Fail","Parameter ","Response & Comments"]
["Fitted with driver and front passenger airbags",null,null,"none"]
["Fitted with head rests to all seats",null,null,"none"]
["Fitted with lap & diagonal inertia reel seat belts to all seats",null,null,"none"]
["Interior Systems","Pass","Fail","Parameter ","Response & Comments"]
["Drivers seat adjustable for height, rake & reach",null,null,"none"]
["Fitted with steering wheel column position adjustment (desirable)",null,null,"none"]
["Fitted with a heater/demister system capable of providing 25°C interior",null,null,"none"]
["Fitted with an air-conditioning system capable of providing 25°C interior",null,null,"none"]
["Fitted with electrically operated cab windows",null,null,"none"]
["Fitted with electrically adjustable rear view mirrors",null,null,"none"]
["Fitted with radio / CD player with minimum VHF(FM) & MW(AM) reception",null,null,"none"]
["Breakdown Equipment","Pass","Fail","Parameter ","Response & Comments"]
["Fitted with a full size spare wheel and tyre",null,null,"none"]
["Provided with a jack and jack handle capable of lifting fully loaded vehicle",null,null,"none"]
["Provided with a wheel brace capable of unscrewing wheel nuts",null,null,"none"]
["Provided with two warning triangles",null,null,"none"]
["Registration & Delivery","Pass","Fail","Parameter ","Response & Comments"]
["Vehicle to be registered by supplier in Republic of Cyprus",null,null,"none"]
["Vehicle to be fitted with Republic of Cyprus number plates",null,null,"none"]
["Vehicle to be delivered into BFC Vehicle Depot at RAF Akrotiri",null,null,"none"]
["Vehicle to be delivered in ready to use condition",null,null,"none"]
["Please provide a delivery timescale from start of contract.",null,null,"state timescale for delivery"]