|  |  |
| --- | --- |
| **Item** | **Rate** |
| General Contractors Preliminaries |  |
| Provision of black powder coated pedestrian barriers to the perimeter of the quaysides |  |
| Installation of lockable gate to the central quayside |  |
| Installation of high level fencing between GWR building and sub-station structure |  |
| Clean and make good of cobbled surfaces where required |  |
| Installation of security cages to tar boilers and electrical location cabinets |  |
| Installation of LED lighting to existing lamp standards |  |
| Painting and repairs to existing shipkeeping storage containers |  |
| Cladding and repairs to existing shipkeeping Portacabin |  |
| Removal and disposal from site of waste materials |  |
| Installation of warning signage |  |
| General builders work in connection and making good |  |
| Provision of As-Built drawings and O&M manuals for all works as necessary |  |
| **Total** |  |