Appendix 5

Broadway Play Area

Paving specification:

Finished length 16 metres

Dig out grass and soil – remove from site.

Lay pin kerb retainers, type 1 subbase and well compacted.

600x600 grey paving stones laid on a base of sharp sand and cement.

Remove all excess materials from site.