Appendix 4

South Beach Play Area

Specification for Play Area:

The play area is more rectangular in shape of some 280 square metres.

The surface will be that of black wet-pour with required base preparation as below.

The existing surface when removed will need the depth of the subbase to be checked to ensure there is a minimum depth of 150mm and additional subbase to be added if required. A maximum of 20mm of wet-pour is required, to the finished final level. (Please see Appendix 4a)

Bowes Street Play Area

Specification for Play Area:

The play area required is more rectangular in shape of some 303 square metres.

The surface will be that of black wet-pour with required base preparation. The present surface is bark chip, and this will be removed and give an approximate depth of 300mm. This will need to be built back up with Type 1 sub-base to allow for a minimum of 20mm wet pour to the final finished level.

There will be a need to install pin kerbs around the boundary as there is currently a timber edge to retain the play chip, this may also need to be removed to allow the installation of the kerbs. (Please see Appendix 4b)