{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Schedule C"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Schedule C","index":0,"n_rows":432,"n_cols":5,"rows_kept":432,"cut":false,"hidden":false,"merged":[]}
["Level","Item","Bill description","Unit","Price (£)"]
[1,"","SERIES 500 DRAINAGE AND SERVICE DUCTS (Scope Paragraph 18.4.3)",""]
["c","","Filter Drains",""]
["c","","Excavate and replace filter material; in verges or edge of carriageway;",""]
[null,"1","Type A filter material.","m³"]
[null,"2","Type B filter material.","m³"]
[null,"3","Type C filter material.","m³"]
["c","","Excavate and replace filter material; in side slopes of cuttings or side slopes of embankments;",""]
[null,"4","Type A filter material.","m³"]
[null,"5","Type B filter material.","m³"]
[null,"6","Type C filter material.","m³"]
["c","","Renewal, Raising or Lowering of Covers and Gratings on Existing Chambers and Gullies",""]
["c","","Renewal; cover size 600mm x 600mm; all chamber sizes; all chamber construction types; not exceeding 150mm;",""]
[null,"7","Class B125.","no"]
[null,"8","Class C250.","no"]
[null,"9","Class D400.","no"]
["c","","Renewal; grating size 450mm x 450mm; all gully sizes; all gully construction types; not exceeding 150mm;",""]
[null,"10","Class B125.","no"]
[null,"11","Class C250.","no"]
[null,"12","Class D400.","no"]
["c","","Raising the level; cover size 600mm x 600mm; all chamber sizes; all chamber construction types; not exceeding 150mm;",""]
[null,"13","All types.","no"]
["c","","Raising the level; grating size 450mm x 450mm; all chamber sizes; all chamber construction types; not exceeding 150mm;",""]
[null,"14","All types.","no"]
["c","","Lowering the level; grating size 450mm x 450mm; all chamber sizes; all chamber construction types; not exceeding 150mm;",""]
[null,"15","All types.","no"]
["c","","Cleaning Existing Drainage Systems",""]
["c","","Cleaning; piped drainage system; accessed from pavements, footways and/or paved areas not requiring all-terrain vehicles; not exceeding 20 metres;",""]
[null,"16","Internal diameter not exceeding nominal 150mm.","m"]
[null,"17","Internal diameter exceeding nominal 150mm but not exceeding nominal 225mm.","m"]
[null,"18","Internal diameter exceeding nominal 225mm but not exceeding nominal 300mm.","m"]
[null,"19","Internal diameter exceeding nominal 300mm but not exceeding nominal 450mm.","m"]
["c","","Cleaning; piped drainage system; accessed from pavements, footways and/or paved areas not requiring all-terrain vehicles; exceeding 20 metres but not exceeding 50 metres;",""]
[null,"20","Internal diameter not exceeding nominal 150mm.","m"]
[null,"21","Internal diameter exceeding nominal 150mm but not exceeding nominal 225mm.","m"]
[null,"22","Internal diameter exceeding nominal 225mm but not exceeding nominal 300mm.","m"]
[null,"23","Internal diameter exceeding nominal 300mm but not exceeding nominal 450mm.","m"]
["c","","Cleaning; piped drainage system; accessed from pavements, footways and/or paved areas not requiring all-terrain vehicles; exceeding 50 metres but not exceeding 100 metres;",""]
[null,"24","Internal diameter not exceeding nominal 150mm.","m"]
[null,"25","Internal diameter exceeding nominal 150mm but not exceeding nominal 225mm.","m"]
[null,"26","Internal diameter exceeding nominal 225mm but not exceeding nominal 300mm.","m"]
[null,"27","Internal diameter exceeding nominal 300mm but not exceeding nominal 450mm.","m"]
["c","","Cleaning; piped drainage system; accessed from pavements, footways and/or paved areas not requiring all-terrain vehicles; exceeding 100 metres;",""]
[null,"28","Internal diameter not exceeding nominal 150mm.","m"]
[null,"29","Internal diameter exceeding nominal 150mm but not exceeding nominal 225mm.","m"]
[null,"30","Internal diameter exceeding nominal 225mm but not exceeding nominal 300mm.","m"]
[null,"31","Internal diameter exceeding nominal 300mm but not exceeding nominal 450mm.","m"]
["c","","Cleaning; piped drainage system; accessed from pavements, footways and/or paved areas requiring all-terrain vehicles; not exceeding 20 metres;",""]
[null,"32","Internal diameter not exceeding nominal 150mm.","m"]
[null,"33","Internal diameter exceeding nominal 150mm but not exceeding nominal 225mm.","m"]
[null,"34","Internal diameter exceeding nominal 225mm but not exceeding nominal 300mm.","m"]
[null,"35","Internal diameter exceeding nominal 300mm but not exceeding nominal 450mm.","m"]
["c","","Cleaning; piped drainage system; accessed from pavements, footways and/or paved areas requiring all-terrain vehicles; exceeding 20 metres but not exceeding 50 metres;",""]
[null,"36","Internal diameter not exceeding nominal 150mm.","m"]
[null,"37","Internal diameter exceeding nominal 150mm but not exceeding nominal 225mm.","m"]
[null,"38","Internal diameter exceeding nominal 225mm but not exceeding nominal 300mm.","m"]
[null,"39","Internal diameter exceeding nominal 300mm but not exceeding nominal 450mm.","m"]
["c","","Cleaning; piped drainage system; accessed from pavements, footways and/or paved areas requiring all-terrain vehicles; exceeding 50 metres but not exceeding 100 metres;",""]
[null,"40","Internal diameter not exceeding nominal 150mm.","m"]
[null,"41","Internal diameter exceeding nominal 150mm but not exceeding nominal 225mm.","m"]
[null,"42","Internal diameter exceeding nominal 225mm but not exceeding nominal 300mm.","m"]
[null,"43","Internal diameter exceeding nominal 300mm but not exceeding nominal 450mm.","m"]
["c","","Cleaning; piped drainage system; accessed from pavements, footways and/or paved areas requiring all-terrain vehicles; exceeding 100 metres;",""]
[null,"44","Internal diameter not exceeding nominal 150mm.","m"]
[null,"45","Internal diameter exceeding nominal 150mm but not exceeding nominal 225mm.","m"]
[null,"46","Internal diameter exceeding nominal 225mm but not exceeding nominal 300mm.","m"]
[null,"47","Internal diameter exceeding nominal 300mm but not exceeding nominal 450mm.","m"]
["c","","Cleaning; catchpits; accessed from pavements, footways and/or paved areas not requiring all-terrain vehicles; not exceeding 3 number;",""]
[null,"48","All sizes.","no"]
["c","","Cleaning; catchpits; accessed from pavements, footways and/or paved areas not requiring all-terrain vehicles; exceeding 3 number bit not exceeding 10 number;",""]
[null,"49","All sizes.","no"]
["c","","Cleaning; catchpits; accessed from pavements, footways and/or paved areas not requiring all-terrain vehicles; exceeding 10 number;",""]
[null,"50","All sizes.","no"]
["c","","Cleaning; manholes; accessed from pavements, footways and/or paved areas not requiring all-terrain vehicles; not exceeding 3 number;",""]
[null,"51","Rectangular or square chambers not exceeding 1000mm in length.","no"]
[null,"52","Internal diameter not exceeding 1500mm.","no"]
[null,"53","Internal diameter exceeding 1500mm but not exceeding 2100mm.","no"]
[null,"54","Internal diameter exceeding 2100mm.","no"]
["c","","Cleaning; manholes; accessed from pavements, footways and/or paved areas not requiring all-terrain vehicles; exceeding 3 number bit not exceeding 10 number;",""]
[null,"55","Rectangular or square chambers not exceeding 1000mm in length.","no"]
[null,"56","Internal diameter not exceeding 1500mm.","no"]
[null,"57","Internal diameter exceeding 1500mm but not exceeding 2100mm.","no"]
[null,"58","Internal diameter exceeding 2100mm.","no"]
["c","","Cleaning; manholes; accessed from pavements, footways and/or paved areas not requiring all-terrain vehicles; exceeding 10 number;",""]
[null,"59","Rectangular or square chambers not exceeding 1000mm in length.","no"]
[null,"60","Internal diameter not exceeding 1500mm.","no"]
[null,"61","Internal diameter exceeding 1500mm but not exceeding 2100mm.","no"]
[null,"62","Internal diameter exceeding 2100mm.","no"]
["c","","Cleaning; manholes; accessed from pavements, footways and/or paved areas requiring all-terrain vehicles; not exceeding 3 number;",""]
[null,"63","Rectangular or square chambers not exceeding 1000mm in length.","no"]
[null,"64","Internal diameter not exceeding 1500mm.","no"]
[null,"65","Internal diameter exceeding 1500mm but not exceeding 2100mm.","no"]
[null,"66","Internal diameter exceeding 2100mm.","no"]
["c","","Cleaning; manholes; accessed from pavements, footways and/or paved areas requiring all-terrain vehicles; exceeding 3 number bit not exceeding 10 number;",""]
[null,"67","Rectangular or square chambers not exceeding 1000mm in length.","no"]
[null,"68","Internal diameter not exceeding 1500mm.","no"]
[null,"69","Internal diameter exceeding 1500mm but not exceeding 2100mm.","no"]
[null,"70","Internal diameter exceeding 2100mm.","no"]
["c","","Cleaning; manholes; accessed from pavements, footways and/or paved areas requiring all-terrain vehicles; exceeding 10 number;",""]
[null,"71","Rectangular or square chambers not exceeding 1000mm in length.","no"]
[null,"72","Internal diameter not exceeding 1500mm.","no"]
[null,"73","Internal diameter exceeding 1500mm but not exceeding 2100mm.","no"]
[null,"74","Internal diameter exceeding 2100mm.","no"]
["c","","Cleaning; gullies; all locations; not exceeding 20 number;",""]
[null,"75","All sizes.","no"]
["c","","Cleaning; gullies; all locations; exceeding 20 number but not exceeding 50 number;",""]
[null,"76","All sizes.","no"]
["c","","Cleaning; gullies; all locations; exceeding 50 number but not exceeding 100 number;",""]
[null,"77","All sizes.","no"]
["c","","Cleaning; gullies; all locations; exceeding 100 number;",""]
[null,"78","All sizes.","no"]
["c","","Cleaning; gully covers and aprons; all locations; not exceeding 20 number;",""]
[null,"79","All sizes.","no"]
["c","","Cleaning; gully covers and aprons; all locations; exceeding 20 number but not exceeding 50 number;",""]
[null,"80","All sizes.","no"]
["c","","Cleaning; gully covers and aprons; all locations; exceeding 50 number but not exceeding 100 number;",""]
[null,"81","All sizes.","no"]
["c","","Cleaning; gully covers and aprons; all locations; exceeding 100 number;",""]
[null,"82","All sizes.","no"]
["c","","Cleaning; Interceptors; all locations; not exceeding 20 number;",""]
[null,"83","All sizes.","no"]
["c","","Cleaning; Interceptors; all locations; exceeding 20 number but not exceeding 50 number;",""]
[null,"84","All sizes.","no"]
["c","","Cleaning; Interceptors; all locations; exceeding 50 number but not exceeding 100 number;",""]
[null,"85","All sizes.","no"]
["c","","Cleaning; Interceptors; all locations; exceeding 100 number;",""]
[null,"86","All sizes.","no"]
["c","","Cleaning; Soakaways; Priority soakaways; all locations;",""]
[null,"87","Volume not exceeding 50m3","m3"]
[null,"88","Volume exceeding 50m3 in steps of 50m3","m3"]
["c","","Cleaning; Soakaways; Non priority soakaways; all locations;",""]
[null,"89","Volume not exceeding 50m3","m3"]
[null,"90","Volume exceeding 50m3 in steps of 50m3","m3"]
["c","","Replacement of Drains in Trenches",""]
["c","","Replacement of drains in trenches; to MCHW HCD F1; in verges or edge of carriageway; not exceeding 15 metres in length per length of replacement;",""]
[null,"91","150mm internal diameter; average depth to invert 1.5 metres; trench type Z.","m"]
[null,"92","Adjustment of the rate in item 71 above where the average depth to invert varies by NIL mm to and including 250mm.","m"]
[null,"93","Adjustment of the rate in item 71 above where the average depth to invert varies by 251 mm to and including 500mm.","m"]
[null,"94","Adjustment of the rate in item 71 above where the average depth to invert varies by 501 mm to and including 750mm.","m"]
[null,"95","Adjustment of the rate in item 71 above where the average depth to invert varies by 751 mm to and including 1000mm.","m"]
[null,"96","225mm internal diameter; average depth to invert 1.5 metres; trench type Z.","m"]
[null,"97","Adjustment of the rate in item 75 above where the average depth to invert varies by NIL mm to and including 250mm.","m"]
[null,"98","Adjustment of the rate in item 75 above where the average depth to invert varies by 251 mm to and including 500mm.","m"]
[null,"99","Adjustment of the rate in item 75 above where the average depth to invert varies by 501 mm to and including 750mm.","m"]
[null,"100","Adjustment of the rate in item 75 above where the average depth to invert varies by 751 mm to and including 1000mm.","m"]
[null,"101","300mm internal diameter; average depth to invert 2.0 metres; trench type B.","m"]
[null,"102","Adjustment of the rate in item 80 above where the average depth to invert varies by NIL mm to and including 250mm.","m"]
[null,"103","Adjustment of the rate in item 80 above where the average depth to invert varies by 251 mm to and including 500mm.","m"]
[null,"104","Adjustment of the rate in item 80 above where the average depth to invert varies by 501 mm to and including 750mm.","m"]
[null,"105","Adjustment of the rate in item 80 above where the average depth to invert varies by 751 mm to and including 1000mm.","m"]
["c","","Replacement of drains in trenches; to MCHW HCD F1; in side slopes of cuttings or side slopes of embankments; not exceeding 15 metres in length per length of replacement;",""]
[null,"106","150mm internal diameter; average depth to invert 1.5 metres; trench type Z.","m"]
[null,"107","Adjustment of the rate in item 85 above where the average depth to invert varies by NIL mm to and including 250mm.","m"]
[null,"108","Adjustment of the rate in item 85 above where the average depth to invert varies by 251 mm to and including 500mm.","m"]
[null,"109","Adjustment of the rate in item 85 above where the average depth to invert varies by 501 mm to and including 750mm.","m"]
[null,"110","Adjustment of the rate in item 85 above where the average depth to invert varies by 751 mm to and including 1000mm.","m"]
[null,"111","225mm internal diameter; average depth to invert 1.5 metres; trench type Z.","m"]
[null,"112","Adjustment of the rate in item 90 above where the average depth to invert varies by NIL mm to and including 250mm.","m"]
[null,"113","Adjustment of the rate in item 90 above where the average depth to invert varies by 251 mm to and including 500mm.","m"]
[null,"114","Adjustment of the rate in item 90 above where the average depth to invert varies by 501 mm to and including 750mm.","m"]
[null,"115","Adjustment of the rate in item 90 above where the average depth to invert varies by 751 mm to and including 1000mm.","m"]
[null,"116","300mm internal diameter; average depth to invert 2.0 metres; trench type B.","m"]
[null,"117","Adjustment of the rate in item 95 above where the average depth to invert varies by NIL mm to and including 250mm.","m"]
[null,"118","Adjustment of the rate in item 95 above where the average depth to invert varies by 251 mm to and including 500mm.","m"]
[null,"119","Adjustment of the rate in item 95 above where the average depth to invert varies by 501 mm to and including 750mm.","m"]
[null,"120","Adjustment of the rate in item 95 above where the average depth to invert varies by 751 mm to and including 1000mm.","m"]
["c","","Replacement of drains in trenches; to MCHW HCD F1; in verges or edge of carriageway; exceeding 15 metres in length per length of replacement;",""]
[null,"121","150mm internal diameter; average depth to invert 1.5 metres; trench type Z.","m"]
[null,"122","Adjustment of the rate in item 100 above where the average depth to invert varies by NIL mm to and including 250mm.","m"]
[null,"123","Adjustment of the rate in item 100 above where the average depth to invert varies by 251 mm to and including 500mm.","m"]
[null,"124","Adjustment of the rate in item 100 above where the average depth to invert varies by 501 mm to and including 750mm.","m"]
[null,"125","Adjustment of the rate in item 100 above where the average depth to invert varies by 751 mm to and including 1000mm.","m"]
[null,"126","225mm internal diameter; average depth to invert 1.5 metres; trench type Z.","m"]
[null,"127","Adjustment of the rate in item 105 above where the average depth to invert varies by NIL mm to and including 250mm.","m"]
[null,"128","Adjustment of the rate in item 105 above where the average depth to invert varies by 251 mm to and including 500mm.","m"]
[null,"129","Adjustment of the rate in item 105 above where the average depth to invert varies by 501 mm to and including 750mm.","m"]
[null,"130","Adjustment of the rate in item 105 above where the average depth to invert varies by 751 mm to and including 1000mm.","m"]
[null,"131","300mm internal diameter; average depth to invert 2.0 metres; trench type B.","m"]
[null,"132","Adjustment of the rate in item 110 above where the average depth to invert varies by NIL mm to and including 250mm.","m"]
[null,"133","Adjustment of the rate in item 110 above where the average depth to invert varies by 251 mm to and including 500mm.","m"]
[null,"134","Adjustment of the rate in item 110 above where the average depth to invert varies by 501 mm to and including 750mm.","m"]
[null,"135","Adjustment of the rate in item 110 above where the average depth to invert varies by 751 mm to and including 1000mm.","m"]
["c","","Replacement of drains in trenches; to MCHW HCD F1; in side slopes of cuttings or side slopes of embankments; exceeding 15 metres in length per length of replacement;",""]
[null,"136","150mm internal diameter; average depth to invert 1.5 metres; trench type Z.","m"]
[null,"137","Adjustment of the rate in item 115 above where the average depth to invert varies by NIL mm to and including 250mm.","m"]
[null,"138","Adjustment of the rate in item 115 above where the average depth to invert varies by 251 mm to and including 500mm.","m"]
[null,"139","Adjustment of the rate in item 115 above where the average depth to invert varies by 501 mm to and including 750mm.","m"]
[null,"140","Adjustment of the rate in item 115 above where the average depth to invert varies by 751 mm to and including 1000mm.","m"]
[null,"141","225mm internal diameter; average depth to invert 1.5 metres; trench type Z.","m"]
[null,"142","Adjustment of the rate in item 120 above where the average depth to invert varies by NIL mm to and including 250mm.","m"]
[null,"143","Adjustment of the rate in item 120 above where the average depth to invert varies by 251 mm to and including 500mm.","m"]
[null,"144","Adjustment of the rate in item 120 above where the average depth to invert varies by 501 mm to and including 750mm.","m"]
[null,"145","Adjustment of the rate in item 120 above where the average depth to invert varies by 751 mm to and including 1000mm.","m"]
[null,"146","300mm internal diameter; average depth to invert 2.0 metres; trench type B.","m"]
[null,"147","Adjustment of the rate in item 125 above where the average depth to invert varies by NIL mm to and including 250mm.","m"]
[null,"148","Adjustment of the rate in item 125 above where the average depth to invert varies by 251 mm to and including 500mm.","m"]
[null,"149","Adjustment of the rate in item 125 above where the average depth to invert varies by 501 mm to and including 750mm.","m"]
[null,"150","Adjustment of the rate in item 125 above where the average depth to invert varies by 751 mm to and including 1000mm.","m"]
["c","","Replacement of Connections to Drains, Piped Culverts, Chambers and Land or Mole Drains",""]
["c","","Extra over replacement of drains in trenches; replacement of connection to drain;",""]
[null,"151","Internal diameters 150mm drain to 150mm drain.","no"]
[null,"152","Internal diameters 150mm drain to 225mm drain.","no"]
[null,"153","Internal diameters 150mm drain to 300mm drain and above.","no"]
["c","","Extra over replacement of drains in trenches; replacement of connection to piped culvert;",""]
[null,"154","Internal diameters 150mm drain to piped culvert of all diameters.","no"]
[null,"155","Internal diameters 225mm drain to piped culvert of all diameters.","no"]
["c","","Extra over replacement of drains in trenches; replacement of connection to chamber;",""]
[null,"156","Internal diameters 150mm drain to chamber of all diameters.","no"]
[null,"157","Internal diameters 225mm drain to chamber of all diameters.","no"]
[null,"158","Internal diameters 300mm drain to chamber of all diameters.","no"]
["c","","Extra over replacement of drains in trenches; replacement of connection to land or mole drain;",""]
[null,"159","Internal diameters 100mm land or mole drain to drain of all diameters.","no"]
["c","","Replacement of Gullies",""]
[null,"160","Replacement of gullies; as MCHW HCD F13; Class D400 grating.","no"]
["c","","Drainage (repair defects, not resulting from an incident caused by a third party) and Disposal of Waste",""]
["c","","Drainage (repair defects, not resulting from an incident caused by a third party)",""]
[null,"161","Gully emptier including driver and operative.","hr"]
[null,"162","Vactor unit including driver and operative.","hr"]
[null,"163","CCTV unit including technician.","hr"]
["c","","Disposal of waste;",""]
[null,"164","Inert waste.","t"]
[null,"165","Wet waste gully emptying arisings.","t"]
[null,"166","Wet waste drainage arisings.","t"]
[null,"167","Green waste.","t"]
[1,"","Series 700 PAVEMENTS (Scope Paragraph 18.6.1)",""]
["c","","Repairs and Patching",""]
["c","","Local Repairs not exceeding 5 number Local Repairs per Task;",""]
[null,"1","In carriageways.","kg"]
[null,"2","In footways.","kg"]
["c","","Local Repairs exceeding 5 but not exceeding 20 number Local Repairs per Task;",""]
[null,"3","In carriageways.","kg"]
[null,"4","In footways.","kg"]
["c","","Local Repairs exceeding 20 number Local Repairs per Task;",""]
[null,"5","In carriageways.","kg"]
[null,"6","In footways.","kg"]
[2,"","Hand Lay Patching",""]
["c","","Patching; Hand lay; not exceeding 10 square metres of patching per Task;",""]
["c","","Individual patch area not exceeding 1 square metre; in carriageways;",""]
[null,"7","Material ref: WC1 or WC2; layer not exceeding 50mm thick","m2"]
[null,"8","Material ref: WC1 or WC2; layer not exceeding 50mm thick laid over material refs BC1 or BC3 layer not exceeding 100mm thick; combined thickness not exceeding 150mm.","m2"]
[null,"9","Material ref: WC1 or WC2; layer not exceeding 50mm thick laid over material refs BC1 or BC3 layer not exceeding 100mm thick laid over material refs: BA1 or BA3 layer not exceeding 200mm thick; combined thickness not exceeding 350mm.","m2"]
["c","","Individual patch area not exceeding 5 square metres; in footways and paved areas;",""]
[null,"10","Material ref: PWC1 or FWC1; layer not exceeding 25mm thick","m2"]
[null,"11","Material ref: PWC1 or FWC1; layer not exceeding 25mm thick laid over material refs PBC1 or FBC1 layer not exceeding 75mm thick; combined thickness not exceeding 100mm.","m2"]
["c","","Individual patch area exceeding 5 square metres but not exceeding 10 square metres; in footways and paved areas;",""]
[null,"12","Material ref: PWC1 or FWC1; layer not exceeding 25mm thick","m2"]
[null,"13","Material ref: PWC1 or FWC1; layer not exceeding 25mm thick laid over material refs PBC1 or FBC1 layer not exceeding 75mm thick; combined thickness not exceeding 100mm.","m2"]
["c","","Patching; Hand lay; exceeding 10 square metres but not exceeding 20 square metres of patching per Task;",""]
["c","","Individual patch area not exceeding 1 square metre; in carriageways;",""]
[null,"14","Material ref: WC1 or WC2; layer not exceeding 50mm thick","m2"]
[null,"15","Material ref: WC1 or WC2; layer not exceeding 50mm thick laid over material refs BC1 or BC3 layer not exceeding 100mm thick; combined thickness not exceeding 150mm.","m2"]
[null,"16","Material ref: WC1 or WC2; layer not exceeding 50mm thick laid over material refs BC1 or BC3 layer not exceeding 100mm thick laid over material refs: BA1 or BA3 layer not exceeding 200mm thick; combined thickness not exceeding 350mm.","m2"]
["c","","Individual patch area not exceeding 5 square metres; in footways and paved areas;",""]
[null,"17","Material ref: PWC1 or FWC1; layer not exceeding 25mm thick","m2"]
[null,"18","Material ref: PWC1 or FWC1; layer not exceeding 25mm thick laid over material refs PBC1 or FBC1 layer not exceeding 75mm thick; combined thickness not exceeding 100mm.","m2"]
["c","","Individual patch area exceeding 5 square metres but not exceeding 10 square metres; in footways and paved areas;",""]
[null,"19","Material ref: PWC1 or FWC1; layer not exceeding 25mm thick","m2"]
[null,"20","Material ref: PWC1 or FWC1; layer not exceeding 25mm thick laid over material refs PBC1 or FBC1 layer not exceeding 75mm thick; combined thickness not exceeding 100mm.","m2"]
["c","","Individual patch area exceeding 10 square metres but not exceeding 15 square metres; in footways and paved areas;",""]
[null,"21","Material ref: PWC1 or FWC1; layer not exceeding 25mm thick","m2"]
[null,"22","Material ref: PWC1 or FWC1; layer not exceeding 25mm thick laid over material refs PBC1 or FBC1 layer not exceeding 75mm thick; combined thickness not exceeding 100mm.","m2"]
["c","","Individual patch area exceeding 15 square metres but not exceeding 20 square metres; in footways and paved areas;",""]
[null,"23","Material ref: PWC1 or FWC1; layer not exceeding 25mm thick","m2"]
[null,"24","Material ref: PWC1 or FWC1; layer not exceeding 25mm thick laid over material refs PBC1 or FBC1 layer not exceeding 75mm thick; combined thickness not exceeding 100mm.","m2"]
["c","","Patching; Hand lay; exceeding 20 square metres but not exceeding 50 square metres of patching per Task;",""]
["c","","Individual patch area not exceeding 1 square metre; in carriageways;",""]
[null,"25","Material ref: WC1 or WC2; layer not exceeding 50mm thick","m2"]
[null,"26","Material ref: WC1 or WC2; layer not exceeding 50mm thick laid over material refs BC1 or BC3 layer not exceeding 100mm thick; combined thickness not exceeding 150mm.","m2"]
[null,"27","Material ref: WC1 or WC2; layer not exceeding 50mm thick laid over material refs BC1 or BC3 layer not exceeding 100mm thick laid over material refs: BA1 or BA3 layer not exceeding 200mm thick; combined thickness not exceeding 350mm.","m2"]
["c","","Individual patch area not exceeding 5 square metres; in footways and paved areas;",""]
[null,"28","Material ref: PWC1 or FWC1; layer not exceeding 25mm thick","m2"]
[null,"29","Material ref: PWC1 or FWC1; layer not exceeding 25mm thick laid over material refs PBC1 or FBC1 layer not exceeding 75mm thick; combined thickness not exceeding 100mm.","m2"]
["c","","Individual patch area exceeding 5 square metres but not exceeding 10 square metres; in footways and paved areas;",""]
[null,"30","Material ref: PWC1 or FWC1; layer not exceeding 25mm thick","m2"]
[null,"31","Material ref: PWC1 or FWC1; layer not exceeding 25mm thick laid over material refs PBC1 or FBC1 layer not exceeding 75mm thick; combined thickness not exceeding 100mm.","m2"]
["c","","Individual patch area exceeding 10 square metres but not exceeding 15 square metres; in footways and paved areas;",""]
[null,"32","Material ref: PWC1 or FWC1; layer not exceeding 25mm thick","m2"]
[null,"33","Material ref: PWC1 or FWC1; layer not exceeding 25mm thick laid over material refs PBC1 or FBC1 layer not exceeding 75mm thick; combined thickness not exceeding 100mm.","m2"]
["c","","Individual patch area exceeding 15 square metres but not exceeding 20 square metres; in footways and paved areas;",""]
[null,"34","Material ref: PWC1 or FWC1; layer not exceeding 25mm thick","m2"]
[null,"35","Material ref: PWC1 or FWC1; layer not exceeding 25mm thick laid over material refs PBC1 or FBC1 layer not exceeding 75mm thick; combined thickness not exceeding 100mm.","m2"]
["c","","Individual patch area exceeding 20 square metres but not exceeding 50 square metres; in footways and paved areas;",""]
[null,"36","Material ref: PWC1 or FWC1; layer not exceeding 25mm thick","m2"]
[null,"37","Material ref: PWC1 or FWC1; layer not exceeding 25mm thick laid over material refs PBC1 or FBC1 layer not exceeding 75mm thick; combined thickness not exceeding 100mm.","m2"]
["c","","Patching; Hand lay; exceeding 50 square metres of patching per Task;",""]
["c","","Individual patch area not exceeding 1 square metre; in carriageways;",""]
[null,"38","Material ref: WC1 or WC2; layer not exceeding 50mm thick","m2"]
[null,"39","Material ref: WC1 or WC2; layer not exceeding 50mm thick laid over material refs BC1 or BC3 layer not exceeding 100mm thick; combined thickness not exceeding 150mm.","m2"]
[null,"40","Material ref: WC1 or WC2; layer not exceeding 50mm thick laid over material refs BC1 or BC3 layer not exceeding 100mm thick laid over material refs: BA1 or BA3 layer not exceeding 200mm thick; combined thickness not exceeding 350mm.","m2"]
["c","","Individual patch area not exceeding 5 square metres; in footways and paved areas;",""]
[null,"41","Material ref: PWC1 or FWC1; layer not exceeding 25mm thick","m2"]
[null,"42","Material ref: PWC1 or FWC1; layer not exceeding 25mm thick laid over material refs PBC1 or FBC1 layer not exceeding 75mm thick; combined thickness not exceeding 100mm.","m2"]
["c","","Individual patch area exceeding 5 square metres but not exceeding 10 square metres; in footways and paved areas;",""]
[null,"43","Material ref: PWC1 or FWC1; layer not exceeding 25mm thick","m2"]
[null,"44","Material ref: PWC1 or FWC1; layer not exceeding 25mm thick laid over material refs PBC1 or FBC1 layer not exceeding 75mm thick; combined thickness not exceeding 100mm.","m2"]
["c","","Individual patch area exceeding 10 square metres but not exceeding 15 square metres; in footways and paved areas;",""]
[null,"45","Material ref: PWC1 or FWC1; layer not exceeding 25mm thick","m2"]
[null,"46","Material ref: PWC1 or FWC1; layer not exceeding 25mm thick laid over material refs PBC1 or FBC1 layer not exceeding 75mm thick; combined thickness not exceeding 100mm.","m2"]
["c","","Individual patch area exceeding 15 square metres but not exceeding 20 square metres; in footways and paved areas;",""]
[null,"47","Material ref: PWC1 or FWC1; layer not exceeding 25mm thick","m2"]
[null,"48","Material ref: PWC1 or FWC1; layer not exceeding 25mm thick laid over material refs PBC1 or FBC1 layer not exceeding 75mm thick; combined thickness not exceeding 100mm.","m2"]
["c","","Individual patch area exceeding 20 square metres but not exceeding 50 square metres; in footways and paved areas;",""]
[null,"49","Material ref: PWC1 or FWC1; layer not exceeding 25mm thick","m2"]
[null,"50","Material ref: PWC1 or FWC1; layer not exceeding 25mm thick laid over material refs PBC1 or FBC1 layer not exceeding 75mm thick; combined thickness not exceeding 100mm.","m2"]
["c","","Individual patch area exceeding 50 square metres; in footways and paved areas;",""]
[null,"51","Material ref: PWC1 or FWC1; layer not exceeding 25mm thick","m2"]
[null,"52","Material ref: PWC1 or FWC1; layer not exceeding 25mm thick laid over material refs PBC1 or FBC1 layer not exceeding 75mm thick; combined thickness not exceeding 100mm.","m2"]
[2,"","Patching; Machine lay; exceeding 10 square metres but not exceeding 20 square metres of patching per Task;",""]
["c","","Individual patch area not exceeding 5 square metres; in carriageways;",""]
[null,"53","Material ref: WC1 or WC2; layer not exceeding 50mm thick","m2"]
[null,"54","Material refs: WC1 or WC2; layer not exceeding 50mm thick laid over material refs BC1 or BC3 layer not exceeding 100mm thick; combined thickness not exceeding 150mm.","m2"]
[null,"55","Material refs: WC1 or WC2; layer not exceeding 50mm thick laid over material refs BC1 or BC3 layer not exceeding 100mm thick laid over material refs: BA1 or BA3 layer not exceeding 200mm thick; combined thickness not exceeding 350mm.","m2"]
["c","","Individual patch area exceeding 5 square metres but not exceeding 10 square metres; in carriageways;",""]
[null,"56","Material ref: WC1 or WC2; layer not exceeding 50mm thick","m2"]
[null,"57","Material refs: WC1 or WC2; layer not exceeding 50mm thick laid over material refs BC1 or BC3 layer not exceeding 100mm thick; combined thickness not exceeding 150mm.","m2"]
[null,"58","Material refs: WC1 or WC2; layer not exceeding 50mm thick laid over material refs BC1 or BC3 layer not exceeding 100mm thick laid over material refs: BA1 or BA3 layer not exceeding 200mm thick; combined thickness not exceeding 350mm.","m2"]
[null,"59","Material ref: WC5; layer not exceeding 50mm thick","m2"]
[null,"60","Material refs: WC5; layer not exceeding 50mm thick laid over material refs BC1 or BC3 layer not exceeding 100mm thick; combined thickness not exceeding 150mm.","m2"]
[null,"61","Material refs: WC5; layer not exceeding 50mm thick laid over material refs BC1 or BC3 layer not exceeding 100mm thick laid over material refs:  BA1 or BA3 layer not exceeding 200mm thick; combined thickness not exceeding 350mm.","m2"]
[null,"62","Material ref: WC6; layer not exceeding 50mm thick","m2"]
[null,"63","Material refs: WC6; layer not exceeding 50mm thick laid over material refs BC1 or BC3 layer not exceeding 100mm thick; combined thickness not exceeding 150mm.","m2"]
[null,"64","Material refs: WC6; layer not exceeding 50mm thick laid over material refs BC1 or BC3 layer not exceeding 100mm thick laid over material refs:  BA1 or BA3 layer not exceeding 200mm thick; combined thickness not exceeding 350mm.","m2"]
[null,"65","Material ref: WC8; layer not exceeding 50mm thick","m2"]
[null,"66","Material refs: WC8; layer not exceeding 50mm thick laid over material refs BC1 or BC3 layer not exceeding 100mm thick; combined thickness not exceeding 150mm.","m2"]
[null,"67","Material refs: WC8; layer not exceeding 50mm thick laid over material refs BC1 or BC3 layer not exceeding 100mm thick laid over material refs:  BA1 or BA3 layer not exceeding 200mm thick; combined thickness not exceeding 350mm.","m2"]
["c","","Individual patch area exceeding 10 square metres but not exceeding 15 square metres; in carriageways;",""]
[null,"68","Material ref: WC1 or WC2; layer not exceeding 50mm thick","m2"]
[null,"69","Material refs: WC1 or WC2; layer not exceeding 50mm thick laid over material refs BC1 or BC3 layer not exceeding 100mm thick; combined thickness not exceeding 150mm.","m2"]
[null,"70","Material refs: WC1 or WC2; layer not exceeding 50mm thick laid over material refs BC1 or BC3 layer not exceeding 100mm thick laid over material refs: BA1 or BA3 layer not exceeding 200mm thick; combined thickness not exceeding 350mm.","m2"]
[null,"71","Material ref: WC5; layer not exceeding 50mm thick","m2"]
[null,"72","Material refs: WC5; layer not exceeding 50mm thick laid over material refs BC1 or BC3 layer not exceeding 100mm thick; combined thickness not exceeding 150mm.","m2"]
[null,"73","Material refs: WC5; layer not exceeding 50mm thick laid over material refs BC1 or BC3 layer not exceeding 100mm thick laid over material refs:  BA1 or BA3 layer not exceeding 200mm thick; combined thickness not exceeding 350mm.","m2"]
[null,"74","Material ref: WC6; layer not exceeding 50mm thick","m2"]
[null,"75","Material refs: WC6; layer not exceeding 50mm thick laid over material refs BC1 or BC3 layer not exceeding 100mm thick; combined thickness not exceeding 150mm.","m2"]
[null,"76","Material refs: WC6; layer not exceeding 50mm thick laid over material refs BC1 or BC3 layer not exceeding 100mm thick laid over material refs:  BA1 or BA3 layer not exceeding 200mm thick; combined thickness not exceeding 350mm.","m2"]
[null,"77","Material ref: WC8; layer not exceeding 50mm thick","m2"]
[null,"78","Material refs: WC8; layer not exceeding 50mm thick laid over material refs BC1 or BC3 layer not exceeding 100mm thick; combined thickness not exceeding 150mm.","m2"]
[null,"79","Material refs: WC8; layer not exceeding 50mm thick laid over material refs BC1 or BC3 layer not exceeding 100mm thick laid over material refs:  BA1 or BA3 layer not exceeding 200mm thick; combined thickness not exceeding 350mm.","m2"]
["c","","Individual patch area exceeding 15 square metres but not exceeding 20 square metres; in carriageways;",""]
[null,"80","Material ref: WC1 or WC2; layer not exceeding 50mm thick","m2"]
[null,"81","Material refs: WC1 or WC2; layer not exceeding 50mm thick laid over material refs BC1 or BC3 layer not exceeding 100mm thick; combined thickness not exceeding 150mm.","m2"]
[null,"82","Material refs: WC1 or WC2; layer not exceeding 50mm thick laid over material refs BC1 or BC3 layer not exceeding 100mm thick laid over material refs: BA1 or BA3 layer not exceeding 200mm thick; combined thickness not exceeding 350mm.","m2"]
[null,"83","Material ref: WC5; layer not exceeding 50mm thick","m2"]
[null,"84","Material refs: WC5; layer not exceeding 50mm thick laid over material refs BC1 or BC3 layer not exceeding 100mm thick; combined thickness not exceeding 150mm.","m2"]
[null,"85","Material refs: WC5; layer not exceeding 50mm thick laid over material refs BC1 or BC3 layer not exceeding 100mm thick laid over material refs:  BA1 or BA3 layer not exceeding 200mm thick; combined thickness not exceeding 350mm.","m2"]
[null,"86","Material ref: WC6; layer not exceeding 50mm thick","m2"]
[null,"87","Material refs: WC6; layer not exceeding 50mm thick laid over material refs BC1 or BC3 layer not exceeding 100mm thick; combined thickness not exceeding 150mm.","m2"]
[null,"88","Material refs: WC6; layer not exceeding 50mm thick laid over material refs BC1 or BC3 layer not exceeding 100mm thick laid over material refs:  BA1 or BA3 layer not exceeding 200mm thick; combined thickness not exceeding 350mm.","m2"]
[null,"89","Material ref: WC8; layer not exceeding 50mm thick","m2"]
[null,"90","Material refs: WC8; layer not exceeding 50mm thick laid over material refs BC1 or BC3 layer not exceeding 100mm thick; combined thickness not exceeding 150mm.","m2"]
[null,"91","Material refs: WC8; layer not exceeding 50mm thick laid over material refs BC1 or BC3 layer not exceeding 100mm thick laid over material refs:  BA1 or BA3 layer not exceeding 200mm thick; combined thickness not exceeding 350mm.","m2"]
["c","","Patching; Machine lay; exceeding 20 square metres but not exceeding 50 square metres of patching per Task;",""]
["c","","Individual patch area not exceeding 5 square metres; in carriageways;",""]
[null,"92","Material ref: WC1 or WC2; layer not exceeding 50mm thick","m2"]
[null,"93","Material refs: WC1 or WC2; layer not exceeding 50mm thick laid over material refs BC1 or BC3 layer not exceeding 100mm thick; combined thickness not exceeding 150mm.","m2"]
[null,"94","Material refs: WC1 or WC2; layer not exceeding 50mm thick laid over material refs BC1 or BC3 layer not exceeding 100mm thick laid over material refs: BA1 or BA3 layer not exceeding 200mm thick; combined thickness not exceeding 350mm.","m2"]
["c","","Individual patch area exceeding 5 square metres but not exceeding 10 square metres; in carriageways;",""]
[null,"95","Material ref: WC1 or WC2; layer not exceeding 50mm thick","m2"]
[null,"96","Material refs: WC1 or WC2; layer not exceeding 50mm thick laid over material refs BC1 or BC3 layer not exceeding 100mm thick; combined thickness not exceeding 150mm.","m2"]
[null,"97","Material refs: WC1 or WC2; layer not exceeding 50mm thick laid over material refs BC1 or BC3 layer not exceeding 100mm thick laid over material refs: BA1 or BA3 layer not exceeding 200mm thick; combined thickness not exceeding 350mm.","m2"]
["c","","Individual patch area exceeding 10 square metres but not exceeding 15 square metres; in carriageways;",""]
[null,"98","Material ref: WC1 or WC2; layer not exceeding 50mm thick","m2"]
[null,"99","Material refs: WC1 or WC2; layer not exceeding 50mm thick laid over material refs BC1 or BC3 layer not exceeding 100mm thick; combined thickness not exceeding 150mm.","m2"]
[null,"100","Material refs: WC1 or WC2; layer not exceeding 50mm thick laid over material refs BC1 or BC3 layer not exceeding 100mm thick laid over material refs: BA1 or BA3 layer not exceeding 200mm thick; combined thickness not exceeding 350mm.","m2"]
["c","","Individual patch area exceeding 15 square metres but not exceeding 20 square metres; in carriageways;",""]
[null,"101","Material ref: WC1 or WC2; layer not exceeding 50mm thick","m2"]
[null,"102","Material refs: WC1 or WC2; layer not exceeding 50mm thick laid over material refs BC1 or BC3 layer not exceeding 100mm thick; combined thickness not exceeding 150mm.","m2"]
[null,"103","Material refs: WC1 or WC2; layer not exceeding 50mm thick laid over material refs BC1 or BC3 layer not exceeding 100mm thick laid over material refs: BA1 or BA3 layer not exceeding 200mm thick; combined thickness not exceeding 350mm.","m2"]
["c","","Individual patch area exceeding 20 square metres but not exceeding 50 square metres; in carriageways;",""]
[null,"104","Material ref: WC1 or WC2; layer not exceeding 50mm thick","m2"]
[null,"105","Material refs: WC1 or WC2; layer not exceeding 50mm thick laid over material refs BC1 or BC3 layer not exceeding 100mm thick; combined thickness not exceeding 150mm.","m2"]
[null,"106","Material refs: WC1 or WC2; layer not exceeding 50mm thick laid over material refs BC1 or BC3 layer not exceeding 100mm thick laid over material refs: BA1 or BA3 layer not exceeding 200mm thick; combined thickness not exceeding 350mm.","m2"]
["c","","Patching; Machine lay; exceeding 50 square metres of patching per Task;",""]
["c","","Individual patch area not exceeding 5 square metres; in carriageways;",""]
[null,"107","Material ref: WC1 or WC2; layer not exceeding 50mm thick","m2"]
[null,"108","Material refs: WC1 or WC2; layer not exceeding 50mm thick laid over material refs BC1 or BC3 layer not exceeding 100mm thick; combined thickness not exceeding 150mm.","m2"]
[null,"109","Material refs: WC1 or WC2; layer not exceeding 50mm thick laid over material refs BC1 or BC3 layer not exceeding 100mm thick laid over material refs: BA1 or BA3 layer not exceeding 200mm thick; combined thickness not exceeding 350mm.","m2"]
["c","","Individual patch area exceeding 5 square metres but not exceeding 10 square metres; in carriageways;",""]
[null,"110","Material ref: WC1 or WC2; layer not exceeding 50mm thick","m2"]
[null,"111","Material refs: WC1 or WC2; layer not exceeding 50mm thick laid over material refs BC1 or BC3 layer not exceeding 100mm thick; combined thickness not exceeding 150mm.","m2"]
[null,"112","Material refs: WC1 or WC2; layer not exceeding 50mm thick laid over material refs BC1 or BC3 layer not exceeding 100mm thick laid over material refs: BA1 or BA3 layer not exceeding 200mm thick; combined thickness not exceeding 350mm.","m2"]
["c","","Individual patch area exceeding 10 square metres but not exceeding 15 square metres; in carriageways;",""]
[null,"113","Material ref: WC1 or WC2; layer not exceeding 50mm thick","m2"]
[null,"114","Material refs: WC1 or WC2; layer not exceeding 50mm thick laid over material refs BC1 or BC3 layer not exceeding 100mm thick; combined thickness not exceeding 150mm.","m2"]
[null,"115","Material refs: WC1 or WC2; layer not exceeding 50mm thick laid over material refs BC1 or BC3 layer not exceeding 100mm thick laid over material refs: BA1 or BA3 layer not exceeding 200mm thick; combined thickness not exceeding 350mm.","m2"]
["c","","Individual patch area exceeding 15 square metres but not exceeding 20 square metres; in carriageways;",""]
[null,"116","Material ref: WC1 or WC2; layer not exceeding 50mm thick","m2"]
[null,"117","Material refs: WC1 or WC2; layer not exceeding 50mm thick laid over material refs BC1 or BC3 layer not exceeding 100mm thick; combined thickness not exceeding 150mm.","m2"]
[null,"118","Material refs: WC1 or WC2; layer not exceeding 50mm thick laid over material refs BC1 or BC3 layer not exceeding 100mm thick laid over material refs: BA1 or BA3 layer not exceeding 200mm thick; combined thickness not exceeding 350mm.","m2"]
["c","","Individual patch area exceeding 20 square metres but not exceeding 50 square metres; in carriageways;",""]
[null,"119","Material ref: WC1 or WC2; layer not exceeding 50mm thick","m2"]
[null,"120","Material refs: WC1 or WC2; layer not exceeding 50mm thick laid over material refs BC1 or BC3 layer not exceeding 100mm thick; combined thickness not exceeding 150mm.","m2"]
[null,"121","Material refs: WC1 or WC2; layer not exceeding 50mm thick laid over material refs BC1 or BC3 layer not exceeding 100mm thick laid over material refs: BA1 or BA3 layer not exceeding 200mm thick; combined thickness not exceeding 350mm.","m2"]
["c","","Individual patch area exceeding  50 square metres; in carriageways;",""]
[null,"122","Material ref: WC1 or WC2; layer not exceeding 50mm thick","m2"]
[null,"123","Material refs: WC1 or WC2; layer not exceeding 50mm thick laid over material refs BC1 or BC3 layer not exceeding 100mm thick; combined thickness not exceeding 150mm.","m2"]
[null,"124","Material refs: WC1 or WC2; layer not exceeding 50mm thick laid over material refs BC1 or BC3 layer not exceeding 100mm thick laid over material refs: BA1 or BA3 layer not exceeding 200mm thick; combined thickness not exceeding 350mm.","m2"]
[1,"","Series 1100 KERBS, FOOTWAYS AND PAVED AREAS (Scope Paragraph 18.6.1)",""]
["c","","Replacement of Kerbs, Channels, Combined Drainage and Kerb Blocks and Linear Drainage Channel Systems",""]
["c","","Replacement of kerbs; continuous lengths not exceeding 10 metres;",""]
[null,"1","All types 150mm x 305mm.","m"]
[null,"2","All types 125mm x 255mm.","m"]
[null,"3","All types 125mm x 150mm. Replacement of kerbs; continuous lengths exceeding 10 metres;","m"]
[null,"4","All types 150mm x 305mm.","m"]
[null,"5","All types 125mm x 255mm.","m"]
[null,"6","All types 125mm x 150mm.","m"]
["c","","Replacement of channels; continuous lengths not exceeding 10 metres;",""]
[null,"7","All types 255 x 125mm.","m"]
[null,"8","All types 150 x 125mm.","m"]
["c","","Replacement of channels; continuous lengths exceeding 10 metres;",""]
[null,"9","All types 255 x 125mm.","m"]
[null,"10","All types 150 x 125mm.","m"]
["c","","Replacement of combined drainage and kerb blocks; continuous lengths not exceeding 10 metres;",""]
[null,"11","Kerb type HB2 with 277mm x 205mm/295mm base unit.","m"]
[null,"12","Access unit HB2 with 277mm x 205mm/295mm base unit.","m"]
[null,"13","ACO KerbDrain units depths not exceeding 305mm depth.","m"]
[null,"14","ACO KerbDrain units depths exceeding 305mm but exceeding 480mm depth.","m"]
["c","","Replacement of combined drainage and kerb blocks; continuous lengths exceeding 10 metres;",""]
[null,"15","Kerb type HB2 with 277mm x 205mm/295mm base unit.","m"]
[null,"16","Access unit HB2 with 277mm x 205mm/295mm base unit.","m"]
[null,"17","ACO KerbDrain units depths not exceeding 305mm depth.","m"]
[null,"18","ACO KerbDrain units depths exceeding 305mm but exceeding 480mm depth.","m"]
["c","","Replacement of linear drainage channel systems; continuous lengths not exceeding 10 metres;",""]
[null,"19","Channel section 100mm wide with slotted class D400 cast iron grating.","m"]
["c","","Replacement of linear drainage channel systems; continuous lengths exceeding 10 metres;",""]
[null,"20","Channel section 100mm wide with slotted class D400 cast iron grating.","m"]
[]
[]
[null,null,"Note: Above rates are based on Mon to Fri 0700-1900hrs"]
[]
[null,null,"Out of Hours Uplift for Night Working (Mon to Fri 1900-0700hrs)","%"]
[null,null,"Out of Hours Uplift for Weekend Working (0700hrs on Sat to 0700 on Mon)","%"]