**Map A- Location of Works**A map of a city

Description automatically generated

**Table 2 – Table of Works**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Ref** | **Work** | **Access** | **Preparation** | **Notes** | **ditch width** | **ditch depth** |
| B01 | Bund | easy |  | Partially built. Needs reinstalling | 4 | 2 |
| B02 | Bund | hard | remove trees and fence |  | 3.5 | 1.5 |
| B03 | Bund | hard | remove trees and fence |  | 5 | 1.5 |
| B04 | Bund | easy |  |  | 3 | 1.25 |
| B05 | Bund | easy | remove fence |  | 4 | 1 |
| B06 | Bund | easy | remove fence |  | 6 | 1 |
| B07 | Bund | easy |  | Near pond | 6 | 1 |
| B08 | Bund | easy |  | Possible foot drain needs blocking | 6 | 0.75 |
| B09 | Bund | easy |  |  | 3 | 3 |
| B10 | Bund | easy |  |  | 4 | 2.5 |
| B12 | Bund | hard | remove trees and fence | Access from outside fen challenging terrain | 6 | 3 |
| B13 | Bund | medium | remove trees and fence | Access issues within woodland | 5 | 1.5 |
| B14 | Bund | medium | remove trees | Existing bund needs proper install | 3 | 1.5 |
| B15 | Bund | easy | remove trees |  | 3 | 1 |
| B16 | Bund | easy |  |  | 3 | 1 |
| B17 | Bund | easy |  |  | 7 | 3 |
| B18 | Bund | easy |  |  | 4 | 1 |
| B19 | Bund | easy |  |  | 6 | 2.5 |
| B20 | Bund | easy |  |  | 7 | 2.5 |
| B21 | Bund | medium |  |  | 6 | 2 |
| B22 | Bund | easy |  |  | 3 | 1 |
| B23 | Bund | easy |  |  | 4 | 0.5 |
| B24 | Bund | easy |  |  | 3 | 1.5 |
| B25 | Bund | easy | remove trees |  | 4 | 2 |
| B26 | Bund | medium | remove trees and fence | Pick route through the trees | 4 | 1.5 |
| B27 | Bund | medium | remove trees | Access? | 6 | 1.5 |
| B28 | Bund | medium | remove trees | Bund near deer seat | 6 | 1.5 |
| B29 | Bund | easy |  | Collar or sluice | 6 | 3 |
| B30 | Bund | easy |  |  | 4 | 2 |
|  |  |  |  |  |  |  |
| CD01 | Bund and profile | easy |  | Catch dyke- pull in soil | 3 | 1.75 |
| CD02 | Bund and profile | easy |  | Catch dyke- pull in soil | 3 | 1.5 |
| CD03 | Bund and profile | easy |  | Catch dyke- pull in soil | 4 | 1.75 |
| CD04 | Bund and profile | medium | remove trees | Catch dyke- pull in soil | 4 | 1.25 |
| CD05 | Bund and profile | easy | remove trees | Catch dyke- pull in soil | 3 | 1.5 |
| CD06 | Bund and profile | medium |  | Catch dyke- pull in soil | 4 | 1.5 |
| CD07 | Bund and profile | medium | remove trees | Catch dyke- pull in soil | 4 | 2 |
| CD08 | Bund and profile | medium | remove trees | Catch dyke- pull in soil | 4 | 1.5 |
| CD09 | Bund and profile | medium | remove trees | Catch dyke- pull in soil | 6 | 2 |
| CD10 | Bund and profile | medium | remove trees | Catch dyke- pull in soil | 6 | 2 |
| CD12 | Bund and profile | medium | remove trees | Catch dyke- pull in soil | 4 | 1 |
| CD13 | Bund and profile | easy | remove trees and fence | Catch dyke- pull in soil | 4 | 1 |
| CD14 | Bund and profile | easy | remove trees | Catch dyke- pull in soil | 3 | 1 |
|  |  |  |  |  |  |  |
| NC1 | Create Culvert | easy | remove trees | Create culvert under track | 10 | 1.5 |

**Diagram 1- Proposed design of bunds**

A diagram of a water flow

Description automatically generated with medium confidence