**PRICING SCHEDULE – RIVERBANK REPAIRS AT MILL AND MARSH MEADOWS**

**CONTRACTOR: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

|  |  |  |  |
| --- | --- | --- | --- |
| **ITEM** | **WORKS** | **UNIT** | **PRICE** |
| **Marsh Meadows** |  |  |
| 1 | Supply and install 10.8 m section of new steel piling in front of the existing piling to the same level as the adjacent piling, and the land behind levelled to suit the adjacent land. |  |  |
| 2 | Supply and install 7.8 m section of new steel piling as above. |  |  |
| 3 | Supply and install 4.1 m section of new steel piling as above. |  |  |
| 4 | Supply and install 2.2 m section of new steel piling as above. |  |  |
| 5 | Supply and install 1200 mm long single course of concrete sandbags. |  |  |
| **Mill Meadows** |  |  |
| 6A | **Option A** – Supply and install a new river wall in 25 m sections in galvanized sheet steel piling, with hardwood timber capping and waling. |  |  |
| 6B | **Option B** – Supply and install a new river wall in 25 m sections in concrete and block construction. |  |  |
| 7 | Repair of the 8 m section of river wall under the River and Rowing Museum jetty. |  |  |
| 8 | Supply and install a ladder for exit from the river close to the River and Rowing Museum landing stage.  |  |  |

**Additional notes:**

Price are to be submitted in GBP and exclusive of VAT.

Any additional proposed items should be included separately within the schedule. No additional costs will be considered by the Council unless these are clearly stated in the pricing schedule response.