Appendix 4

Broadway Play Area

Fencing specification:

Supply and erect 1.2 m high galvanised and powder coated bow top play safe fencing.

Use 30x 10 top and bottom rails with 12mm round bar set at 95mm centres.

Panels fixed to 50 x 50 x 3mm posts set in concrete at 2.75 m centres.

1 of 1.2m playsafe single gate.