Version: 20/11/2023 14:34

| **Q no.** | **Received**  **(date)** | **From**  **(supplier name)** | **Allocated to**  **(initials)** | **Question** | **Response** | **Response Issued**  **(date)** | **To all tenderers**  **(Y/N)** |
| --- | --- | --- | --- | --- | --- | --- | --- |
| 1 | 14/11/2023 |  | MP | Please can you confirm the fencing style, 358 mesh is included in drawings but not in the fence design | Some drawings incorrectly include 358 mesh.  Please note: All fences/gates should be of the same v-mesh make up as per the following drawings throughout:  3362-116 T2 (Fence Detail – TYPE A) 231023  3362-117 T3 (Fence Detail – TYPE B) 231030  If gates require a slightly different mesh (i.e., double mesh) please note this in the tender return. | 20/11/  23 | Y |
| 2 | 14/11/2023 |  | MP | Who provides maglocks and gate closers | G4S to supply Maglock – Contractor/gate supplier to install.  Door closers to be provided by the Contractor | 20/11/  23 | Y |
| 3 | 14/11/2023 |  | MP | Can soil/waste be left on site | No, all waste to be removed from site | 20/11/  23 | Y |
| 4 | 15/11/2023 |  | MP | Please confirm electrical requirements | The electrical supply to each gate requires 2x 63mm twin-wall duct:   1. Electrical high power – all electrical cables are to be supplied and installed by the contractor. 2. Chubb & G4S to install data cables – ducts and draw wires to be supplied by contractor (2 nr draw wires).   Allowance for G4S and Chubb data cabling to be made and included within programme | 20/11/  23 | Y |
| 5 | 14/11/2023 |  | MP | Is the data cable on the Nursery fencing to remain? | Yes, this will need to be removed, temporarily hosted and reattached post completion | 20/11/  23 | Y |
| 6 | 14/11/2023 |  | MP | Are tree stumps to remain | Tree stumps require removing as part of the new road instating. | 20/11/  23 | Y |
| 7 | 15/11/2023 |  | MP | Also are we able to offer similar alternatives to Jackson fencing. | Substitute products  1.Details: If products of different manufacture to those specified are proposed, submit details with the tender giving reasons for each proposed substitution. Substitutions, which have not been notified at tender stage, may not be considered.  2. Compliance: Substitutions accepted will be subject to the verification requirements of clauseA31/200 | 20/11/  23 | Y |
| 8 | 16/11/2023 |  | MP | Removed path does this include removing soil and re-grassing. | Removal of soils are to be included by the contractor.  Grass to be tended for seeding. | 20/11/23 | Y |
| 9 | 16/11/2023 |  | MP | Entry Post to Area A does this require bollard, Location 3? | Yes, bollards to be included for:  Location 3 bollard adjacent to external access post to prevent vehicle collision.  Location 8 bollard to be included to prevent car access and ensure public footpath remains unimpeded. | 20/11/  23 | Y |
| 10 | 16/11/2023 |  | MP | Electrical surface mounting requirement | All surface mounted electrics should be encased within trunking to be specified by contractor. This must include G4S and Chubb cables being surface mounted to ensure all are managed and consistent. | 20/11/  23 | Y |
| 11 | 16/11/2023 |  | MP | How do I present my Nursery rabbit proofing fence design without affecting my tender price. | Please tender for the specified drawings. i.e. v mesh and gravel border  Please then also include a row under Pricing List 4.7 “Other: Contractor to add as appropriate” Please make it evident this is an additional line and should not be calculated alongside the gravel/v mesh design if required.  The product should be specified within the tender return documents. Should this remove/reduce the requirement for gravel / v-mesh fencing please list the savings within a separate line.  Additionally, please ensure any programme change is reflected within the proposed programme | 20/11/  23 | Y |
| 12 | 16/11/2023 |  | GM | Will you provide an advanced deposit | Advanced deposits (payments) are not provided for. Payment for the delivery of materials on site can be agreed. | 20/11/  23 | Y |
|  |  |  |  |  |  |  |  |