4.4.1.1 TRAFFIC SIGNS

* Clean all traffic sign faces and reference numbers areas less than 5m2

|  |  |
| --- | --- |
|  | Clean signs in accordance with CM 125 [Ref 21.N] and manufacturers' instructions.Rectify defects in accordance with CM 125 [Ref 21.N] and CS 126 [Ref 14.N].Provide traffic signs cyclic and repair maintenance activity data in accordance with the requirements of the ADMM [Ref 1.N].(GM 701 – PG83) |

# maintenance requirements

* Traffic signs – Clean all traffic sign faces and reference numbers every 2 years – rectify defects as instructed.

(GM 701 – PG83)

# UNIT / MEASUREMENT / ITEMISATION

* The units of measurement shall be:
1. Clean all traffic sign faces and reference numbers, marker post faces and reference numbers and clean all illuminated and non-illuminated (retroflective) bollards…...number.
2. Clean all traffic sign faces and reference numbers of all Gantry signs…... number.
* The measurement of clean all traffic sign faces and reference numbers shall be each sign.
* The measurement of clean all marker post faces and reference numbers shall be each marker post.
* The measurement of clean all traffic sign faces and reference numbers of all Gantry signs shall be each gantry.
* Separate items shall be provided for cleaning of traffic signs, post faces and bollards in accordance with Chapter II paragraphs 3 and 4 and the following:

Group Feature

I 1 Sub-Asset Type.

II 1 Item.

(MOM Schd. B Issue 7 PG18/19)

# additional information

* Traffic signs shall be maintained by cleaning the entire sign face and reference numbers, in accordance with CS125, and using methods recommended by the sign face manufacturer which do not damage the face.
* Cleaning shall not be carried out when the ambient temperature is 2°C or less and falling or when the Operations are likely to result in the formation of ice on the footway or carriageway.
* Cleaning operations to be undertaken in accordance with the Working at Height Regulations 2015, and all relevant Health and Safety regulations. Ladders shall not be leant against sign faces.
* The *Contractor* shall maintain a daily record sheet during cleaning operations giving sign locations, and submit to the *Service Manager*.
* Any damage or Defects to traffic signs shall be repaired or made safe immediately if considered a danger to the public following an instruction from the *Service Manager*.

 (M&RC-SPEC PG24)