**West Bergholt MUGA/tennis court core results December 2020**

The **core:**

 Extracted from the middle of the MUGA using a tracked drilling rig by Cowan Drilling Services on 3rd December.

The core revealed from a visual inspection on site:

 50mm surfacing/base layer of up to10mm open textured asphalt overlying

 170mm sub-base of graded unbound crushed rock with minimal fines content overlying

 Soft to firm light brown silty clay

The **implications** to consider are:

 Reducing the the centres of the drainage holes and/or their size having regard to the limited depth of construction so as to minimise the disturbance of such.

 A need to ensure continuing attention is paid to all trees in the vicinity to minimise the impact of potential subsidence on the site

**Brian Butcher**