****

**IMPERIAL WAR MUSEUM- CHURCHILL WAR ROOMS SHOP**

**TENDER WORKS PRICING SCHEDULE**

|  |  |
| --- | --- |
| ***Component*****Strip out Rooms 66a, 67, 68 and South wall room 66** | ***Refer to Drawing No :*****273/001.0****273/002.0****273/003.0****273/004.0****273/101.0****273/102.0** |
| ***Specification/ Description:***Removal of existing shop fitting items and fixtures. Refer to notes and drawings for scope and spec.Inspect site Please note this is a listed building and a number of fittings and ducts are existing historic to remain. Fiber board wall paneling is historic and to remain.After strip out allow for meeting with Listed Building officials on site prior to undertaking works.  |
| ***Item*** | ***Quantity*** | ***Price (£)*** |
| Perimeter shop fitting items front of house | See site |  |
| Cash desk and freestanding/mid floor items front of house | 1x See site |  |
| Existing flooring to rooms 66a, 67, 68 | 1x See site |  |
| Wall graphics and signs if applicable | See site |  |
| Contemporary Lighting and cabling | 1x see site |  |
| Contemporary power and lighting if not required for new | See site |  |
| If possible infil over archway connecting rooms 67 and 68 | See site |  |
|  |  |  |
|  |  |  |
|  | **TOTAL** |  |

|  |  |
| --- | --- |
| ***Component*****Preparation, Decorations & Flooring** | ***Refer to Drawing:*****273/001.0****273/002.0****273/003.0****273/004.0****273/101.0****273/102.0** |
| ***Specification/ Description:***Refer to drawings |
| ***Item*** | ***Quantity*** | ***Price (£)*** |
| Prepare floor in rooms 66a, 67 & 68 suitable for new sheet vinyl floor finish | Refer to drawings |  |
| Supply and fit new sheet vinyl flooring proposed Marmoleum | Refer to drawings |  |
| Rub down, make good and prepare for decorating to all walls, skirtings, doors, frames and columns in retail areas 66a, 67, 68 and south wall 66 | Refer to drawings |  |
| Clean and prepare and decorate ceiling and ceiling beams in rooms 66a, 67, 68 as spec | Refer to drawings |  |
| Decoration of existing ducts and pipework [if already decorated] | Refer to site |  |
| Allow for glass mirror to be bonded or mechanically fixed to arch way wall.  | 1x Refer to layout |  |
|  |  |  |
|  | **TOTAL** |  |
|  |  |  |
| ***Component/Interactive*****Small Power & Heating** | ***Refer to Drawing No :*****273/001.0****273/002.0****273/003.0****273/004.0****273/101.0****273/102.0****273/210.0****273/212.0****273/215.0****273/217.0****273/218.1****273/407.0** |
| ***Specification/ Description:***Supply and install cables/sockets/ and conduit in accordance with the layouts and requirement and working with the existing provision.Develop a proposal for the supply and fit of an electric radiator system as performance spec on drawings. |
| ***Item*** | ***Quantity*** | ***Price (£)*** |
| Power and data as layout including to 2x cash desks | Refer to drawings |  |
| Power for new lighting | Refer to drawings |  |
| Electric radiator heating system | Refer to drawings |  |
| Switching for lighting system | Refer to drawings |  |
| Allow for power and lighting to display case  | X2 |  |
| Allow for LED lighting to underside of shelf to cash desk | X1 |  |
| Allow for power and installation of free issue equipment to DVD unit | 1x |  |
| Allow for power and installation of free issue equipment to print on demand unit [POD] | 1x |  |
| Allow for power and installation of ipad to 1x cash desk | 1x |  |
|  | **TOTAL** |  |

|  |  |
| --- | --- |
| ***Component*****Lighting** | ***Refer to Drawing No :*****273/002.0****273/004.0****273/101.0****273/102.0** |
| ***Specification/ Description:***Supply and install new lighting as specification. Note there may be some long lead items to take into account. |
| ***Item*** | ***Quantity*** | ***Price (£)*** |
| Supply and install Track | Refer to drawings |  |
| Supply and install spot Lights | Refer to drawings |  |
| Supply and install wall lights | Refer to drawings |  |
| Supply and install pendant light fittings  | Refer to drawings |  |
| Allow for final focus of lighting once store is merchandised | Refer to drawings |  |
| Lighting to 2x display cases noted in small power above. | - |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  | **TOTAL** |  |

|  |  |
| --- | --- |
| ***Component*****Supply and fit graphic decals to walls** | ***Refer to Drawing No :*****273/002.0****273/101.0****273/102.0** |
| ***Specification/ Description:***Retail area walls |
| ***Item*** | ***Quantity*** | ***Price (£)*** |
| Application direct to prepared wall of decal graphic artwork to be supplied. Quotes similar to IWM London. Allow PC sum | X5 |  |
|  |  |  |
|  |  |  |
|  | **TOTAL** |  |

|  |  |
| --- | --- |
| ***Component*****Wall Panels** | ***Refer to Drawing No :*****273/002.0****273/101.0****273/102.0****273/201.0****273/202.0****273/203.0** |
| ***Specification/ Description:***Refer to drawings for locations and site to confirm configuration. Wall panels comprise mdf back panel with ply end sections and steel protection strip to base. Front face in dark oak veneer. Panels with Peerless system [or similar approved] slotted upright merchandising system. Panels with Picture hanging rail system. Panels fitted to walls using split batten system and in accordance with fixing details and advise and approval from listed building. Refer to fixing method statement and ensure allowance for fixing in accordance with listed building requirements. Finish to meet min Class 1 |
| ***Item*** | ***Quantity*** | ***Price (£)*** |
| Typical slotted upright wall bays | Refer to drawings |  |
| Typical half bay slotted upright wall bays | Refer to drawings |  |
|  |  |  |
|  |  |  |
|  | **TOTAL** |  |

|  |  |
| --- | --- |
| ***Component*****Perimeter low storage unit** | ***Refer to Drawing No :*****273/002.0****273/101.0****273/102.0****273/204.0** |
| ***Specification/ Description:***Allow for units constructed of solid oak frame with solid core laminated mdf body and hinged cupboard doors and finger pull detail to top edge. Finish to meet min Class 1 |
| ***Item*** | ***Quantity*** | ***Price (£)*** |
| Low level storage unit 980mm width | 2x |  |
|  |  |  |
|  |  |  |
|  | **TOTAL** |  |

|  |  |
| --- | --- |
| ***Component*****Perimeter Shelves** | ***Refer to Drawing No :*****273/002.0****273/101.0****273/102.0****273/205.0** |
| ***Specification/ Description:***Supply of shelves complete with metal supports and brackets by Peerless [or similar other approved] Metal finish BZP steel.Shelves of solid oak frame with laminated top. Finish to meet min Class 1*Please provide unit price.* |
| ***Item*** | ***Quantity*** | ***Price (£)*** |
| Shelves 900mm width | Provide unit price  |  |
| Shelves 450mm width | Provide unit price |  |
|  |  |  |
|  |  |  |
|  | **TOTAL** |  |

|  |  |
| --- | --- |
| ***Component*****Perimeter Shelves with Hanging Rails** | ***Refer to Drawing No :*****273/002.0****273/101.0****273/102.0****273/206.0** |
| ***Specification/ Description:***Supply shelves with under shelf hanging rails. Shelves as above. Metal support brackets by Peerless [or similar other approved]Rails in BZP steel finish. Finish to meet min Class 1*Please provide unit price.* |
| ***Item*** | ***Quantity*** | ***Price (£)*** |
| Rail type A  | Provide unit price |  |
| Rail type B | Provide unit price |  |
| Rail type C [half bay] | Provide unit price |  |
|  |  |  |
|  |  |  |
|  | **TOTAL** |  |

|  |  |
| --- | --- |
| ***Component*****Perimeter Timber Rail** | ***Refer to Drawing No :*****273/002.0****273/101.0****273/102.0****273/207.0** |
| ***Specification/ Description:***Supply solid oak hanging rail with metal bracket and metal hanger stop bar as detailed. Metal support brackets by Peerless [or similar other approved] BZP steel finishFinish to meet min Class 1*Please provide unit price.* |
| ***Item*** | ***Quantity*** | ***Price (£)*** |
| Rail type A | Provide unit price |  |
| Rail type B [half bay forward rail] | Provide unit price |  |
|  |  |  |
|  |  |  |
|  | **TOTAL** |  |

|  |  |
| --- | --- |
| ***Component*****Perimeter peg board panels** | ***Refer to Drawing No :*****273/002.0****273/101.0****273/102.0****273/208.0** |
| ***Specification/ Description:***Supply bespoke peg board panels with suitable bracket metal work for use with perimeter bay arrangement. Peg boards of 6mm ply with dark oak veneer front. Peg holes as indicated. Each board with brackets for hanging on to shopfitting slotted upright. Metal support brackets by Peerless [or similar other approved] BZP steel finishSupply suitable euro hooks to suit peg board.Finish to meet min Class 1*Please provide unit price.* |
| ***Item*** | ***Quantity*** | ***Price (£)*** |
| Peg board 450mm x 700mm | Provide unit price |  |
| Euro hooks to suit above panel | Provide pack or unit price |  |
|  |  |  |
|  |  |  |
|  | **TOTAL** |  |

|  |  |
| --- | --- |
| ***Component*****Perimeter book shelves** | ***Refer to Drawing No :*****273/002.0****273/101.0****273/102.0****273/209.0** |
| ***Specification/ Description:***Supply angled book shelves as details. Note 2x types for use on perimeter bay system. Shelves of solid oak frame, laminate faces and with suitable metal bracket system to fit into uprights of perimeter bay system. Metal support brackets by Peerless [or similar other approved] BZP steel finishFinish to meet min Class 1*Please provide unit price.* |
| ***Item*** | ***Quantity*** | ***Price (£)*** |
| Shelf type A | Provide unit price |  |
| Shelf type B | Provide unit price |  |
|  |  |  |
|  |  |  |
|  | **TOTAL** |  |

|  |  |
| --- | --- |
| ***Component*****Perimeter DVD Shelves** | ***Refer to Drawing No :*****273/002.0****273/101.0****273/102.0****273/210.0****273/210.1** |
| ***Specification/ Description:***DVD shelf unit of mdf panel with solid core laminate to all faces. Powder coated steel shelves fixed to panel set out as shown. Panel with metal support brackets by Peerless [or similar other approved] BZP steel finishTV unit of mdf panel with solid core laminate to all faces as above. Powder coated steel dvd display shelf. TV panel to sit above DVD shelf panels fitted to slotted uprights of bay system. Metal support brackets by Peerless [or similar other approved] BZP steel finish TV/DVD player to be supplied by IWM. Provide cable holes and cable management.Finish to meet min Class 1 |
| ***Item*** | ***Quantity*** | ***Price (£)*** |
| DVD shelf unit | 2x |  |
| TV unit | 1x |  |
|  |  |  |
|  |  |  |
|  | **TOTAL** |  |

|  |  |
| --- | --- |
| ***Component*****Perimeter poster unit** | ***Refer to Drawing No :*****273/002.0****273/101.0****273/102.0****273/211.0** |
| ***Specification/ Description:***Unit constructed of solid oak frame with inset in top with clear acrylic cover. Unit notched at regular intervals to take clear acrylic dividers. Base with recess to sit posters into. Unit to freestand in front of wall panel.Finish to meet min Class 1*Please provide unit price.* |
| ***Item*** | ***Quantity*** | ***Price (£)*** |
| Perimeter poster unit | 3x |  |
| Acrylic dividers  | 15x |  |
|  |  |  |
|  |  |  |
|  | **TOTAL** |  |

|  |  |
| --- | --- |
| ***Component*****Perimeter poster/print unit back wall** | ***Refer to Drawing No :*****273/002.0****273/101.0****273/102.0****273/203.0****273/212.0** |
| ***Specification/ Description:***Perimeter wall panel constructed to match look and feel of typical wall panel drawing 273/201. Wall to have peg board with slotted upright as shown. Unit with mdf back panel, ply end sections and dark oak veneer to front. Central sections to be peg board. Allow for picture hanging system and steel protection to bottom edge. Fixed on split batten system and in accordance with fixing method statement.Refer to drawing for detail and spec.Finish to meet min Class 1 |
| ***Item*** | ***Quantity*** | ***Price (£)*** |
| Perimeter poster/print unit back wall  | Refer to drawings |  |
|  |  |  |
|  |  |  |
|  | **TOTAL** |  |

|  |  |
| --- | --- |
| ***Component/Interactive*****Perimeter Print Shelves** | ***Refer to Drawing No :*****273/002.0****273/101.0****273/102.0****273/203.0****273/213.0** |
| ***Specification/ Description:***Print bays made in 2x sizes to fit room 66a. Bays constructed similar to poster bays but with bespoke sizes as shown. Unit with mdf back panel, ply end sections and dark oak veneer to front. Central sections to be peg board. Allow for picture hanging system and steel protection to bottom edge.Folded steel shelves with brackets to fit slotted upright system. Fixed on split batten system and in accordance with fixing method statement.Shelves with clear acrylic front strip. Metalwork by Peerless [or similar other approved] powder coated finish.Finish to meet min Class 1*Please provide unit price for print shelves* |
| ***Item*** | ***Quantity*** | ***Price (£)*** |
| Print bay 770mm  | 2x |  |
| Print bay 1000mm | 5x |  |
| Print shelves 770mm | 8x |  |
| Print shelves 1000mm  | 20x |  |
|  |  |  |
|  |  |  |
|  | **TOTAL** |  |

|  |  |
| --- | --- |
| ***Component/Interactive*****Freestanding Display Items** | ***Refer to Drawing No :*****273/214.0** |
| ***Specification/ Description:***Supply freestanding clip board constructed of solid oak with preparatory clip.Supply freestanding oak display plinth in 2x sizes.Refer to drawing for spec and sizesFinish to meet min Class 1*Please provide unit price*  |
| ***Item*** | ***Quantity*** | ***Price (£)*** |
| Clip board | Provide unit price |  |
| Display box type A | Provide unit price |  |
| Display box type B | Provide unit price |  |
|  |  |  |
|  |  |  |
|  | **TOTAL** |  |

|  |  |
| --- | --- |
| ***Component*****Print on demand** | ***Refer to Drawing No :*****273/002.0****273/101.0****273/102.0****273/203.0****273/215.0** |
| ***Specification/ Description:***Print on demand unit to fit onto wall bay system. Unit of 18mm mdf with solid core laminate to front face and edges. Unit has removable front for access to cables and power source. Face mounted screen free issue from IWM to be fitted by contractor. .Provide cable holes and cable management.Finish to meet min Class 1 |
| ***Item*** | ***Quantity*** | ***Price (£)*** |
| Print on demand unit  | 1x |  |
|  |  |  |
|  |  |  |
|  | **TOTAL** |  |

|  |  |
| --- | --- |
| ***Component*****Freestanding display box** | ***Refer to Drawing No :*****273/216.0** |
| ***Specification/ Description:***Freestanding display box with clear polished glass top cube UV bonded. Glass fits into groove in base. Removable display pad with fabric cover as spec on drawing.Finish to meet min Class 1*Please provide unit price* |
| ***Item*** | ***Quantity*** | ***Price (£)*** |
| Freestanding display box | Provide unit price |  |
|  |  |  |
|  |  |  |
|  | **TOTAL** |  |

|  |  |
| --- | --- |
| ***Component*****Room 68 Perimeter ‘window’ display** | ***Refer to Drawing No :*****273/002.0****273/101.0****273/102.0****273/203.0****273/217.0** |
| ***Specification/ Description:***Supply and fit display unit with glazed door. Unit with top and bottom infils decorated as spec. Unit carcase finished with solid core laminate to front and sides. Internally provide toughened glass shelves on library strip. Internally side cheeks finished in laminate. Lockable door with framing to look like sash window decorated to ral colour. Provide LED strip lighting to top and sides. Provide cable management within unit and neat cable run to unit. Fixings in accordance with fixing method statement.Finish to meet min Class 1 |
| ***Item*** | ***Quantity*** | ***Price (£)*** |
| ‘Window’ display unit complete with shelves and lighting | 1x |  |
|  |  |  |
|  |  |  |
|  | **TOTAL** |  |

|  |  |
| --- | --- |
| ***Component*****Room 68 Curved wall base unit** | ***Refer to Drawing No :*****273/002.0****273/101.0****273/102.0****273/218.0****273/218.1** |
| ***Specification/ Description:***Unit constructed to fit site conditions and faceted wall panels it sits against. Front edge is curved to reflect original curve of room. Allow for units constructed of solid oak frame with solid core laminated mdf body and hinged cupboard doors and finger pull detail to top edge. Unit to be made in sections and contractor to advise.Note one unit adapted to take radiator.Finish to meet min Class 1 |
| ***Item*** | ***Quantity*** | ***Price (£)*** |
| Room 68 curved wall base unit | 1x |  |
|  |  |  |
|  |  |  |
|  | **TOTAL** |  |

|  |  |
| --- | --- |
| ***Component*****Room 68 Pegboard Display wall** | ***Refer to Drawing No :*****273/002.0****273/101.0****273/102.0****273/203.0****273/219.0** |
| ***Specification/ Description:***Perimeter wall panel constructed to match look and feel of typical wall panel drawing 273/201. Wall to have peg board with slotted upright as shown. Unit with mdf back panel, ply end sections and dark oak veneer to front. Central sections to be peg board. Allow for picture hanging system and steel protection to bottom edge. Fixed on split batten system and in accordance with fixing method statement.Refer to drawing for detail and spec.Finish to meet min Class 1 |
| ***Item*** | ***Quantity*** | ***Price (£)*** |
| Room 68 peg board wall | 1x |  |
|  |  |  |
|  |  |  |
|  | **TOTAL** |  |

|  |  |
| --- | --- |
| ***Component*****Perimeter Low storage unit 1500mm** | ***Refer to Drawing No :*****273/002.0****273/101.0****273/102.0****273/220.0** |
| ***Specification/ Description:***Allow for units constructed of solid oak frame with solid core laminated mdf body and hinged cupboard doors and finger pull detail to top edge. Finish to meet min Class 1 |
| ***Item*** | ***Quantity*** | ***Price (£)*** |
| Perimeter Low storage unit 1500mm | 1x |  |
|  |  |  |
|  |  |  |
|  | **TOTAL** |  |
| ***Component*****Room 67 Cash desk** | ***Refer to Drawing No :*****273/002.0****273/101.0****273/102.0****273/CRW\_301.0****273/CRW\_301.1****273/CRW\_301.2** |
| ***Specification/ Description:***Cash desk unit comprised of side counter area of solid oak frame and oak veneer top. Solid oak frame and oak veneer swing side section for access. Raised area in solid core laminate with solid oak frame. Under counter with cupboards and shelves and pull out tissue shelf. Allow for cable management and cable access ways throughout unit. IWM to supply all till equipment and contractor to fit. IWM to supply free issue ipad in bouncepad and contractor to fit. Refer to details.Finish to meet min Class 1 |
| ***Item*** | ***Quantity*** | ***Price (£)*** |
| Room 67 cash desk  | 1x |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  | **TOTAL** |  |

|  |  |
| --- | --- |
| ***Component*****Room 68 Cash desk** | ***Refer to Drawing No :*****273/002.0****273/101.0****273/102.0****273/CRW\_302.0****273/CRW\_302.1****273/CRW\_302.2** |
| ***Specification/ Description:***Cash desk unit comprised of solid oak frame and oak veneer top. Customer side shelf with ‘dump bin’ detail. Customer side peg board under with LED lighting. Under counter with cupboards and shelves and pull out tissue shelf. Allow for cable management and cable access ways throughout unit. IWM to supply all till equipment and contractor to fit. IWM to supply free issue ipad in bouncepad and contractor to fit. Refer to details.Allow for wall mounted magnetic panel as shown in elevations.Finish to meet min Class 1 |
| ***Item*** | ***Quantity*** | ***Price (£)*** |
| Room 68 cash desk  | 1x |  |
| Room 68 magnetic wall panel near to cash desk | 1x |  |
|  |  |  |
|  |  |  |
|  | **TOTAL** |  |

|  |  |
| --- | --- |
| ***Component*****Room 67 Basic Display Table** | ***Refer to Drawing No :*****273/002.0****273/101.0****273/102.0****273/401.0****273/401.1****273/402.0** |
| ***Specification/ Description:***Table comprises two parts upper and lower both mobile on lockable castors. Upper of solid oak frame with solid core laminate top on 18mm ply. Ends with solid core laminate faced peg board.Low display unit fits under upper table. This of solid oak frame with laminate top front, back and sides.Finish to meet min Class 1 |
| ***Item*** | ***Quantity*** | ***Price (£)*** |
| Room 67 Basic Table with 1 low nest table and peg board ends | 3x |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  | **TOTAL** |  |

|  |  |
| --- | --- |
| ***Component*****Room 68 Basic Display Table** | ***Refer to Drawing No :*****273/002.0****273/101.0****273/102.0****273/403.0****273/403.1****273/404.0** |
| ***Specification/ Description:***Table comprises two parts upper and lower both mobile on lockable castors. Upper of solid oak frame with solid core laminate top on 18mm ply. Ends with solid core laminate faced peg board.Low display unit fits under upper table. This of solid oak frame with laminate top front, back and sides.Finish to meet min Class 1 |
| ***Item*** | ***Quantity*** | ***Price (£)*** |
| Room 68 Basic Table with 2 low nest tables and peg board ends | 2x |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  | **TOTAL** |  |

|  |  |
| --- | --- |
| ***Component*****Table top angled book display** | ***Refer to Drawing No :******273/405.0*** |
| ***Specification/ Description:***Freestanding unit with solid oak end supports and angled ply book stand. This with laminate finish to faces as shown.Finish to meet min Class 1*Please provide unit price* |
| ***Item*** | ***Quantity*** | ***Price (£)*** |
| Room 68 Basic Table with 2 low nest tables and peg board ends | Provide unit price |  |
|  |  |  |
|  | **TOTAL** |  |
|  |  |  |
| ***Component*****Postcard Unit** | ***Refer to Drawing No :******273/406.0*** |
| ***Specification/ Description:***Freestanding mobile unit with lockable castors. Solid oak frame with mdf side and back panels with laminate finish. Note shelves shown are to match those now implemented in IWM London where this unit can be viewed to match. Shelves to be folded powder coated steel with 50mm clear acrylic up-stand to front edge. Shelves adjustable on Peerless ferrules [or similar to approval] Sign card holder. Sign card by IWM. |
| ***Item*** | ***Quantity*** | ***Price (£)*** |
| Postcard unit | 1x |  |
|  |  |  |
|  |  |  |
|  | **TOTAL** |  |

|  |  |
| --- | --- |
| ***Component*****Room 67 Freestanding Display Case** | ***Refer to Drawing No :*****273/002.0****273/101.0****273/102.0****273/203.0****273/407.0** |
| ***Specification/ Description:***Freestanding display case with discreet anchor to wall behind it. Fix in accordance with fixing method statement. Unit constructed of solid dark oak frame with dark oak veneer sides top and base. Lockable clear toughened glass doors on glass door hinges. Internally toughened glass shelves on adjustable shelf support system. Fixed glazing panel to back side of unit. Internal low level storage unit in dark oak with cabinet hinges and finger pull to top edge of doors. LED light strip. All cables and cable management to be concealed. |
| ***Item*** | ***Quantity*** | ***Price (£)*** |
| Room 67 Freestanding Display Case | 1x |  |
|  |  |  |
|  |  |  |
|  | **TOTAL** |  |

|  |  |
| --- | --- |
| ***Component*****General Items** | ***Refer to Drawing No :*** |
| ***Specification/ Description:***Contractor to describe any other costs to the client necessary to deliver a complete installation as specification and not included elsewhere in the documentation including for example:*Contractor’s prelims**Contractor’s design development and drawings for approval**Samples of all finishes for approval**O&M manual**As Built drawings* |
| ***Item*** | ***Quantity*** | ***Price (£)*** |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  | **TOTAL** |  |

|  |  |
| --- | --- |
|  | **Price (£)** |
| **ITEM** |   |
|  |  |
|  |   |
|  |   |
|  |   |
|  |   |
|  |   |
|  |   |
|  |   |
|  |   |
|  |   |
|  |   |
|  |   |
|  |   |
|  |   |
|  |   |
|  |   |
|  |   |
|  |   |
|  |   |
|  |   |
|  |   |
|  |   |
|  |   |
|  |   |
|  |   |
|  |   |
|  |  |
|  |   |
|  |   |
|  |   |
|  |   |
|  |   |
|  |   |
|  |   |
|  |   |
|  |   |
|  |   |
|  |  |
| ***GRAND TOTAL*** |  **£** |