{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["Schedule B","Schedule C","Schedule D"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Schedule B","index":0,"n_rows":65,"n_cols":5,"rows_kept":65,"cut":false,"hidden":false,"merged":[]}
["Level","Item","Bill description","Unit","Rate"]
[1,"4.3","0500 - Drainage and Service Ducts",""]
["c","","Ditches",""]
[null,"4.3.5","Clear ditches by removing all material that could impair operation (weed / vegetation growth, silt, debris/rubbish, or eroded banks where present that impede flow and impair operation)","m"]
["c","4.3.10","Filter drains",""]
[null,"4.3.11.1","Edge scrape, clear weed / vegetation growth, cut back to remove build up of material from edge of carriage way through to filter material (Filter Drain and Combined carrier and Filter drain) that could impair operation","m"]
[null,"4.3.11.2","Weed spray along Filter Drain and Combined carrier and Filter drain","m"]
["c","","Balancing / attenuation ponds",""]
[null,"4.3.12","Cycle isolation valves","no."]
["c","","Ancillary items (PCDs, siphons, trash screens, penstocks)",""]
[null,"4.3.13","Clear all material that could impair operation and ensure fit for operation","no."]
["c","4.3.14","Swales",""]
[null,"4.3.14.1","Clear weed / vegetation growth, remove any litter, debris and sediment that could impair operation","m2"]
[null,"4.3.14.2","Undertake a grass cut of the swale to maintain the grass sward between 100mm and 200mm in height","m2"]
["c","4.3.15","Basins",""]
[null,"4.3.15.1","Clear weed / vegetation growth, remove any litter, debris and sediment that could impair operation","m2"]
[null,"4.3.15.2","Undertake a grass cut of the grassed areas of the basin to maintain the grass sward between 100mm and 200mm in height","m2"]
["c","4.3.16","Grassed surface water channel",""]
[null,"4.3.16.1","Undertake a grass cut of all areas of the grassed surface water drainage system to maintain the grass sward at a maximum of 75mm in height","m2"]
[null,"4.3.16.2","Clear weed / vegetation growth, remove any litter, debris and sediment that could impair operation prior to grass cutting","m2"]
[]
[1,"4.8","3000 - Landscape and ecology",""]
["c","","Hedgerows (General)",""]
[null,"4.8.1","Trim hedgerows, maintain and preserve clear carriageway width, sight lines and stopping distance, including junctions, access points, curves and bends","m"]
["c","","Woodland",""]
[null,"4.8.2","Thin/ coppice","m2"]
["c","4.8.3","Grass and vegetation",""]
[null,"4.8.3.1","Maintain and preserve sight lines and stopping distance, including junctions, access points, curves, bends and central reserve.","m2"]
[null,"4.8.3.2","Maintain and preserve CCTV camera operational visibility splays","no."]
[null,"4.8.3.3","Maintain and preserve road users visibility of road traffic signs and signals","no."]
["c","4.8.4","Grass and vegetation",""]
[null,"4.8.4.1","Ensure illumination / lumination from lighting is not obscured.","no."]
[null,"4.8.4.2","Remove obstructions and / or maintain vegetation to facilitate safe access for inspection and maintenance of feeder pillars and technology equipment","no."]
[null,"4.8.4.3","Remove obstructions and maintain vegetation to provide safe access to an use of footways, cycle tracks, bridleways, footpaths and paved pedestrian areas","m2"]
["c","4.8.5","Grass and vegetation",""]
[null,"4.8.5.1","Undertake amenity cut of amenity grass areas, including gate way features, village verges and special landscape features","m2"]
[null,"4.8.5.2","Undertake 2m wide swathe cut of all highway verges to ensure strip remains unobstructed by vegetation throughout the year (in addition to visibility splay maintenance)","m"]
[null,"4.8.5.3","Grass cut the central reserve","m2"]
["c","4.8.6","Grass and vegetation",""]
[null,"4.8.6.1","Remove obstructions and/or maintain vegetation to facilitate safe use of customer facilities. This includes but not limited to emergency roadside telephones and emergency refuge areas.","no."]
[null,"4.8.6.2","Remove vegetation affecting the stability, integrity or operation of structures or other affected property assets.","no."]
["c","","Injurious weeds",""]
[null,"4.8.7","Maintain affected property to control the spread or increase of identified instances of injurious weeds","m2"]
["c","","Invasive plant species",""]
[null,"4.8.8","Maintain affected property to control the spread or increase of identified instances of invasive plant species","m2"]
["c","","Grassland (Open Grassland)",""]
[null,"4.8.9","Maintain habitat integrity, including removal of scrub encroachment","m2"]
["c","","Heath and moorland",""]
[null,"4.8.10","Maintain habitat integrity, including removal of scrub encroachment and tree saplings throughout","m2"]
["c","","Conservation grassland / wildflower grassland",""]
[null,"4.8.11","Maintain habitat integrity, including removal of scrub encroachment and undesirable weed species","m2"]
["c","","Rock scree",""]
[null,"4.8.12","Removal of scrub encroachment","m2"]
["c","","Shrubs (General)",""]
[null,"4.8.13","Maintain habitat integrity, including removal of scrub encroachment","m2"]
["c","","Shrubs (Ornamental)",""]
[null,"4.8.14","Maintain design requirements / amenity function","m2"]
["c","","Woodlands and trees, including veteran trees",""]
[null,"4.8.15","Maintain habitat integrity, including removal of scrub encroachment","m2"]
["c","","Hedgerows (Habitat)",""]
[null,"4.8.16","Maintain habitat integrity, including removal of undesirable species","m2"]
["c","","Wildlife structures and tunnels",""]
[null,"4.8.17","Remove all material that could impair operation","no"]
[]
[null,null,"Note: There are no uplifts applicable for Night or Weekend Working for these works"]

{"sheet":"Schedule C","index":1,"n_rows":21,"n_cols":5,"rows_kept":21,"cut":false,"hidden":false,"merged":[]}
["Level","Item","Bill description","Unit","Rate"]
[1,"","Series 3000 Landscape and ecology (Scope Paragraphs 18.13.2)",""]
["c","","Maintenance of Established Trees",""]
["c","","Removal of branch or limb from tree;",""]
[null,"1","Height not exceeding 4.0m","no"]
[null,"2","Height exceeding  4.0 but not exceeding 10.0m","no"]
["c","","Grass Cutting Reactive Services and Disposal of Waste",""]
["c","","Grass cutting reactive services;",""]
[null,"3","Grass cutter including driver and operators.","hr"]
[null,"4","Disposal of waste.","t"]
["c","","Make safe areas of invasive pests",""]
[null,"5","Make safe areas of invasive pests (including brown tail moth), either through the use of biological solution or by cutting out the affected vegetation to hardstandings and paved areas, topsoil heaps, planted beds, open ditches, filter drains, grassed areas and waterbodies","m2"]
[null,"6","Make safe areas of invasive pests (including brown tail month), either through the use of biological solution or by cutting out affected vegetation to individual trees and shrubs","no"]
["c","","Control and Maintenance of Shrubs, Trees, Woodland, Grassland, Grass and Vegetation",""]
[null,"7","Remove obstructions that prevent safe access, inspection and maintenance of all equipment, as instructed by the Service Manager","m2"]
[]
[]
[null,null,"Note: Above rates are based on Mon to Fri 0700-1900hrs"]
[]
[null,null,"Out of Hours Uplift for Night Working (Mon to Fri 1900-0700hrs)","%"]
[null,null,"Out of Hours Uplift for Weekend Working (0700hrs on Sat to 0700 on Mon)","%"]

{"sheet":"Schedule D","index":2,"n_rows":21,"n_cols":4,"rows_kept":21,"cut":false,"hidden":false,"merged":[]}
[null,"Unit","Day Rate (Shift)","Night Rate (shift)"]
[]
["STRIMMING TEAM - "]
["Supply 2 x Man inclusive of plant/equipment","shift",0,0]
["Supply 3 x Man inclusive of plant/equipment","shift",0,0]
[]
["UNI-MOG SWATHE CUTTING"]
["Unimog & operator / Fuel (including attachments)","shift",0,0]
["Robocut Including Operator ","shift",0,0]
["(Reform) Flail mower & Operator","shift",0,0]
[]
["MISC"]
[]
["3 man herbicide team including chemical","shift",0,0]
["3 man arb team including plant (incl chipper)","shift",0,0]
["2 man arb team including plant (incl chipper)","shift",0,0]
["Emergency call out - 2 Man Arb Team including Plant (incl chipper)","shift",0,0]
["Emergency call out - 3 Man Arb Team including Plant (incl chipper)","shift",0,0]
[]
[]
["Shift rates to be based on 10 hours"]