**West Midlands Fire and Rescue Authority**

**Safe and Well Equipment Framework Agreement**

**Expressions of Interest Form**

**Supplier Name:…………………………………………………………………..**

**Contact Name:……………………………………………………………………..**

**Business Address:……………………………………………………………..**

**Telephone Number:…………………………………………………………….**

**Email:…………………………………………………………………………………**

|  |  |  |
| --- | --- | --- |
| **Item** | **Question** | **Response** |
| **1.** | Would your company be interested in bidding for this framework? |  |
| **2.** | What products could your company supply from the attached product lists for each Lot? |  |
| **3.** | Are there any products not identified that could be added to the framework? |  |
| **4.** | Could your company deliver to all of the UK FRS’s detailed on the NFCC website? |  |
| **5.** | Would there be any delivery charges for orders? |  |
| **6.** | Could call off orders be placed, and stock held at your locations? |  |
| **7.** | Does your company have minimum order quantities? |  |

**Please find attached on page 2 to 4 a list of products required under each Lot**

**Please return this completed form to:** **procurement@wmfs.net** **by 21st July 2020**

**Lot 1 – Fire Resistant Bedding**

|  |  |  |
| --- | --- | --- |
| **Item No.**  | **Description**  | **Requirements**  |
| 1  | Single Bed Pack   | 1 x pillow 2 x pillowcases 2 x Fitted Sheet 1 x Duvet (13.5 tog) 2 x Duvet Covers  |
| 2  | Double Bed Pack  | 2 x pillows 4 x pillowcases 2 x Fitted Sheet  1 x Duvet (13.5 tog) 2 x Duvet Covers  |
| 4  | Kingsize Bed Pack  | 2 x pillows 4 x pillowcases 2 x fitted sheets 1 x Duvet (13.5 tog) 2 x Duvet Covers  |
| 5  | Standard Pillow  | 50cm x 75cm  |
| 6  | Pillowcase  | To fit standard 50cm x 75cm  |
| 7  | Single bedsheet  | Flat   |
| 8  | Single bedsheet  | Fitted  |
| 9  | Double bedsheet  | Flat   |
| 10  | Double bedsheet  | Fitted  |
| 11  | King size bedsheet  | Flat   |
| 12  | King size bedsheet  | Fitted  |
| 13  | Bed throw  | Size 180cm x 230cm  |
| 14  | Bed throw  | Size 228cm x 228cm  |
| 15  | Duvet cover  | Single size  |
| 16  | Duvet cover  | Double size  |
| 17  | Duvet cover  | King size  |
| 18  | Duvet  | Single (10.5 tog)  |
| 19  | Duvet  | Single (13.5 tog)  |
| 20  | Duvet  | Single (15 tog)  |
| 21  | Duvet  | Double (10.5 tog)  |
| 22  | Duvet  | Double (13.5 tog)  |
| 23  | Duvet  | Double (15 tog)  |
| 24  | Duvet  | King (10.5 tog)  |
| 25  | Duvet  | King (13.5 tog)  |
| 26  | Duvet  | King (15 tog)  |
| 27  | Mattress cover/topper  | Fitted single up to 26cm depth  |
| 28  | Mattress cover/topper  | Flat single up to 26cm depth  |
| 29  | Mattress cover/topper  | Fitted double up to 26cm depth  |
| 30  | Mattress cover/topper  | Flat double up to 26cm depth  |
| 31  | Mattress cover/topper  | Fitted King up to 26cm depth  |
| 32  | Mattress cover/topper  | Flat King up to 26cm depth  |
| 33  | Cellular blankets  | Single size 165cm x 210cm  |

**Lot 2 – Home Safety Security Equipment**

|  |  |  |
| --- | --- | --- |
| **Item No.**  | **Description**  | **Specification**  |
| 1  | Blanking Plates  | Aluminum plates 300mm x 75mm which should be =>.9mm or <1.5mm with 6 holes 4 x corner and two central positioned countersunk holes  |
| 2  | Blanking Plates  | Aluminum plates 320mm x 95mm which should be =>.9mm or <1.5mm with 6 holes 4 x corner and two central positioned countersunk holes   |
| 3  | Internal lockable letter box cover  | Steel constructed lockable device which can be placed over existing letter box with options for fixing e.g. heavy-duty stick pads and screws which should also be provided.  The overall min width is 330mm - max width 450mm  The overall min height 80mm – max height 110mm Max depth 30mm  Full installation instructions should be provided.   |
| 4  | Thumb Locks  | A UPVC jammer that can be used on letterboxes.   |
| 5  | External mailbox  | Steel construction 312mm x 320mm with two keys and a fitting kit.  Colours should be predominantly black or white but bidders should state in their bids colours offered.  |
| 6  | Key Safe  | A high security device to meet the Police preferred specification which is, Secured by Design Logo  |
| 7  | Key Safe  | A low security device for internal use with a minimum of a four-digit reprogrammable code  |
| 8  | Arson letterboxes  | For internal use with an in-built fire extinguisher which activates automatically in the event of fire. Costs should also be provided in the pricing schedule for a box without an extinguisher.  Replacement extinguishers should be available   It should be lockable with at least two keys and have the facility to lock plate closed. Dimensions as follows: Actual mailbox not to exceed 600x450x125mm  The framework should be constructed from steel and offer protection for homes from arson attacks. Full installation instructions should be available.   |
| 9  | Arson letter bags  | For internal use with an in-built fire extinguisher which activates automatically in the event of fire. Costs should also be provided in the pricing schedule for a bag without an extinguisher.  Replacement extinguishers should be available   A securable zip closed (can be locked) and the facility to lock internal plate closed. Dimensions as follows:  Actual Mailbag not to exceed 600x500x75mm  The bag should be constructed from a tough, durable and flame-retardant material and the framework constructed from steel Full installation instructions should be available.  |