A close up of a word

Description automatically generated

Resurfacing specification

Hailsham Town Council is looking to resurface the remainder of the pathways and roads at their Ersham Road Cemetery. Areas marked on the map below. This comprises of pathways and roads which are to be blended in with existing work that has already been completed.

Requirements are: -

* Prelim items including, welfare, Traffic management, site supervision etc
* To sweep clean and prepare, to supply and lay avg. 25mm of 6mm surface course asphalt = 273m²
* To cut all necessary keys, to raise ironwork, to sweep clean, to apply bitumen tack coat and to overlay avg. 30mm of 10mm surface course asphalt = 533m²

The map below highlights the remaining areas to be completed within this tender and estimated m².

Aerial view of a green area

Description automatically generated