**The Crescent Play Area**

|  |  |  |
| --- | --- | --- |
| **Description** | **Work Needed** | **Action** |
| Swings – 1 Bay 2 Seat (Cradle) | **Cradle Swings** Damaged wet pour – trip hazard | **Cradle Swings** **AGREED:** No further action to be taken.  |
| Swings – 1 Bay 2 Seat (Flat) | **Flat Swings** Damaged wet pour – trip hazard | **Flat Swings** **AGREED:** No further action to be taken.  |
| Free Standing Slide | **Slide**Damaged wet pour – trip hazard  | **Slide**Remove & Dispose of existing wet pour flooring and replace with either wet pour or grass matt.  |

**Northfield Park, Leicester Road**

|  |  |  |
| --- | --- | --- |
| **Description** | **Work Needed** | **Action** |
| Swings – 2 Bay 3 Seat (Cradle) | Wetpour surface has subsided in some areas | Remove & Dispose of existing wet pour flooring and replace with either wet pour or grass matt.  |

**Oakfield Park, Hospital Lane**

|  |  |  |
| --- | --- | --- |
| **Description** | **Work Needed** | **Action** |
| Rocket – Climbing Frame | Gaps opening between the surface | Resurface the rocket climbing frame area. Remove and dispose of existing wet pour replace with new wet pour or grass matt. |
| Igloo – Climbing Frame | Surface has subsided in some areas | Resurface the igloo climbing frame area. Remove and dispose of existing wet pour replace with new wet pour or grass matt. |
| Swings – 2 Bay 4 Seat (Cradle) | 1. Algae/moss growth
2. Tree debris
3. Gaps between the surface
4. Wear to the shackles
5. Chain wear

 | Remove cradle swings and wet pour and make ground good.  |
| Swings – 2 Bay 4 Seat  | 1. Movement in the cast iron bracket when the swing is under load
2. Trip hazard at the edge of the surface
3. The seat has minor damage
4. Chains are corroded and the links are worn in excess of 40%
5. Wear to the shackles
6. The swing seat connectors are loose

 | Remove cradle swings and replace with new ones with grass matt not wet pour.  |
| Swings – 2 Bay 4 Seat (Flat) | 1. Trip hazard at the edges of the surface
2. Gaps in the opening between the surfacing and the edging
3. Replace missing swing chains and seat
4. Minor damage to seat
5. Swing frame is bent
6. Chain links are worn in excess of 40% and require renewing
7. Wear to the shackles

 | Remove flat swings and replace with new ones with grass matt not wet pour. |
| Free Standing Slide | Gaps in the opening between the surfacing and the edging  | Fill in wet pour gaps |
| Multi Use Games Area (MUGA) |  | Remove this equipment and seek quotations for a replacement climbing frame. |
| Table Tennis | Surface has eroded | Add grass matt to the eroded areas.  |