2. Specification

**Ward Williams Associates**
Compass House

Truro Business Park

Threemilestone

Truro

Cornwall

TR4 9LD

Tel: (01872) 272906

Fax:(01872) 222042

Idless Nursery – Supply and Installation of Glass Houses

**HORTICULTURAL**

**NURSERY,**

**IDLESS,**

**TRURO**

Truro City Council

**Overview**

Truro City Council is issuing an invitation to tender (ITT) to providers of commercial quality horticultural Glasshouses for the supply and installation of two Greenhouses situated at their new nursery site in Idless, Truro.

The proposed works are to assist in the relocation of a commercial horticultural nursery facility to Idless Woods. Works will include the supply and installation of suitable frame and glazing suitable to with stand exposure to extreme weather conditions due to the exposed location within Cornwall. The design will also incorporate necessary ventilation requirement for each greenhouse. An option to incorporate automatic openings for ventilation will be considered. Materials supplied and installed are to be of commercial horticultural nursery quality. Domestic quality products will not be accepted.

An appropriate base is to be specified by the successful contractor and provided to Truro City Council, this element of work is anticipated to be undertaken by others ahead of the supply and installation of glass houses, although costs for this work will be considered as an additional item that may or may not be incorporated with the works. Construction of the base will not form part of the works under this project.

Location of the glass houses is identified in the below plan (glass houses highlighted in green).



**Outline specification**

**Size requirements**

* 1 No. glass house measuring 8m wide and 21m long
* 1 No. glass house measuring 5m wide and 9m long (Prop House)
1. **Base Requirements:**

Include to provide a detailed specification to identify the necessary groundworks and reinforced concrete raft slab requirements (size and specification) for each greenhouse. Construction works relating to enabling groundworks and reinforced concrete base will not form part of the tender evaluation.

Glasshouse supplier may submit a separate price for groundworks and

concrete base work as a turnkey tender option.

1. **Frame requirements:**
* Mill finish aluminium or hot dipped galvanised steel construction with full glass sides.
* braced single span structure
* Apex profile roof system.
* Structural design to be suitable to withstand severe exposure rated for wind speed due to the current site location.
1. **Glazing Requirements:**
* All glazing to be minimum of 4mm toughened glass
* 300mm impact resistant kick panel to be installed at base
1. **Ventilation Requirements:**
* Adequate louvered side ventilation relative to size of each greenhouse
* Suitable number of roof openings to be provided for ventilation requirements of each greenhouse.
* Automatic opening will be considered for ventilation (to be priced as a separate schedule of rate)
1. **Ancillary Works:**
* Include to supply and install suitable rainwater goods including gutters and rainwater downpipes.

**Schedule of Rates**

It is the intention that Truro City Council will separately provide the following, however could you please provide costs for the following.:

* Groundworks and installation of reinforced concrete raft slab base.
	+ Glasshouse supplier may submit a separate price for groundworks and concrete base work as a turnkey tender option.
* Heating system
* Staging and shelving / live shelving
* Automatic Shading
* Electrical system
* Irrigation system