{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["Schedule B","Schedule C","Schedule D"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Schedule B","index":0,"n_rows":9,"n_cols":5,"rows_kept":9,"cut":false,"hidden":false,"merged":[]}
["Level","Item","Bill description","Unit","Rate"]
[1,"4.2","400 - Road Restraint System Road restraint system, and all barrier systems (excluding concrete barriers)",""]
[null,"4.2.1","Check all Road Restraint System","m"]
["c","4.2.2","Tighten or replace screws and bolts and re-tension Road Restraint System requiring re-tensioning.",""]
[null,"4.2.2.1","RRS - Tensioned Corrugated Beam (includes barrier length, transitions and Terminals)","m"]
[null,"4.2.2.2","RRS - Wire Rope Safety Barrier (includes barrier length, transitions and Terminals)","m"]
[]
[]
[null,null,"Note: There are no uplifts applicable for Night or Weekend Working for these works"]

{"sheet":"Schedule C","index":1,"n_rows":196,"n_cols":5,"rows_kept":196,"cut":false,"hidden":false,"merged":[]}
["Level","Item","Bill description","Unit","Rate"]
[1,"","Series 300 FENCING (Scope Paragraph 18.2.1)",""]
["c","","Replacement of Fencing and Gates",""]
["c","","Replacement of post and 3-rail fencing as MCHW HCD H15; 1.1 metres high;",""]
[null,"1","Individual lengths not exceeding 3 metres.","m"]
[null,"2","Individual lengths exceeding 3 metres but not exceeding 10 metres.","m"]
[null,"3","Individual lengths exceeding 10 metres.","m"]
["c","","Replacement of post and 4-rail fencing as MCHW HCD H3; 1.3 metres high;",""]
[null,"4","Individual lengths not exceeding 3 metres.","m"]
[null,"5","Individual lengths exceeding 3 metres but not exceeding 10 metres.","m"]
[null,"6","Individual lengths exceeding 10 metres.","m"]
["c","","Replacement of timber close boarded fencing as MCHW HCD H14; 1.8 metres high;",""]
[null,"7","Individual lengths not exceeding 3 metres.","m"]
[null,"8","Individual lengths exceeding 3 metres but not exceeding 10 metres.","m"]
[null,"9","Individual lengths exceeding 10 metres.","m"]
["c","","Replacement of timber palisade fencing as MCHW HCD H14; 1.8 metres high;",""]
[null,"10","Individual lengths not exceeding 3 metres.","m"]
[null,"11","Individual lengths exceeding 3 metres but not exceeding 10 metres.","m"]
[null,"12","Individual lengths exceeding 10 metres.","m"]
["c","","Concrete foundation to timber post for post and rail, close boarded and palisade fencing;",""]
[null,"13","Not exceeding 5 posts per Task Order.","no"]
[null,"14","Exceeding 5 posts per Task Order.","no"]
[null,"15","Replacement of galvanised steel single field gate as MCHW HCD H17; 3.6 metres wide.","no"]
[null,"16","Replacement of timber field gate as MCH\" H21; 3.6 metres wide.","no"]
[1,"","Series 400 ROAD RESTRAINT SYSTEMS (VEHICLE AND PEDESTRIAN) (Scope Paragraph 18.3.2)",""]
["c","","Replacement of Safety Barriers; designed to be impacted on one side only; straight or curved exceeding 120 metres radius;",""]
[null,"1","Containment performance class N2, working width class W1","m"]
[null,"2","Containment performance class N2, working width class W2","m"]
[null,"3","Containment performance class N2, working width class W3","m"]
[null,"4","Containment performance class N2, working width class W4","m"]
[null,"5","Containment performance class H1, working width class W3","m"]
[null,"6","Containment performance class H1, working width class W4","m"]
[null,"7","Containment performance class H2, working width class W3","m"]
[null,"8","Containment performance class H2, working width class W4","m"]
["c","","Replacement of Safety Barriers; designed to be impacted on both sides; straight or curved exceeding 120 metres radius;",""]
[null,"9","Containment performance class N2, working width class W1","m"]
[null,"10","Containment performance class N2, working width class W2","m"]
[null,"11","Containment performance class N2, working width class W3","m"]
[null,"12","Containment performance class N2, working width class W4","m"]
[null,"13","Containment performance class H1, working width class W3","m"]
[null,"14","Containment performance class H1, working width class W4","m"]
[null,"15","Item removed","m"]
[null,"16","Containment performance class H2, working width class W4","m"]
["c","","Replacement of Safety Barriers; designed to be impacted on one side only; curved exceeding 50 metres radius but not exceeding 120 metres radius;",""]
[null,"17","Containment performance class N2, working width class W1","m"]
[null,"18","Containment performance class N2, working width class W2","m"]
[null,"19","Containment performance class N2, working width class W3","m"]
[null,"20","Containment performance class N2, working width class W4","m"]
[null,"21","Containment performance class H1, working width class W3","m"]
[null,"22","Containment performance class H1, working width class W4","m"]
[null,"23","Containment performance class H2, working width class W3","m"]
[null,"24","Containment performance class H2, working width class W4","m"]
["c","","Replacement of Safety Barriers; designed to be impacted on both sides; curved exceeding 50 metres radius but not exceeding 120 metres radius;",""]
[null,"25","Containment performance class N2, working width class W1","m"]
[null,"26","Containment performance class N2, working width class W2","m"]
[null,"27","Containment performance class N2, working width class W3","m"]
[null,"28","Containment performance class N2, working width class W4","m"]
[null,"29","Containment performance class H1, working width class W3","m"]
[null,"30","Containment performance class H1, working width class W4","m"]
[null,"31","Item removed","m"]
[null,"32","Containment performance class H2, working width class W4","m"]
["c","","Replacement of Safety Barriers; designed to be impacted on one side only; curved not exceeding 50 metres radius;",""]
[null,"33","Containment performance class N2, working width class W1","m"]
[null,"34","Containment performance class N2, working width class W2","m"]
[null,"35","Containment performance class N2, working width class W3","m"]
[null,"36","Containment performance class N2, working width class W4","m"]
[null,"37","Containment performance class H1, working width class W3","m"]
[null,"38","Containment performance class H1, working width class W4","m"]
[null,"39","Containment performance class H2, working width class W3","m"]
[null,"40","Containment performance class H2, working width class W4","m"]
["c","","Replacement of Safety Barriers; designed to be impacted on both sides; curved not exceeding 50 metres radius;",""]
[null,"41","Containment performance class N2, working width class W1","m"]
[null,"42","Containment performance class N2, working width class W2","m"]
[null,"43","Containment performance class N2, working width class W3","m"]
[null,"44","Containment performance class N2, working width class W4","m"]
[null,"45","Containment performance class H1, working width class W3","m"]
[null,"46","Containment performance class H1, working width class W4","m"]
[null,"47","Item removed","m"]
[null,"48","Containment performance class H2, working width class W4","m"]
["c","","Replacement of transitions;",""]
[null,"49","Containment performance class N2, working width class W1","no"]
[null,"50","Containment performance class N2, working width class W2","no"]
[null,"51","Containment performance class N2, working width class W3","no"]
[null,"52","Containment performance class N2, working width class W4","no"]
[null,"53","Containment performance class H1, working width class W3","no"]
[null,"54","Containment performance class H1, working width class W4","no"]
[null,"55","Containment performance class H2, working width class W3","no"]
[null,"56","Containment performance class H2, working width class W4","no"]
["c","","Replacement of posts;  designed to be impacted on one side only;",""]
[null,"57","Containment performance class N2, working width class W1","no"]
[null,"58","Containment performance class N2, working width class W2","no"]
[null,"59","Containment performance class N2, working width class W3","no"]
[null,"60","Containment performance class N2, working width class W4","no"]
[null,"61","Containment performance class H1, working width class W3","no"]
[null,"62","Containment performance class H1, working width class W4","no"]
[null,"63","Containment performance class H2, working width class W3","no"]
[null,"64","Containment performance class H2, working width class W4","no"]
["c","","Replacement of posts;  designed to be impacted on both sides;",""]
[null,"65","Containment performance class N2, working width class W1","no"]
[null,"66","Containment performance class N2, working width class W2","no"]
[null,"67","Containment performance class N2, working width class W3","no"]
[null,"68","Containment performance class N2, working width class W4","no"]
[null,"69","Containment performance class H1, working width class W3","no"]
[null,"70","Containment performance class H1, working width class W4","no"]
[null,"71","Containment performance class H2, working width class W3","no"]
[null,"72","Containment performance class H2, working width class W4","no"]
["c","","Replacement of mounting brackets;",""]
[null,"73","Containment performance class N2, working width class W1","no"]
[null,"74","Containment performance class N2, working width class W2","no"]
[null,"75","Containment performance class N2, working width class W3","no"]
[null,"76","Containment performance class N2, working width class W4","no"]
[null,"77","Containment performance class H1, working width class W3","no"]
[null,"78","Containment performance class H1, working width class W4","no"]
[null,"79","Containment performance class H2, working width class W3","no"]
[null,"80","Containment performance class H2, working width class W4","no"]
["c","","Replacement of terminal section; designed to be impacted on one side only;",""]
[null,"81","Terminal P1, D.1.1","no"]
[null,"82","Terminal P4, D.1.1","no"]
["c","","Replacement of terminal section; designed to be impacted on both sides;",""]
[null,"83","Terminal P1, D.1.1","no"]
[null,"84","Terminal P4, D.1.1","no"]
["c","","Replacement of full height anchorage; designed to be impacted on one side only;",""]
[null,"85","Containment performance class N2, working width class W1","no"]
[null,"86","Containment performance class N2, working width class W2","no"]
[null,"87","Containment performance class N2, working width class W3","no"]
[null,"88","Containment performance class N2, working width class W4","no"]
[null,"89","Containment performance class H1, working width class W3","no"]
[null,"90","Containment performance class H1, working width class W4","no"]
[null,"91","Containment performance class H2, working width class W3","no"]
[null,"92","Containment performance class H2, working width class W4","no"]
["c","","Replacement of full height anchorage; designed to be impacted on both sides;",""]
[null,"93","Containment performance class N2, working width class W1","no"]
[null,"94","Containment performance class N2, working width class W2","no"]
[null,"95","Containment performance class N2, working width class W3","no"]
[null,"96","Containment performance class N2, working width class W4","no"]
[null,"97","Containment performance class H1, working width class W3","no"]
[null,"98","Containment performance class H1, working width class W4","no"]
[null,"99","Containment performance class H2, working width class W3","no"]
[null,"100","Containment performance class H2, working width class W4","no"]
["c","","Replacement of expansion joint anchorage;  designed to be impacted on one side only;",""]
[null,"101","Containment performance class N2, working width class W1","no"]
[null,"102","Containment performance class N2, working width class W2","no"]
[null,"103","Containment performance class N2, working width class W3","no"]
[null,"104","Containment performance class N2, working width class W4","no"]
[null,"105","Containment performance class H1, working width class W3","no"]
[null,"106","Containment performance class H1, working width class W4","no"]
[null,"107","Containment performance class H2, working width class W3","no"]
[null,"108","Containment performance class H2, working width class W4","no"]
["c","","Replacement of expansion joint anchorage;  designed to be impacted on both sides;",""]
[null,"109","Containment performance class N2, working width class W1","no"]
[null,"110","Containment performance class N2, working width class W2","no"]
[null,"111","Containment performance class N2, working width class W3","no"]
[null,"112","Containment performance class N2, working width class W4","no"]
[null,"113","Containment performance class H1, working width class W3","no"]
[null,"114","Containment performance class H1, working width class W4","no"]
[null,"115","Containment performance class H2, working width class W3","no"]
[null,"116","Containment performance class H2, working width class W4","no"]
["c","","Replacement of connection to bridge parapet;",""]
[null,"117","Containment performance class N2, working width class W1","no"]
[null,"118","Containment performance class N2, working width class W2","no"]
[null,"119","Containment performance class N2, working width class W3","no"]
[null,"120","Containment performance class N2, working width class W4","no"]
[null,"121","Containment performance class H1, working width class W3","no"]
[null,"122","Containment performance class H1, working width class W4","no"]
[null,"123","Containment performance class H2, working width class W3","no"]
[null,"124","Containment performance class H2, working width class W4","no"]
["c","","Concrete foundation to replacement posts;",""]
[null,"125","Containment performance class N2, working width class W1","no"]
[null,"126","Containment performance class N2, working width class W2","no"]
[null,"127","Containment performance class N2, working width class W3","no"]
[null,"128","Containment performance class N2, working width class W4","no"]
[null,"129","Containment performance class H1, working width class W3","no"]
[null,"130","Containment performance class H1, working width class W4","no"]
[null,"131","Containment performance class H2, working width class W3","no"]
[null,"132","Containment performance class H2, working width class W4","no"]
["c","","Socketed foundation to replacement posts;",""]
[null,"133","Containment performance class N2, working width class W1","no"]
[null,"134","Containment performance class N2, working width class W2","no"]
[null,"135","Containment performance class N2, working width class W3","no"]
[null,"136","Containment performance class N2, working width class W4","no"]
[null,"137","Containment performance class H1, working width class W3","no"]
[null,"138","Containment performance class H1, working width class W4","no"]
[null,"139","Containment performance class H2, working width class W3","no"]
[null,"140","Containment performance class H2, working width class W4","no"]
["c","","Replacement of crash cushion;  designed to be impacted on one side only;",""]
[null,"141","Crash cushion Z1 Class A D.1.1 redirective","no"]
[null,"142","Crash cushion Z1 Class A D.1.1 non redirective","no"]
["c","","Replacement of crash cushion;  designed to be impacted on both sides;",""]
[null,"143","Crash cushion Z1 Class A D.1.1 redirective","no"]
[null,"144","Crash cushion Z1 Class A D.1.1 non redirective","no"]
[]
[]
[null,null,"Note: Above rates are based on Mon to Fri 0700-1900hrs"]
[]
[null,null,"Out of Hours Uplift for Night Working (Mon to Fri 1900-0700hrs)","%"]
[null,null,"Out of Hours Uplift for Weekend Working (0700hrs on Sat to 0700 on Mon)","%"]

{"sheet":"Schedule D","index":2,"n_rows":14,"n_cols":5,"rows_kept":14,"cut":false,"hidden":false,"merged":[[10,2,10,4]]}
[null,"Description","Days","Nights","Weekends"]
[1,"Three man gang with barrier rig"]
[2,"Three man gang with barrier rig and Excavator"]
[3,"Four man gang with barrier rig"]
[4,"Four man gang with barrier rig and Excavator"]
[5,"Emergency Makesafe"]
[6,"Coring gang"]
[7,"Two man gang Post testing"]
[8,"Inspection of repairs Shift"]
[9,"Grab Wagon"]
[10,"Delivery of materials to site "]
[]
[]
[null,"Shift rates to be based on 10 hours"]