****

Specification – Supply, installation and commissioning of holding tank

Reference: BUS003\_0095

**A red truck parked on a gravel road next to water

Description automatically generated**

## Background

Pellows Waste disposal is a family run business which has been established over 50 years, making us Cornwall's oldest liquid waste disposal contractor. Pellows specialise in septic tank emptying as well as all other areas of drain maintenance, liquid waste collection, transport and disposal. Pellows cover the whole of the South West and have many vehicles to suite even the smallest of country lanes. We operate a 24/7 telephone line for emergency and regular work and pride ourselves on our prompt and reliable service.

Our drivers are some of the most experienced in the business and share our company vision to provide the best customer care and service possible while maintaining exceptional value for money.

Pellows is entering a transformative stage. Our new sewage treatment works and offices will be game changing for the organisation and the staff.

Part of this works requires a new holding tank:

## Specification

Pellows is seeking the design, build, installation and commissioning of a holding tank.

Specific requirements of this tender, which the tenderers will need to satisfy, and the successful tenderer will be required to deliver on are:

* 2 x 200 tonne storage tank for liquid wastewater.
* Tanks to be above ground
* Tanks requires two low level outlets: one designed for the artic lorries to connect up to and the other is designed for the onsite pump station.
* Material is not specified – but MUST be suitable for holding wastewater.
* Tanks to have an operational design life of 10 years minimum, subject to maintenance in line with the manufacturer’s recommendations.
* Ladder extra as an extra cost.

Costs to include:

* Supply, delivery and transportation to the Pellows site, installation, commissioning, including testing and training.
* The design, materials, installations, inspections, maintenance and operations of the tank to comply with all relevant Regulatory requirements and standards e.g. British Standards (BS), European Standards / Norm (EN), international Standards Organisation (ISO) or equivalent.
* Work to be carried out during normal working hours. Installation to be completed by February 2025.
* Details of lead time is essential.