**Expression of Interest**

**Hunton Bridge Rock Armour, Kington**

**Background**

The River Arrow is causing the north side embankment to scour, posing a risk to the bridge structure.


The proposed scheme is to install approximately 31m of rock armour along the north side embankment to avert further erosion. 0.5m rock armour is to be installed at a slope of 30º, maintaining the embankment’s existing height.

**Proposed solution**

Rock Armour as per the PCI Pack

We are bound by ecological constraints to complete works by 1st October due to the River.

**Location**

****