Appendix 6

Broadway Play Area

Specification for Play Area:

The play area required is more circular in shape with a boundary fencing of some 66 linear metres.

Within the boundary fencing the surface will be that of wetpour with required base preparation.