**PRICING SCENARIO ORDER NUMBER – DBS/001**

# FOR THE PROVISION OF A PORTLAND STONE

# ARMY HEADSTONE

# The wording and layout below will be engraved on the stone.

# Please ensure it is correct.

|  |  |  |
| --- | --- | --- |
| Regimental Badge/Crest | Royal Corps of Army Music | - |

|  |  |  |
| --- | --- | --- |
| Number and Rank | 12345678 MUSICIAN | 16 |

|  |  |  |
| --- | --- | --- |
| Name and Honours | PORTLAND STONE | 13 |

|  |  |  |
| --- | --- | --- |
| Regiment or Corps | **ROYAL CORPS OF ARMY MUSIC** | **21** |

|  |  |  |
| --- | --- | --- |
| Date of Death and Age | **15TH  FEBRUARY 2056 • AGE 19** | **21** |

|  |  |  |
| --- | --- | --- |
| Religious Emblem | Star of David | - |

|  |  |  |
| --- | --- | --- |
| Next of Kin’s Inscription (Max 4 Lines of up to 28 letters and spaces per line) | **THOSE WE LOVE**  **DON’T GO AWAY**  **THEY WALK BESIDE US**  **EVERYDAY** | **11**  **10**  **16**  **8** |

**119 (inc Plot No.)**

Total Number of Characters: 3 (plot number on rear of headstone)

Fixing Requirements: *Concrete Shoe Foundation (fixing method to be confirmed by contactor with the local/cemetery/churchyard authority)*

To be Manufactured By: 16 Sep 2056. To be fixed by but not before: 30 Sep 2056

Church/Cemetery details: Caister Cemetery, Great Yarmouth, Norfolk, NR30 5NL

Grave Details**:** Section East, Grave No 42

Contact at Church/Cemetery:

Details of Funeral Director**:**

Special Instructions: Permit attached and fees paid. Grave section and number to be engraved on the rear of the headstone in the following format – E42.

**Pricing Scenario 1**

To be completed by Tenderer - for pricing evaluation purposes please complete the prices in the table below (as provided in 705616451 Schedule 2 – Schedule of Requirements) for the above Scenario tasking order.

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Item No | Description  of Service | Quantity | Price (£) – As per Schedule 2  Year 1 | Price (£) – As per Schedule 2  Year 2 | Price (£) – As per Schedule 2  Option Year 1 | Price (£)– As  Schedule 2  Option Year 2 | Total Item Price (£)  (Y1+Y2+  Op Y1+Op Y2) |
| 3 | ARMY HEADSTONE  Drawing No A/74/1\*  To include engraving of brackets, colons, commas, full stops, hyphens, inverted commas, oblique strokes, and semi-colons. | 1 |  |  |  |  |  |
| 8 | Regimental/Service crest | 1 |  |  |  |  |  |
| 9 | Religious or Cultural Emblem (other than Latin/Broad cross) | 1 |  |  |  |  |  |
| 10 | Letters and Numbers (per character)  (All numerals to be inscribed on same level top and bottom). Height as detailed in layout drawings, either 22.2mm (7/8”), 15.8mm (5/8”) or 10mm (3/8”) high.  NOTE- engraving of brackets, colons, commas, full stops, hyphens, inverted commas, oblique strokes, and semi-colons included in items 1-5) | 119 |  |  |  |  |  |
| 11 | Fixing of memorial in the UK (to include NI) with a Concrete Foundation Shoe in accordance with NAMM shape and dimension guidelines (Appendix 1 to Annex B to Schedule 2) | 1 |  |  |  |  |  |
| **Scenario 1 Total** | | | | | | |  |

**PRICING SCENARIO ORDER NUMBER – DBS/002**

# FOR THE PROVISION OF A PORTLAND STONE

# ROYAL NAVY HEADSTONE

**The wording and layout below will be engraved on the stone.**

**Please ensure it is correct.**

|  |  |  |
| --- | --- | --- |
| RN/RM Crest | **Royal Navy Crest (to be placed within Broad Cross)** | **-** |
|  |  |  |
| Inits, Name and Honours | **PORTLAND STONE** | **13** |
|  |  |  |
| Rating, Branch, Serv No | **AB1 ET(WESM)(CIS) 12345678** | **20** |
|  |  |  |
| Ship or Unit | **ROYAL NAVY** | **9** |
|  |  |  |
| Date of Death and Age | **15TH FEBRUARY 2056 • AGE 19** | **21** |
|  |  |  |
| Religious Emblem | **Broad Cross (with Royal Navy Crest in centre)** | **-** |
|  |  |  |
| Next of Kin’s Inscription  (Max 4 Lines of up to 28 letters and spaces per line) | **THOSE WE LOVE**  **DON’T GO AWAY**  **THEY WALK BESIDE US**  **EVERYDAY** | **11**  **10**  **16**  **8** |

Total Number of Characters:

**108**

Fixing Requirements: *Matching Base with Dowels (fixing method to be confirmed by contactor with the local cemetery/churchyard authority)*

To be Manufactured By: 16 Sep 2056 To be fixed by : 30 Sep 2056

Churchyard/Cemetery details: Caister Cemetery, Great Yarmouth, Norfolk, NR30 5NL

Grave Details: Section East, Grave No 42

Contact at Church/Cemetery:

Details of Funeral Director:

Special Instructions: Permit attached and fees paid. Concrete beam in place. Headstone to be cut short by 7” as it will sit on a base/beam.

**Pricing Scenario 2**

To be completed by Tenderer - for pricing evaluation purposes please complete the prices in the table below (as provided in 705616451 Schedule 2 – Schedule of Requirements) for the above Scenario tasking order.

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Item No | Description  of Service | Quantity | Price (£) – As per Schedule 2  Year 1 | Price (£) – As per Schedule 2  Year 2 | Price (£) – As per Schedule 2  Option Year 1 | Price (£)– As per Schedule 2  Option Year 2 | Total Item Price (£)  (Y1+Y2+  Op Y1+Op Y2) |
| 1 | ROYAL **NAVY** HEADSTONE  Drawing No **2283**/58\*  To include engraving of brackets, colons, commas, full stops, hyphens, inverted commas, oblique strokes, and semi-colons. | 1 |  |  |  |  |  |
| 7A | Broad Cross | 1 |  |  |  |  |  |
| 8 | Regimental/Service crest | 1 |  |  |  |  |  |
| 9 | Religious or Cultural Emblem (other than Latin/Broad cross) |  |  |  |  |  |  |
| 10 | Letters and Numbers (per character)  (All numerals to be inscribed on same level top and bottom). Height as detailed in layout drawings, either 22.2mm (7/8”), 15.8mm (5/8”) or 10mm (3/8”) high.  NOTE- engraving of brackets, colons, commas, full stops, hyphens, inverted commas, oblique strokes, and semi-colons included in items 1-5) | 108 |  |  |  |  |  |
| 12 | Fixing of memorial in the UK (to include NI) with an above ground matching base for fixing on a concrete beam/raft, including all necessary drilling and 3 x 12mm stainless steel dowels (Appendix 2 to Annex B to Schedule 2) | 1 |  |  |  |  |  |
| **Scenario 2 Total** | | | | | | |  |

**PRICING SCENARIO ORDER NUMBER – DBS/003**

# FOR THE PROVISION OF A PORTLAND STONE

# RAF HEADSTONE

# The wording and layout below will be engraved on the stone.

# Please ensure it is correct.

|  |  |  |
| --- | --- | --- |
| RAF Crest | **Copy provided** | **-** |
|  |  |  |
| Rank | AIR SPECIALIST 1 | 14 |
|  |  |  |
| Name, Honours, Decorations | **PORTLAND STONE** | **13**  AL3 |
|  |  |  |
| Service Number (airmen) | 30123456 | 8 |
|  |  |  |
| Service | ROYAL AIR FORCE | 13 |
|  |  |  |
| Date of Death and Age | **15TH FEBRUARY 2056 • AGE 19** | 21 |
|  |  |  |
| Religious Emblem | **LATIN CROSS (6”)** | **-** |
|  |  |  |
| Personal Inscription (Max 4 Lines of up to 28 letters and spaces per line) | **THOSE WE LOVE**  **DON’T GO AWAY**  **THEY WALK BESIDE US**  **EVERYDAY** | **11**  **10**  **16**  **8** |

Total Number of Characters:

**114124**

Fixing Requirements: *~~Concrete Shoe Foundation~~/~~Matching Base with Dowels~~/Independent Foundation and Matching Base with dowels and Ground Anchor (fixing method to be confirmed by contactor with the local cemetery/churchyard authority)*

To be Manufactured By: 16 Sep 2056 To be fixed by/not before: 30 Sep 2056

Churchyard/Cemetery details: Caister Cemetery, Great Yarmouth, Norfolk, NE30 5NL

Grave Details: Section East, Grave No. 42

Contact at Church/Cemetery:

Details of Funeral Director:

Special Instructions:

Permit attached and fees paid. Headstone to be cut by 7” and will sit on an independent foundation with a matching base.

**Pricing Scenario 3**

To be completed by Tenderer - for pricing evaluation purposes please complete the prices in the table below (as provided in 705616451 Schedule 2 – Schedule of Requirements) for the above Scenario tasking order.

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Item No | Description  of Service | Quantity | Price (£) – As per Schedule 2  Year 1 | Price (£) – As per Schedule 2  Year 2 | Price (£) – As per Schedule 2  Option Year 1 | Price (£)– As per Schedule 2  Option Year 2 | Total Item Price (£)  (Y1+Y2+  Op Y1+Op Y2) |
| 18 | KARIN GRANITE ARMY HEADSTONE  Drawing No A/74/1\*  To include engraving of brackets, colons, commas, full stops, hyphens, inverted commas, oblique strokes, and semi-colons. | 1 |  |  |  |  |  |
| 21B | Karin Granite - Latin Cross 6” | 1 |  |  |  |  |  |
| 23 | Karin Granite - Regimental/Service Crest | 1 |  |  |  |  |  |
| 24 | Karin Granite - Religious or Cultural Emblem (other than Latin/Broad Cross) |  |  |  |  |  |  |
| 25 | Karin Granite - Letters and Numbers (per character)  (Letters and numbers are to be incised and painted with Sign Writing Black Enamel with a Gloss Finish. All numerals to be inscribed on same level top and bottom). Height as detailed in layout drawings, either 22.2mm (7/8”), 15.8mm (5/8”) or 10mm (3/8”) high.  (NOTE- engraving of brackets, colons, commas, full stops, hyphens, inverted commas, oblique strokes, and semi-colons included in items 16-20) | 114 |  |  |  |  |  |
| 28A | Fixing of a Karin Granite memorial in the UK (to include NI) with an above ground matching base and Independent Foundation for memorial to be fixed at ground level, including all necessary drilling, 2 x 16mm stainless steel dowels and ground anchor (Appendix 6 to Annex B to Schedule 2) | 1 |  |  |  |  |  |
| **Scenario 3 Total** | | | | | | |  |

**PRICING SCENARIO ORDER NUMBER – DBS//004**

# FOR THE PROVISION OF A KARIN GRANITE STONE

# ARMY HEADSTONE

# The wording and layout below will be engraved on the stone.

# Please ensure it is correct.

|  |  |  |
| --- | --- | --- |
| Regimental Badge/Crest | Royal Corps of Army Music | - |
|  |  |  |
| Number and Rank | 12345678 MUSICIAN | 16 |
|  |  |  |
| Name and Honours | KARIN GRANITE | 12 |
|  |  |  |
| Regiment or Corps | **ROYAL CORPS OF ARMY MUSIC** | **21** |
|  |  |  |
| Date of Death and Age | **15TH FEBRUARY 2056 • AGE 19** | **21** |
|  |  |  |
| Religious Emblem | Star of David | - |
|  |  |  |
| Next of Kin’s Inscription (Max 4 Lines of up to 28 letters and spaces per line) | **THOSE WE LOVE**  **DON’T GO AWAY**  **THEY WALK BESIDE US**  **EVERYDAY** | **11**  **10**  **16**  **8** |

Total Number of Characters: 3 (plot number on rear of headstone)

**118 (inc. Plot No.)**

Fixing Requirements: *Concrete Shoe Foundation (fixing method to be confirmed by contactor with the local/cemetery/churchyard authority)*

To be Manufactured By:16 Sep 2056 To be fixed by/not before: 30 Sep 2056

Church/Cemetery details: Caister Cemetery, Great Yarmouth, Norfolk, NE30 5NL

Grave Details**:** Section East, Grave no. 42

Contact at Church/Cemetery:

Details of Funeral Director**:**

Special Instructions: Grave section and number to be engraved on the rear of the headstone in the following format - SA/2.

**Pricing Scenario 4**

To be completed by Tenderer - for pricing evaluation purposes please complete the prices in the table below (as provided in 705616451 Schedule 2 – Schedule of Requirements) for the above Scenario tasking order.

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Item No | Description  of Service | Quantity | Price (£) – As per Schedule 2  Year 1 | Price (£) – As per Schedule 2  Year 2 | Price (£) – As per Schedule 2  Option Year 1 | Price (£)– As per  Schedule 2  Option Year 2 | Total Item Price (£)  (Y1+Y2+  Op Y1+Op Y2) |
| 18 | KARIN GRANITE ARMY HEADSTONE  Drawing No A/74/1\*  To include engraving of brackets, colons, commas, full stops, hyphens, inverted commas, oblique strokes, and semi-colons. | 1 |  |  |  |  |  |
| 23 | Karin Granite - Regimental/Service Crest | 1 |  |  |  |  |  |
| 24 | Karin Granite - Religious or Cultural Emblem (other than Latin/Broad Cross) | 1 |  |  |  |  |  |
| 25 | Karin Granite - Letters and Numbers (per character)  (Letters and numbers are to be incised and painted with Sign Writing Black Enamel with a Gloss Finish. All numerals to be inscribed on same level top and bottom). Height as detailed in layout drawings, either 22.2mm (7/8”), 15.8mm (5/8”) or 10mm (3/8”) high.  (NOTE- engraving of brackets, colons, commas, full stops, hyphens, inverted commas, oblique strokes, and semi-colons included in items 16-20) | 118 |  |  |  |  |  |
| 11 | Fixing of a Karin Granite memorial in the UK (to include NI) with a Concrete Foundation Shoe in accordance with NAMM shape and dimension guidelines (Appendix 4 to Annex B to Schedule 2) | 1 |  |  |  |  |  |
| **Scenario 4 Total** | | | | | | |  |

**PRICING SCENARIO ORDER NUMBER – DBS//005**

# FOR THE PROVISION OF A KARIN GRANITE STONE

# ROYAL NAVY HEADSTONE

**The wording and layout below will be engraved on the stone.**

**Please ensure it is correct.**

|  |  |  |
| --- | --- | --- |
| RN/RM Crest | **Royal Navy Crest (to be placed within Broad Cross)** | **-** |
|  |  |  |
| Inits, Name and Honours | **KARIN GRANITE** | **12** |
|  |  |  |
| Rating, Branch, Serv No | **AB1 ET(WESM)(CIS) 12345678** | **20** |
|  |  |  |
| Ship or Unit | **ROYAL NAVY** | **9** |
|  |  |  |
| Date of Death and Age | **15TH FEBRUARY 2056 • AGE 19** | **21** |
|  |  |  |
| Religious Emblem | **Broad Cross (with Royal Navy Crest in centre)** | **-** |
|  |  |  |
| Next of Kin’s Inscription  (Max 4 Lines of up to 28 letters and spaces per line) | **THOSE WE LOVE**  **DON’T GO AWAY**  **THEY WALK BESIDE US**  **EVERYDAY** | **11**  **10**  **16**  **8** |

Total Number of Characters:

**107**

Fixing Requirements: *Matching Base with Dowels (fixing method to be confirmed by contactor with the local cemetery/churchyard authority)*

To be Manufactured By: 16 Sep 2056 To be fixed by/not before: 30 Sep 2056

Churchyard/Cemetery details: Caister Cemetery, Great Yarmouth, Norfolk, NR30 5NL

## Grave Details: Section East, Grave no 42

Contact at Church/Cemetery:

Details of Funeral Director:

Special Instructions: Permit attached and fees paid. Concrete beam in place. Headstone to be cut short by 7” as it will sit on a base/beam.

**Pricing Scenario 5**

To be completed by Tenderer - for pricing evaluation purposes please complete the prices in the table below (as provided in 705616451 Schedule 2 – Schedule of Requirements) for the above Scenario tasking order.

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Item No | Description  of Service | Quantity | Price (£) – As per Schedule 2  Year 1 | Price (£) – As per  Schedule 2  Year 2 | Price (£) – As per  Schedule 2  Option Year 1 | Price (£)– As per  Schedule 2  Option Year 2 | Total Item Price (£)  (Y1+Y2+  Op Y1+Op Y2) |
| 17 | KARIN GRANITE ROYAL NAVY HEADSTONE  Drawing No 2283/58\*  To include engraving of brackets, colons, commas, full stops, hyphens, inverted commas, oblique strokes, and semi-colons. | 1 |  |  |  |  |  |
| 22A | Karin Granite - Broad Cross | 1 |  |  |  |  |  |
| 23 | Karin Granite - Regimental/Service Crest | 1 |  |  |  |  |  |
| 25 | Karin Granite - Letters and Numbers (per character)  (Letters and numbers are to be incised and painted with Sign Writing Black Enamel with a Gloss Finish. All numerals to be inscribed on same level top and bottom). Height as detailed in layout drawings, either 22.2mm (7/8”), 15.8mm (5/8”) or 10mm (3/8”) high.  (NOTE- engraving of brackets, colons, commas, full stops, hyphens, inverted commas, oblique strokes, and semi-colons included in items 16-20) | 107 |  |  |  |  |  |
| 27 | Fixing of a Karin Granite memorial in the UK (to include NI) with an above ground matching base for fixing on a concrete beam/raft, including all necessary drilling and 2 x 16mm stainless steel dowels (Appendix 5 to Annex B to Schedule 2) | 1 |  |  |  |  |  |
| **Scenario 5 Total** | | | | | | |  |

**PRICING SCENARIO ORDER NUMBER – DBS//006**

# FOR THE PROVISION OF A KARIN GRANITE STONE

# RAF HEADSTONE

# The wording and layout below will be engraved on the stone.

# Please ensure it is correct.

|  |  |  |
| --- | --- | --- |
| RAF Crest | **Copy enclosed** | **-** |
|  |  |  |
| Rank | AIR SPECIALIST 1 | 14 |
|  |  |  |
| Name, Honours, Decorations | **KARIN GRANITE** | **12**  AL3 |
|  |  |  |
| Service Number (airmen) | 30123456 | 8 |
|  |  |  |
| Service | ROYAL AIR FORCE | 13 |
|  |  |  |
| Date of Death and Age | **15TH FEBRUARY 2056 • AGE 19** | 21 |
|  |  |  |
| Religious Emblem | **LATIN CROSS (6”)** | **-** |
|  |  |  |
| Next of Kin’s Inscription (Max 4 Lines of up to 28 letters and spaces per line) | **THOSE WE LOVE**  **DON’T GO AWAY**  **THEY WALK BESIDE US**  **EVERYDAY** | **11**  **10**  **16**  **8** |

Total Number of Characters:

**113**

Fixing Requirements: *Independent Foundation and Matching Base with dowels and Ground Anchor (fixing method to be confirmed by contactor with the local cemetery/churchyard authority)*

To be Manufactured By: 16 Sep 2056 To be fixed by/not before: 30 Sep 2056

Churchyard/Cemetery details: Caister Cemetery, Great Yarmouth, Norfolk, NR30 5NL

## Grave Details: Section East, Grave No. 42

Contact at Church/Cemetery:

Details of Funeral Director:

Special Instructions: Permit attached and fees paid. Headstone to be cut by 7” and will sit on an independent foundation with a matching base.

**Pricing Scenario 6**

To be completed by Tenderer - for pricing evaluation purposes please complete the prices in the table below (as provided in 705616451 Schedule 2 – Schedule of Requirements) for the above Scenario tasking order.

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Item No | Description  of Service | Quantity | Price (£) – As per Schedule 2  Year 1 | Price (£) – As per  Schedule 2  Year 2 | Price (£) – As per  Schedule 2  Option Year 1 | Price (£) – As per  Schedule 2  Option Year 2 | Total Item Price (£)  (Y1+Y2+  Op Y1+Op Y2) |
| 19 | KARIN GRANITE ROYAL AIR FORCE HEADSTONE  For deaths on or before 07/02/1952 - Drawing No 5393/52\*  For deaths after 07/02/1952 – Drawing No. 13661\*  To include engraving of brackets, colons, commas, full stops, hyphens, inverted commas, oblique strokes, and semi-colons. | 1 |  |  |  |  |  |
| 21B | Karin Granite - Latin Cross 6” | 1 |  |  |  |  |  |
| 23 | Karin Granite - Regimental/Service Crest | 1 |  |  |  |  |  |
| 25 | Karin Granite - Letters and Numbers (per character)  (Letters and numbers are to be incised and painted with Sign Writing Black Enamel with a Gloss Finish. All numerals to be inscribed on same level top and bottom). Height as detailed in layout drawings, either 22.2mm (7/8”), 15.8mm (5/8”) or 10mm (3/8”) high.  (NOTE- engraving of brackets, colons, commas, full stops, hyphens, inverted commas, oblique strokes, and semi-colons included in items 16-20) | 113 |  |  |  |  |  |
| 28A | Fixing of a Karin Granite memorial in the UK (to include NI) with an above ground matching base and Independent Foundation for memorial to be fixed at ground level, including all necessary drilling, 2 x 16mm stainless steel dowels and ground anchor (Appendix 6 to Annex B to Schedule 2) | 1 |  |  |  |  |  |
| **Scenario 6 Total** | | | | | | |  |

**PRICING SCENARIO ORDER NUMBER – DBS/007**

# FOR THE PROVISION OF A NABRESINA LIMESTONE

# ARMY UPM

# The wording and layout below will be engraved on the stone.

# Please ensure it is correct.

|  |  |  |
| --- | --- | --- |
| Regimental Badge/Crest | Royal Corps of Army Music | - |
|  |  |  |
| Number and Rank | 12345678 MUSICIAN | 16 |
|  |  |  |
| Name and Honours | NABRESINA LIMESTONE | 18 |
|  |  |  |
| Regiment or Corps | **ROYAL CORPS OF ARMY MUSIC** | **21** |
|  |  |  |
| Date of Death and Age | **15TH FEBRUARY 2056 • AGE 19** | **21** |
|  |  |  |
| Religious Emblem | N/A |  |
|  |  |  |
| Next of Kin’s Inscription (Max 2 Lines of up to 25 letters and spaces per line) | **A MUCH LOVED SON,**  **WHO WILL BE SORELY MISSED** | **13**  **21** |

Total Number of Characters:

**110**

Fixing Requirements: *To be fixed flush with the ground (fixing method to be confirmed by contactor with the local cemetery/churchyard authority)*

To be Completed By: 16 Sep 2056 To be Fixed By: 30 Sep 2056

Church/Cemetery details: Gloucester Crematorium

Grave Details**:**

Contact at Church/Cemetery:

Details of Funeral Director**:**

Special Instructions:

**Pricing Scenario 7**

To be completed by Tenderer - for pricing evaluation purposes please complete the prices in the table below (as provided in 705616451 Schedule 2 – Schedule of Requirements) for the above Scenario tasking order.

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Item No | Description  of Service | Quantity | Price (£) – As per Schedule 2  Year 1 | Price (£) – As per Schedule 2  Year 2 | Price (£) – As per Schedule 2  Option Year 1 | Price (£)– As per Schedule 2  Option Year 2 | Total Item Price (£)  (Y1+Y2+  Op Y1+Op Y2) |
| 31 | Nabresina Limestone Urn Plot Marker Stone  To include engraving of brackets, colons, commas, full stops, hyphens, inverted commas, oblique strokes, and semi-colons.  Dimensions  304.8mm x 304.8mm x 50.8mm (12” x 12” x 2”) | 1 |  |  |  |  |  |
| 32 | Nabresina Limestone - Regimental/Service crest (actuarily reduced as required) | 1 |  |  |  |  |  |
| 33 | Nabresina Limestone - Letters and Numbers (per character)  To include Service Number, Rank, Name, Regiment/Service, Date of Death and Age. Two lines of Personal Inscription with each line to be no more than 25 symbols and spaces.  (Letters and numbers are to be incised and painted with Sign Writing Black Enamel with a Gloss Finish. All numerals to be inscribed on same level top and bottom). Height as detailed in layout drawings, either 22.2mm (7/8”), 15.8mm (5/8”) or 10.0mm (3/8”) high.  (NOTE- engraving of brackets, colons, commas, full stops, hyphens, inverted commas, oblique strokes, and semi-colons included in item 31) | 110 |  |  |  |  |  |
| 34 | Fixing/placing memorial flush with the ground. | 1 |  |  |  |  |  |
| **Scenario 7 Total** | | | | | | |  |

**PRICING SCENARIO ORDER NUMBER – DBS//008**

# FOR THE PROVISION OF A NABRESINA LIMESTONE

# ROYAL AIR FORCE UPM

# The wording and layout below will be engraved on the stone.

# Please ensure it is correct.

|  |  |  |
| --- | --- | --- |
| Regimental Badge/Crest | RAF CREST | - |
|  |  |  |
| Rank | FLIGHT SERGEANT | 14 |
|  |  |  |
| Name and Honours | NABRESINA LIMESTONE | 18 |
|  |  |  |
| Service Number | **A1234567** | **8** |
|  |  |  |
| Regiment or Corps | **ROYAL AIR FORCE** | **13** |
|  |  |  |
| Date of Death and Age | **15TH FEBRUARY 2056 • AGE 45** | **21** |
|  |  |  |
|  |  |  |
| Next of Kin’s Inscription (Max 2 Lines of up to 25 letters and spaces per line) | **FOREVER IN OUR HEARTS**  **NEVER FORGOTTEN** | **18**  **14** |

Total Number of Characters:

**106**

Fixing Requirements: *To be fixed flush with the ground using an independent foundation (fixing method to be confirmed by contactor with the local cemetery/churchyard authority)*

To be Completed By: 16 Sep 2056 To be Fixed By: 30 Sep2056

Church/Cemetery details: Gloucester Crematorium

Grave Details**:**

Contact at Church/Cemetery:

Details of Funeral Director**:**

Special Instructions:

**Pricing Scenario 8**

To be completed by Tenderer - for pricing evaluation purposes please complete the prices in the table below (as provided in 705616451 Schedule 2 – Schedule of Requirements).

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Item No | Description  of Service | Quantity | Price (£) – As per Schedule 2  Year 1 | Price (£) – As per Schedule 2  Year 2 | Price (£) – As per Schedule 2  Option Year 1 | Price (£)– As per Schedule 2  Option Year 2 | Total Item Price (£)  (Y1+Y2+  Op Y1+Op Y2) |
| 31 | Nabresina Limestone Urn Plot Marker Stone  To include engraving of brackets, colons, commas, full stops, hyphens, inverted commas, oblique strokes, and semi-colons.  Dimensions  304.8mm x 304.8mm x 50.8mm (12” x 12” x 2”) | 1 |  |  |  |  |  |
| 32 | Nabresina Limestone - Regimental/Service crest (actuarily reduced as required) | 1 |  |  |  |  |  |
| 33 | Nabresina Limestone - Letters and Numbers (per character)  To include Service Number, Rank, Name, Regiment/Service, Date of Death and Age. Two lines of Personal Inscription with each line to be no more than 25 symbols and spaces.  (Letters and numbers are to be incised and painted with Sign Writing Black Enamel with a Gloss Finish. All numerals to be inscribed on same level top and bottom). Height as detailed in layout drawings, either 22.2mm (7/8”), 15.8mm (5/8”) or 10.0mm (3/8”) high.  (NOTE- engraving of brackets, colons, commas, full stops, hyphens, inverted commas, oblique strokes, and semi-colons included in item 31) | 106 |  |  |  |  |  |
| 34 | Fixing/placing of a Nabresina Limestone memorial flush with the ground. |  |  |  |  |  |  |
| **Scenario 8 Total** | | | | | | |  |

To be completed by Tenderer

|  |  |
| --- | --- |
| **SCENARIO** | **SCENARIO TOTAL** |
| 1 |  |
| 2 |  |
| 3 |  |
| 4 |  |
| 5 |  |
| 6 |  |
| 7 |  |
| 8 |  |
| Grand Total | This price should be input as the Contract Price in Annex A to DEFFORM 47 and into the DSP in the Commercial Envelope |