| # Wreck/Obstruction Report |

Feature Type: | Wrecks - 5274

### Field | ### Value
Spatial Type | Point
Horizontal Datum | EPSG:4326
Wreck Number | 5274
Position | 54 57.3 N,5 44.808 W
Classification |
Wreck Category | non-dangerous wreck
Position Method |
General Depth | 35
Vertical Datum | Approximate Lowest Astronomical Tide
Depth Method |
Depth Quality | depth unknown
Conspic Visual | not visually conspicuous
Conspic Radar | not radar conspicuous
Last Amended | 20100924
Name | HOUSATONIC
Type | tanker
Flag | GB
Length | 105.8
Beam | 13.7
Draught | 8.2
Tonnage | 3893
Tonnage Type | gross
Cargo | 537
Date Sunk | 19080103
Scour Length |
Circumstances Of Loss | BUILT IN 1893. OWNED AT TIME OF LOSS BY ANGLO-AMERICAN OIL CO. PASSAGE BARROW FOR NEW YORK. STRUCK RUSSELLS ROCK, ON THE MAIDENS. FLARES WERE FIRED ONE OF WHICH FELL BACK ON SHIP STARTING A FIRE, A HUGE EXPLOSION FOLLOWED AND VESSEL SLID OFF ROCKS. 2 LIVES LOST. (DODS, SHIPWRECKS OF THE ULSTER COAST)
Surveying Details | HH100/351/12 26.9.97 WK LOCATED 1970 IN 545718N, 054448.5W. ON E & NE SIDE OF RUSSELL RK. WK LIES AGAINST ROCK FACE. STERN IN 35MTRS, BOW IN 7MTRS. NO SCOUR. SEABED ROCK & SAND. BEST DIVED HALF HOUR BEFORE LW, BELFAST. (P STEELE, 22.5.97). NCA. 24.9.10 LOCATED IN 2008 ON HIGHLANDMAN SHOAL. (HMS ENTERPRISE, HI 1273). NCA.

| # Wreck/Obstruction Report |

Feature Type: | Wrecks - 5183

### Field | ### Value
Spatial Type | Point
Horizontal Datum | EPSG:4326
Wreck Number | 5183
Position | 54 55.586 N,5 43.564 W
Classification |
Wreck Category | non-dangerous wreck
Position Method |
General Depth | 40
Vertical Datum | Approximate Lowest Astronomical Tide
Depth Method |
Depth Quality | depth unknown
Conspic Visual | not visually conspicuous
Conspic Radar | not radar conspicuous
Last Amended | 20141105
Name | OVERTON
Type | steam ship
Flag | GB
Length | 43.7
Beam | 7.4
Draught | 3.2
Tonnage | 426
Tonnage Type | gross
Cargo | 514,534
Date Sunk | 19550907
Scour Length |
Circumstances Of Loss | BUILT IN 1911 BY J T ELTRINGHAM & CO LTD, SOUTH SHIELDS. OWNED AT TIME OF LOSS BY THORNE LINE LTD. ONE BOILER, COMPOUND EXPANSION ENGINE OF 74 NHP, SINGLE SHAFT. MACHINERY AFT BY BARID BROS, NORTH SHIELDS. PASSAGE LIVERPOOL FOR COLERAINE. DROVE ASHORE AND WAS LOST IN FOG. PERCHED ON SADDLE RK, NEAR THE MAIDENS LT HO BUT WAS LATER LOST. (LL & SII).
Surveying Details | H3144/56 5.5.56 SINKING POSN GIVEN AS 545535N, 054330W. (LL & REPORT OF COURT). STS. NCA. 24.9.10 LOCATED 2008 ON MAIDEN SHOAL. (HMS ENTERPRISE, HI 1273). NCA.

| # Wreck/Obstruction Report |

Feature Type: | Wrecks - 5184

### Field | ### Value
Spatial Type | Point
Horizontal Datum | EPSG:4326
Wreck Number | 5184
Position | 54 56.002 N,5 44.064 W
Classification |
Wreck Category | dangerous wreck
Position Method |
Depth | 18
General Depth | 50
Vertical Datum | Approximate Lowest Astronomical Tide
Depth Method |
Depth Quality | least depth unknown, safe clearance at value shown
Conspic Visual | not visually conspicuous
Conspic Radar | not radar conspicuous
Last Amended | 20040123
Name | RAYLIGHT
Type | motor vessel
Flag | GB
Length | 29.6
Beam | 6.7
Draught | 3
Tonnage | 177
Tonnage Type | gross
Date Sunk | 19750804
Scour Length |
Circumstances Of Loss | PASSAGE DUNVEGAN, SKYE FOR BELFAST LOUGH. GROUNDED IN THICK FOG. SANK WITHIN 10 MINUTES. CREW PICKED UP BY THE BR FERRY ULIDIA. (LL VOL. 221)
Surveying Details | H1270/75 12.8.75 AGROUND 1M ESE OF THE MAIDENS LT, OR 545600N, 054400W. (LL, 5 & 6.8.75 & CG BANGOR TELEX DTD 4.8.75). BEARING & DISTANCE DOES NOT AGREE WITH LAT/LONG. INS AS WK USC 10FMS IN 545600N, 054400W. BR STD. 1.11.00 SHOWN AS WK USC 18MTRS ON 2198 [SEP '87 EDN]. AMEND TO WK USC PA 18MTRS. BR STD. 23.1.04 EUT POSN SUPPLIED BY GEODESY: 5456.002N, 0544.064W. NE 2198. 24.9.10 LOCATED 2008 ON MAIDEN SHOAL. (HMS ENTERPRISE, HI 1273). NFA.