| # Wreck/Obstruction Report |

Feature Type: | Wrecks - 5137

### Field | ### Value
Spatial Type | Point
Horizontal Datum | EPSG:4326
Wreck Number | 5137
Position | 54 41.865 N,5 40.361 W
Classification |
Wreck Category | dangerous wreck
Position Method | Differential Global Positioning System
Depth | 9.1
General Depth | 11
Vertical Datum | Approximate Lowest Astronomical Tide
Depth Method | found by multi-beam
Depth Quality | least depth known
Conspic Visual | not visually conspicuous
Conspic Radar | not radar conspicuous
Last Amended | 20100923
Name | TROUTPOOL
Type | steam ship
Flag | GB
Length | 118.9
Beam | 16.8
Draught | 7.9
Tonnage | 4886
Tonnage Type | gross
Cargo | 22
Date Sunk | 19400720
Sonar Length | 97.6
Sonar width | 28.2
Shadow Height | 6.9
Orientation | 45
Scour Length |
Scour Width |
Scour Depth | 001.8
Scour Orientation |
General Comments | SUPERSTRUCTURE DISPERSED
Circumstances Of Loss | BUILT 1927 BY W GRAY & CO LTD, WEST HARTLEPOOL WITH 3 CYLINDER TRIPLE EXPANSION ENGINE, WITH SINGLE SCREW, 3 BOILERS. MACHINERY BY CENTRAL MARINE ENG CO LTD., W HARTLEPOOL. OWNED AT TIME OF LOSS BY POOL SHIPPING CO., ROPNER LTD. STRUCK MINE LAID BY GERMAN AIRCRAFT. 11 OF 43 CREW LOST. STRUCK A MINE AND SANK ON PASSAGE FROM ROSARIO FOR GLASGOW. 11 LIVES WERE LOST.(DODS & SII)
Surveying Details | H0681/40 8.8.40 INS DW IN 544147N, 054027W OR 357DEGS, 1.8M FROM N EXTREMITY BANGOR POINT. (AUTHORITY NOT STATED). - FNM 1968/40. H0681/40 INS CONL LT BUOY WITH TOPMARK, GPFL(3)G.7.5S, 177DEGS 1C FROM WK. (AUTHORITY NOT STATED). - FNM 1969(T)/40. H0681/40 14.10.41 INS LT BUOY ON CHARTS. - FNM 2421/41. H0681/40 14.2.44 BEING DISPERSED. - NM 322(T)/44. H0681/40 22.11.45 AMEND TO WK 4FMS WITH LT BUOY. - NM 3786/45. H0681/40 20.7.49 AMEND TO WK 4.5FMS & AMEND POSN. (SML 7). - NM 1444/49. H0681/40 13.12.54 AMEND TO FOUL WITH LT BUOY. (AUTHORITY NOT STATED) - NM 2790/54. H0681/40 26.9.57 DELETE LT BUOY. (IRISH LTS NM 7/57). - NM 2195/57. H0991/40 7.7.60 AMEND TO WK 5.5FMS. - NM 2210/60. H3089/60 7.3.61 DISPERSED. GEN DEPTH 38FT, SCOUR 44FT. (ECES, 1960). H5605/61 8.12.61 INS AS WK 5FMS 4FT. NC 1753. H5292/71 10.8.72 NOW SHOWN AS WK 10.4MTRS. NC 1753. 9.2.79 SHOWN AS WK 10.4MTRS IN 544147N, 054019W [OGB]. NC 1411. 5.1.04 EUT POSN SUPPLIED BY GEODESY: 5441.787N, 0540.378W. NE 1753. SEP 2010/000156213 23.9.10 EXAMINED 2008 IN 5441.865N, 0540.361W [WGD] USING DGPS. LEAST M/B DEPTH 9.13MTRS. LENGTH 97.6MTRS, WIDTH 28.2MTRS, HT 6.92MTRS. LIES NE/SW. SUPERSTRUCTURE APPARENTLY BROKEN UP AND DISPERSED. (HMS ENTERPRISE, HI 1273). AMEND WK 9.1MTRS IN REVISED POSN. - NM 5218/10.

| # Wreck/Obstruction Report |

Feature Type: | Wrecks - 5133

### Field | ### Value
Spatial Type | Point
Horizontal Datum | EPSG:4326
Wreck Number | 5133
Position | 54 41.0 N,5 44.75 W
Classification |
Wreck Category | dangerous wreck
Position Method |
General Depth | 10
Vertical Datum | Approximate Lowest Astronomical Tide
Depth Method |
Depth Quality | depth unknown
Conspic Visual | not visually conspicuous
Conspic Radar | not radar conspicuous
Last Amended | 20040131
Name | EVELEEN
Type |
Tonnage Type |
Scour Length |
Circumstances Of Loss |
Surveying Details | H03681/42 6.8.43 DW IN 544100N, 054445W APPROX, MARKED BY G CAN LT BUOY. (ADMIRALTY). - NM 1665/43. H03681/42 27.11.43 WK AND BUOY REMOVED. (ADMIRALTY). DELETE FROM CHARTS.- NM 2550/43. 31.1.04 DATA RE-ASSESSED. AMENDED TO LIFT. NC 1752.