| # Wreck/Obstruction Report |

Feature Type: | Obstruction - 5278

### Field | ### Value
Spatial Type | Point
Horizontal Datum | EPSG:4326
gml parent id | fme-gen-f14a8752-0121-4ead-8cdc-0f996ad9818a
Wreck Number | 5278
Position | 54 52.953 N,5 45.113 W
Classification |
Obstruction Category | foul ground
Position Method |
General Depth | 12
Vertical Datum | Approximate Lowest Astronomical Tide
Depth Method |
Depth Quality | depth unknown
Conspic Visual | not visually conspicuous
Conspic Radar | not radar conspicuous
Last Amended | 20031126
Name | STATE OF LOUISIANA (STERN SECTION)
Type | merchant vessel
Flag | GB
Length | 91.4
Tonnage | 1869
Tonnage Type | gross
Cargo | 533,517
Date Sunk | 18781224
Scour Length |
Circumstances Of Loss | BUILT IN 1872. RAN AGROUND ON HUNTER ROCK WHILST EN-ROUTE GLASGOW TO LARNE. FOUR TUGS UNABLE TO PULL VESSEL OFF ROCK & SHE EVENTUALLY BROKE IN THREE. OWNED AT TIME OF LOSS BY STATE STEAMSHIP CO. LTD. 3 MASTED IRON VESSEL, BUILT ON CLYDE, RAN AGROUND ON HUNTER ROCKS. THE BUOY MARKING THE ROCK HAD BEEN DISPLACED AND WAS 400 YARDS FROM ITS CORRECT POSN. VESSEL WAS BADLY HOLED ON ROCKS. CREW & PASSENGERS RESCUED. WK WAS ADVERTISED FOR SALE IN JANUARY 1879, BUT EVENTUALLY BROKE UP. SHE WAS IDENTIFIED BY DIVERS IN 1966 WHO FOUND A CHAMBER POT BEARING THE COMPANY CREST. (SHIPWRECKS OF THE ULSTER COAST)
Surveying Details | HH100/351/12 26.9.97 LOCATED IN 1966. STERN SECTION LIES NE OF SHOALEST POINT OF HUNTER ROCK, IN 545257N, 054503W. SEABED SAND. NO SCOUR. AN ABUNDANCE OF FISH & SEALIFE ON WK. (P STEELE, 22.5.97). INS AS FOUL. BR STD. 5.8.03 EUT POSN SUPPLIED BY GEODESY: 5452.953N, 0545.113W. NE 1237. 24.9.10 LOCATED 2008 ON HUNTER SHOAL. (HMS ENTERPRISE, HI 1273). NCA.

| # Wreck/Obstruction Report |

Feature Type: | Obstruction - 5277

### Field | ### Value
Spatial Type | Point
Horizontal Datum | EPSG:4326
gml parent id | fme-gen-f14a8752-0121-4ead-8cdc-0f996ad9818a
Wreck Number | 5277
Position | 54 52.92 N,5 45.163 W
Classification |
Obstruction Category | foul ground
Position Method |
General Depth | 16
Vertical Datum | Approximate Lowest Astronomical Tide
Depth Method |
Depth Quality | depth unknown
Conspic Visual | not visually conspicuous
Conspic Radar | not radar conspicuous
Last Amended | 20031126
Name | STATE OF LOUISIANA (BOW SECTION)
Type | merchant vessel
Flag | GB
Length | 91.4
Tonnage | 1869
Tonnage Type | gross
Cargo | 533,517
Date Sunk | 18781224
Scour Length |
Circumstances Of Loss | BUILT IN 1872. RAN AGROUND ON HUNTER ROCK WHILST EN-ROUTE GLASGOW TO LARNE. FOUR TUGS UNABLE TO PULL VESSEL OFF ROCK & SHE EVENTUALLY BROKE IN THREE. OWNED AT TIME OF LOSS BY STATE STEAMSHIP CO. LTD. 3 MASTED IRON VESSEL, BUILT ON CLYDE, RAN AGROUND ON HUNTER ROCKS. THE BUOY MARKING THE ROCK HAD BEEN DISPLACED AND WAS 400 YARDS FROM ITS CORRECT POSN. VESSEL WAS BADLY HOLED ON ROCKS. CREW & PASSENGERS RESCUED. WK WAS ADVERTISED FOR SALE IN JANUARY 1879, BUT EVENTUALLY BROKE UP. SHE WAS IDENTIFIED BY DIVERS IN 1966 WHO FOUND A CHAMBER POT BEARING THE COMPANY CREST. (SHIPWRECKS OF THE ULSTER COAST)
Surveying Details | HH100/351/12 26.9.97 VESSEL LOCATED IN 1966. BOW & MIDSHIPS SECTION LIE TO SW OF SHOALEST POINT OF HUNTER ROCK, IN 545255N, 054506W. NO SCOUR. SEABED SAND. AN ABUNDANCE OF FISH & SEALIFE ON THE WK. (P STEELE, 22.5.97). INS AS FOUL. BR STD. 5.8.03 EUT POSN SUPPLIED BY GEODESY: 5452.920N, 0545.163W. NE 1237. 24.9.10 LOCATED 2008 ON HUNTER SHOAL. (HMS ENTERPRISE, HI 1273). NCA.

| # Wreck/Obstruction Report |

Feature Type: | Wrecks - 3619

### Field | ### Value
Spatial Type | Point
Horizontal Datum | EPSG:4326
Wreck Number | 3619
Position | 55 7.763 N,6 2.31 W
Classification |
Wreck Category | dangerous wreck
Position Method | Compass Bearing and Radar Range
Depth | 4.2
General Depth | 5
Vertical Datum | Approximate Lowest Astronomical Tide
Depth Method | found by diver
Depth Quality | least depth known
Conspic Visual | not visually conspicuous
Conspic Radar | not radar conspicuous
Last Amended | 19781218
Name | CLEMENTINE
Type |
Tonnage Type |
Scour Length |
Circumstances Of Loss |
Surveying Details | POSN 550730N, 060200W OR 65 DEGS 2.5CABLES FROM CHURCH AT CUSHENDEN. (AUTHORITY NOT KNOWN). H6683/33 14.11.33 INS WK 2.5FMS IN 550747N, 060215W. (AUTHORITY NOT KNOWN). - NM ACTION. H01746/44 11.4.44 NOW WK 14FT AT 075DEG 1700FT FROM CUSHENDEN CHURCH. (HMS SCOTT). BR STD. 21.6.73 AMEND TO WK 4.2. NC 2199.

| # Wreck/Obstruction Report |

Feature Type: | Wrecks - 3618

### Field | ### Value
Spatial Type | Point
Horizontal Datum | EPSG:4326
Wreck Number | 3618
Position | 55 7.0 N,6 2.0 W
Classification |
Wreck Category | dangerous wreck
Position Method |
General Depth | 7
Vertical Datum | Approximate Lowest Astronomical Tide
Depth Method |
Depth Quality | depth unknown
Conspic Visual | not visually conspicuous
Conspic Radar | not radar conspicuous
Last Amended | 20091112
Name | ESLINGTON FIRTH
Type | steam ship
Flag | GB
Tonnage | 351
Tonnage Type | gross
Cargo | 5
Date Sunk | 19230225
Scour Length |
Circumstances Of Loss | BUILT IN 1920 IN SOUTH SHIELDS. OWNED AT TIME OF LOSS BY CHEVIOT COASTERS. ONE BOILER, COMPOUND EXPANSION ENGINE, SINGLE SHAFT. PASSAGE MARYPORT FOR LONDONDERRY. WENT ASHORE AND ENGINE ROOM & STOKEHOLD FILLED WITH WATER. BECAME CTL. (SIBI). RAN ASHORE 2M N OF CUSHENDUN. (DIVISIONAL OFFICER, BALLYCASTLE).
Surveying Details | H1594/23 ASHORE IN 550700N, 060200W. (DIVISIONAL OFFICER, BALLYCASTLE). NCA. 25.4.23 SALVAGE IN PROGRESS (LL 25.4.23). NCA.

| # Wreck/Obstruction Report |

Feature Type: | Wrecks - 3620

### Field | ### Value
Spatial Type | Point
Horizontal Datum | EPSG:4326
Wreck Number | 3620
Position | 55 9.783 N,6 1.667 W
Classification |
Wreck Category | dangerous wreck
Position Method |
General Depth | 1
Vertical Datum | Approximate Lowest Astronomical Tide
Depth Method |
Depth Quality | depth unknown
Conspic Visual | not visually conspicuous
Conspic Radar | not radar conspicuous
Last Amended | 20091112
Name | SAINT RONAIG
Type |
Flag | GB
Tonnage | 504
Tonnage Type | gross
Date Sunk | 19551214
Scour Length |
Circumstances Of Loss |
Surveying Details | H4572/56 15.8.56 ST IN 550947N, 060140W. (HMS COOK, HN). INS AS ST.- NM 1973/56. H4572/56 29.11.56 WK HAS BROKEN UP. (MOT AND IRISH LTS). DELETED. BR STD.

| # Wreck/Obstruction Report |

Feature Type: | Wrecks - 5273

### Field | ### Value
Spatial Type | Point
Horizontal Datum | EPSG:4326
Wreck Number | 5273
Position | 54 51.15 N,5 44.293 W
Classification |
Wreck Category | dangerous wreck
Position Method |
General Depth | 1
Vertical Datum | Approximate Lowest Astronomical Tide
Depth Method |
Depth Quality | depth unknown
Conspic Visual | not visually conspicuous
Conspic Radar | not radar conspicuous
Last Amended | 20011127
Name | AILSA
Type | steam ship
Flag | GB
Length | 30.5
Tonnage Type |
Cargo | 517
Date Sunk | 18920226
Scour Length |
General Comments | BADLY BROKEN UP
Circumstances Of Loss | VESSEL, EX-ROSE, BUILT 1867, RAN AGROUND 1M N OF MUCK ISLAND, WHILST ON HER REGULAR ROUTE BETWEEN AYR & BELFAST WITH GENERAL CARGO & 1 PASSENGER. OWNED AT TIME OF LOSS BY AYR SHIPPING CO. (SHIPWRECKS OF THE ULSTER COAST & P STEELE)
Surveying Details | HH100/351/12 29.5.97 AILSA, FIRST LOCATED BY DIVERS IN 1965, IN 545109N, 054414W. BADLY BROKEN UP, LYING IN SHALLOW WATER, IN GEN DEPTH 3MTRS. PART OF WK CAN BE SEEN LYING ON THE SHORE ABOVE MHW. NO SCOUR. SEABED ROCK & KELP. CAN BE DIVED AT ANY STATE OF TIDE. (P STEELE, 22.5.97) PLOTS CLOSE INSHORE INSIDE DANGER LINE IN AREA OF UNDERWATER ROCKS. NCA. 5.8.03 WGD POSN SUPPLIED BY GEODESY: 5451.153N, 0544.296W. NCA.

| # Wreck/Obstruction Report |

Feature Type: | Wrecks - 5192

### Field | ### Value
Spatial Type | Point
Horizontal Datum | EPSG:4326
Wreck Number | 5192
Position | 54 57.7 N,5 55.0 W
Classification |
Wreck Category | non-dangerous wreck
Position Method |
General Depth | 10
Vertical Datum | Approximate Lowest Astronomical Tide
Depth Method |
Depth Quality | depth unknown
Conspic Visual | not visually conspicuous
Conspic Radar | not radar conspicuous
Last Amended | 20141105
Name | HMS THRUSH
Type | gunboat
Flag | GB
Length | 50.3
Beam | 9.4
Tonnage | 805
Tonnage Type | displacement
Date Sunk | 19170411
Scour Length |
General Comments | SCATTERED WRECKAGE
Circumstances Of Loss | BUILT IN 1889 BY SCOTTS SHIPBUILDING, GREENOCK. SHE WAS ASIGNED TO THE COASTGUARD (1906), THEN A CABLE SHIP (1915) & FINALLY A SALVAGE SHIP. RAN AGROUND DURING A SNOWSTORM NEAR GLENARM, N. IRELAND. (SHIPS OF THE ROYAL NAVY)
Surveying Details | H1245/69 20.10.69 REMAINS LIE SOME 50YDS FROM THE SHORE IN DEPTHS OF 30-40FT AND CONSIST OF SCATTERED WRECKAGE. (K.BIALOWAS, DIVE REPORT DTD 11.10.69). POSN 545742N, 055500W FOR FILING ONLY.

| # Wreck/Obstruction Report |

Feature Type: | Wrecks - 5209

### Field | ### Value
Spatial Type | Point
Horizontal Datum | EPSG:4326
Wreck Number | 5209
Position | 54 50.9 N,5 43.0 W
Classification |
Wreck Category | dangerous wreck
Position Method |
General Depth | 15
Vertical Datum | Approximate Lowest Astronomical Tide
Depth Method |
Depth Quality | depth unknown
Conspic Visual | not visually conspicuous
Conspic Radar | not radar conspicuous
Last Amended | 20100924
Type | submarine
Tonnage Type |
Scour Length |
Circumstances Of Loss |
Surveying Details | H5983/82 26.10.82 WK (SUB) SHOWN IN 545049N, 054154W [OGB] ON KINGFISHER TRAWLING PLOTS A-PLOT 17 [1982]. POSN FOR FILING ONLY. NCA. 24.9.10 LOCATED 2008 CLOSE IN TO THE ISLE OF MUCK. (HMS ENTERPRISE, HI 1273). FILING POSN AMENDED TO 5450.9N, 0543.0W. NCA.