|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Elms Field** | | | | | | | | | | | | | |
|  | | | | | | | | | | | | | |
|  | **Frequency Schedule** | | | | | | | | | | | | |
| **Description of works required** | **Jul** | **Aug** | **Sep** | **Oct** | **Nov** | **Dec** | **Jan** | **Feb** | **Mar** | **Apr** | **May** | **Jun** | **Total** |
| Cut all amenity grassed areas and play area grass, to include all edges, footpaths & paved areas and to clear of cuttings after each cut **Note:** Cuttings to be removed from site | 2 | 2 | 2 | 2 | 1 | 1 | 1 | 2 | 2 | 2 | 2 | 2 | **21** |
| Prior to grass cutting: litter and debris to be removed. | 2 | 2 | 2 | 2 | 1 | 1 | 1 | 2 | 2 | 2 | 2 | 2 | **21** |
| Strim around all fixed obstacles, benches, dog bins, waste bins, re-cycling bins, streetlights, manhole/inspection covers, utility boxes and play area equipment | 2 | 2 | 2 | 2 | 1 | 1 | 1 | 2 | 2 | 2 | 2 | 2 | **21** |
| Footpath/paved edges to be reinstated, to avoid grass encroachment. |  |  |  | 1 |  |  |  |  |  | 1 |  |  | **2** |
| Wildflower beds to be cut after natural seeding. |  |  | 1 |  |  |  |  |  | 1 |  |  |  | **2** |
| Autumn pick up/leaf collection from amenity areas **Note:** leaves to be removed from site |  |  |  |  | 1 |  |  |  |  |  |  |  | **1** |
| Autumn pick up/leaf collection from play area **Note:** leaves to be removed from site. |  |  |  |  | 1 | 1 |  |  |  |  |  |  | **2** |
|  | | | | | | | | | | | | | |
| **Comments:**  Amenity grass areas to be cut 25 mm height in spring/summer and 50 mm height in autumn/winter.  Wildflower beds to be cut 100 mm in height.  All arisings to be removed. | | | | | | | | | | | | | |