|  |  |  |  |
| --- | --- | --- | --- |
|  | **SCHEDULE OF WORKS / PRICING DOCUMENT** | **TENDER 1** TARMAC | **TENDER 2** POLYMERIC |
|  | **Employer’s requirements** | Tennis courts with 2-year warranty, minimum 10-year design life.  | MUGA with 5-year warranty, minimum 10-year design life (see item 14)  |
| **1** | Site set up including, security, welfare, storage and fencing and removal on completion, allowing for leaving site clear and clean. |  |  |
| **2** | Create new access if required for equipment, allowing for full reinstatement on completion. |  |  |
| **3** | Clean surface to remove all moss and debris, remove all net post sockets and remove detritus from site. Apply environmentally friendly weed killer. |  |  |
| **4** | Repair court where root damaged, removing root and reinstating sub-base and existing asphalt. |  |  |
| **5** | Excavate to perimeter of court to allow for feathering of new surface, but mandating minimum thickness, OR provide additional up-stand kerbs. |  |  |
| **6** | Form drilled drainage holes at 450mm centres and fill with pea shingle |  |  |
| **7** | Provide and install four sets of galvanised sockets to receive four new galvanised and painted posts, minimum 600mm deep. |  |  |
| **8** | Repair as necessary existing perimeter fencing to playground end to lower 300mm and to playground end projection below lower 1000mm (the existing full perimeter fence is assumed to remain throughout works). |  |  |
| **9** | Provide tack coat and lay 6mm porous macadam with minimum compacted thickness of 25mm. |  |  |
| **10** | Provide two layers of porous acrylic spray, colours to be agreed. |  | N/A |
| **11** | White line two courts, setting out to be as agreed sole drawings. |  | N/A |
| **12** | Provide and lay to porous polymeric base with minimum compacted thickness of 12mm. | N/A |  |
| **13** | Provide two coats of porous polyurethane wearing surface, colours to be agreed. | N/A |  |
| **14** | Paint in contrasting colours lines for tennis, mini tennis, netball and basketball, all for competitive purposes. Paint for community use/training football, hockey and walking football pitches. All to be as agreed scaled drawings. | N/A |  |
| **15** | Preliminaries - items as required by Conditions of Contract and on/off site overheads. |  |  |
| **16** | Profit. |  |  |
|  | **FIXED** **SUM TOTAL exc. VAT** | **£** | **£** |