EFW Expressions of Interest

City of Wolverhampton Council own and operate an Energy from Waste plant within the city to dispose of its residual waste. The plant is located at Crown Street, Wolverhampton, WV1 1QB.

An opportunity has arisen for the council to offer to the market its spare capacity. We are looking for expressions of interest from companies who would like further discussions with the council about the opportunity to dispose of waste at the facility commencing in March 2024.

A total tonnage capacity of 4,000 tonnes per month may be available and the council are considering the sale of this capacity either as a single allowance, or smaller lots for 6 to 9 month period.

If you would be interested in exploring this opportunity please let us know by contacting Karen Boden by the published closing date.

The waste acceptance criteria for the plant are as follows:

|  |  |  |
| --- | --- | --- |
| 19 12 wastes from the mechanical treatment of waste (for example sorting, crushing, compacting, pelletising) not otherwise specified |  |  |
| **19 12 12 other wastes (including mixtures of materials) from mechanical treatment of wastes other than those mentioned in 19 12 11**  (not accepted 19 12 11\* other wastes (including mixtures of materials) from mechanical treatment of waste containing dangerous substances ) | Non-Haz |  |
| 20 03 Other Municipal Wastes |  |  |
| **20 03 01 Mixed Municipal Waste** | Non-Haz |  |

All items are required to be less than 1m².

* Plastics and rubber shall be accepted as long as the proportion or quantity within each tipped load is no more than 7% and it can still be classified as European Waste Catalogue (EWC) codes 19 12 12 or 20 03 01.
* All waste delivered shall be unbaled and unwrapped.
* The Net Calorific Value (NCV) of all waste supplied must be within 8 – 11 MJ/kg.
* Waste delivered shall be as dry as possible and shall be reasonably protected from the outside elements to prevent excessive build-up of water and moisture. Moisture content of waste delivered shall be no greater than 32%.