Appendix 10

Planting Schedule

Manor Grove Wheelie Bin Enclosure

|  |  |  |
| --- | --- | --- |
| **Plant Schedule per Bin Store**All plants shall comply to the National Plant Specification and shall be supplied in accordance with the HTA Trade Specification Scheme and be from a Certified Nursery Supplier.  | **Pot size** | **No. required per Bin Store based on 20 linear metres of planting** |
| Viburnum davidii | 5lt  | 12 |
| Skimmia Japonica ‘Rubella’ | 5lt | 12 |
| Hebe ‘Red Edge’ | 5lt | 12 |
| Polygonatum odoratum | 3lt | 12 |
| Trillium flexipes | 3lt | 12 |
| Mahonia aquifolium ‘Apollo’ | 5lt | 12 |
| Sorcococca hookeriana var humilis | 5lt | 12 |

* Perennial weeds shall be dug out.
* Shrubs shall be planted in groups at approximately 3 m² and in groups of three of the same type.
* Shrub beds should have a well formed with a defined edge between the bed and surrounding grass areas.
* All arisings to be disposed off site to authorised tip or recycling centre.
* Cultivate and grade shrub bed; manual clearance of herbaceous weeds, including all roots and perennial weeds. Bring top 300mm of topsoil to a fine tilth. Shrub beds shall be free from weeds, moss and litter. Remove stones and deleterious material over 50mm.
* Plant shrubs in to holes average 300 x 300 x 300 deep. Back fill with excavated material incorporating soil conditioner and general fertiliser.
* Water to field capacity and mulch with 50mm of soil conditioner.
* Maintain for 12 months. To include watering and weeding.
* Replace failed plants prior to handover.