{"text_format":"1","workbook":"xlsx","n_sheets":2,"sheets":["Schedule B Works","Schedule C Works"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Schedule B Works","index":0,"n_rows":31,"n_cols":5,"rows_kept":31,"cut":false,"hidden":false,"merged":[]}
["Level","Item","Bill description","Unit","Rate £)"]
[1,"4.3","0500 - Drainage and Service Ducts",""]
["c","4.3.1","Gullies",""]
[null,"4.3.1.1","Gully Emptying, including clearing aprons, covers and obstructions","no"]
[null,"4.3.1.2","Clear gully aprons, covers and obstructions","no"]
["c","4.3.2","Linear drainage systems",""]
[null,"4.3.2.1","Clearing, rodding, low pressure / high volume jetting and proving Combined Kerb and Drainage System","m"]
[null,"4.3.2.2","Clearing, rodding, jetting and proving Linear Drainage Channels (slot drains)","m"]
[null,"4.3.2.3","Remove debris, obstructions and sweep formed concrete drainage channel (concrete 'V' channel)","m"]
["c","4.3.3","Grips and counterfort drains",""]
[null,"4.3.3.1","Clear weed/vegetation growth and debris, clear, recut drainage Grip inlet and non piped drainage Grip","no."]
[null,"4.3.3.2","Clear weed/vegetation growth and debris clearing, rodding, jetting and proving of drainage Grip inlet and piped drainage Grip","no."]
[null,"4.3.3.3","Clear weed/vegetation growth and debris, clear, recut Counterfort drains","no."]
["c","","Catch Pits",""]
[null,"4.3.4","Clear weed / vegetation growth around frames, clear,  empty silt and debris from Catch Pits","no."]
["c","","Ditches",""]
[null,"4.3.5","Clear ditches by removing all material that could impair operation (weed / vegetation growth, silt, debris/rubbish, or eroded banks where present that impede flow and impair operation)","m"]
["c","","Outfalls, including infiltration tanks/stilling basins and/or settlement ponds",""]
[null,"4.3.6","Clear outfalls by removing all material that could impair operation (Headwalls, Pipe outfall)","no."]
["c","","Interceptors",""]
[null,"4.3.7","Clear weed / vegetation growth, around frames, clear, empty trapped material from Interceptors","no."]
["c","","Manholes",""]
[null,"4.3.8","Clear manholes by removing all material that could impair operation (overgrown vegetation / weed, silt, debris / rubbish)","no."]
["c","","Culverts",""]
[null,"4.3.9","De-silt and remove all material that could impair operation (silt, weed / vegetation growth, debris / rubbish, eroded bank material restricting the free flow of water through the culvert)","no."]
["c","4.3.10","Filter drains",""]
[null,"4.3.11.1","Edge scrape, clear weed / vegetation growth, cut back to remove build up of material from edge of carriage way through to filter material (Filter Drain and Combined carrier and Filter drain) that could impair operation","m"]
[null,"4.3.11.2","Weed spray along Filter Drain and Combined carrier and Filter drain","m"]
[]
[]
[null,null,"Note: There are no uplifts applicable for Night or Weekend Working for these works"]

{"sheet":"Schedule C Works","index":1,"n_rows":126,"n_cols":5,"rows_kept":126,"cut":false,"hidden":false,"merged":[]}
["Level","Item","Bill description","Unit","Rate (£)"]
[1,"","SERIES 500 DRAINAGE AND SERVICE DUCTS (Scope Paragraph 18.4.3)",""]
["c","","Cleaning Existing Drainage Systems",""]
["c","","Cleaning; piped drainage system; accessed from pavements, footways and/or paved areas not requiring all-terrain vehicles; not exceeding 20 metres;",""]
[null,"16","Internal diameter not exceeding nominal 150mm.","m"]
[null,"17","Internal diameter exceeding nominal 150mm but not exceeding nominal 225mm.","m"]
[null,"18","Internal diameter exceeding nominal 225mm but not exceeding nominal 300mm.","m"]
[null,"19","Internal diameter exceeding nominal 300mm but not exceeding nominal 450mm.","m"]
["c","","Cleaning; piped drainage system; accessed from pavements, footways and/or paved areas not requiring all-terrain vehicles; exceeding 20 metres but not exceeding 50 metres;",""]
[null,"20","Internal diameter not exceeding nominal 150mm.","m"]
[null,"21","Internal diameter exceeding nominal 150mm but not exceeding nominal 225mm.","m"]
[null,"22","Internal diameter exceeding nominal 225mm but not exceeding nominal 300mm.","m"]
[null,"23","Internal diameter exceeding nominal 300mm but not exceeding nominal 450mm.","m"]
["c","","Cleaning; piped drainage system; accessed from pavements, footways and/or paved areas not requiring all-terrain vehicles; exceeding 50 metres but not exceeding 100 metres;",""]
[null,"24","Internal diameter not exceeding nominal 150mm.","m"]
[null,"25","Internal diameter exceeding nominal 150mm but not exceeding nominal 225mm.","m"]
[null,"26","Internal diameter exceeding nominal 225mm but not exceeding nominal 300mm.","m"]
[null,"27","Internal diameter exceeding nominal 300mm but not exceeding nominal 450mm.","m"]
["c","","Cleaning; piped drainage system; accessed from pavements, footways and/or paved areas not requiring all-terrain vehicles; exceeding 100 metres;",""]
[null,"28","Internal diameter not exceeding nominal 150mm.","m"]
[null,"29","Internal diameter exceeding nominal 150mm but not exceeding nominal 225mm.","m"]
[null,"30","Internal diameter exceeding nominal 225mm but not exceeding nominal 300mm.","m"]
[null,"31","Internal diameter exceeding nominal 300mm but not exceeding nominal 450mm.","m"]
["c","","Cleaning; piped drainage system; accessed from pavements, footways and/or paved areas requiring all-terrain vehicles; not exceeding 20 metres;",""]
[null,"32","Internal diameter not exceeding nominal 150mm.","m"]
[null,"33","Internal diameter exceeding nominal 150mm but not exceeding nominal 225mm.","m"]
[null,"34","Internal diameter exceeding nominal 225mm but not exceeding nominal 300mm.","m"]
[null,"35","Internal diameter exceeding nominal 300mm but not exceeding nominal 450mm.","m"]
["c","","Cleaning; piped drainage system; accessed from pavements, footways and/or paved areas requiring all-terrain vehicles; exceeding 20 metres but not exceeding 50 metres;",""]
[null,"36","Internal diameter not exceeding nominal 150mm.","m"]
[null,"37","Internal diameter exceeding nominal 150mm but not exceeding nominal 225mm.","m"]
[null,"38","Internal diameter exceeding nominal 225mm but not exceeding nominal 300mm.","m"]
[null,"39","Internal diameter exceeding nominal 300mm but not exceeding nominal 450mm.","m"]
["c","","Cleaning; piped drainage system; accessed from pavements, footways and/or paved areas requiring all-terrain vehicles; exceeding 50 metres but not exceeding 100 metres;",""]
[null,"40","Internal diameter not exceeding nominal 150mm.","m"]
[null,"41","Internal diameter exceeding nominal 150mm but not exceeding nominal 225mm.","m"]
[null,"42","Internal diameter exceeding nominal 225mm but not exceeding nominal 300mm.","m"]
[null,"43","Internal diameter exceeding nominal 300mm but not exceeding nominal 450mm.","m"]
["c","","Cleaning; piped drainage system; accessed from pavements, footways and/or paved areas requiring all-terrain vehicles; exceeding 100 metres;",""]
[null,"44","Internal diameter not exceeding nominal 150mm.","m"]
[null,"45","Internal diameter exceeding nominal 150mm but not exceeding nominal 225mm.","m"]
[null,"46","Internal diameter exceeding nominal 225mm but not exceeding nominal 300mm.","m"]
[null,"47","Internal diameter exceeding nominal 300mm but not exceeding nominal 450mm.","m"]
["c","","Cleaning; catchpits; accessed from pavements, footways and/or paved areas not requiring all-terrain vehicles; not exceeding 3 number;",""]
[null,"48","All sizes.","no"]
["c","","Cleaning; catchpits; accessed from pavements, footways and/or paved areas not requiring all-terrain vehicles; exceeding 3 number bit not exceeding 10 number;",""]
[null,"49","All sizes.","no"]
["c","","Cleaning; catchpits; accessed from pavements, footways and/or paved areas not requiring all-terrain vehicles; exceeding 10 number;",""]
[null,"50","All sizes.","no"]
["c","","Cleaning; manholes; accessed from pavements, footways and/or paved areas not requiring all-terrain vehicles; not exceeding 3 number;",""]
[null,"51","Rectangular or square chambers not exceeding 1000mm in length.","no"]
[null,"52","Internal diameter not exceeding 1500mm.","no"]
[null,"53","Internal diameter exceeding 1500mm but not exceeding 2100mm.","no"]
[null,"54","Internal diameter exceeding 2100mm.","no"]
["c","","Cleaning; manholes; accessed from pavements, footways and/or paved areas not requiring all-terrain vehicles; exceeding 3 number bit not exceeding 10 number;",""]
[null,"55","Rectangular or square chambers not exceeding 1000mm in length.","no"]
[null,"56","Internal diameter not exceeding 1500mm.","no"]
[null,"57","Internal diameter exceeding 1500mm but not exceeding 2100mm.","no"]
[null,"58","Internal diameter exceeding 2100mm.","no"]
["c","","Cleaning; manholes; accessed from pavements, footways and/or paved areas not requiring all-terrain vehicles; exceeding 10 number;",""]
[null,"59","Rectangular or square chambers not exceeding 1000mm in length.","no"]
[null,"60","Internal diameter not exceeding 1500mm.","no"]
[null,"61","Internal diameter exceeding 1500mm but not exceeding 2100mm.","no"]
[null,"62","Internal diameter exceeding 2100mm.","no"]
["c","","Cleaning; manholes; accessed from pavements, footways and/or paved areas requiring all-terrain vehicles; not exceeding 3 number;",""]
[null,"63","Rectangular or square chambers not exceeding 1000mm in length.","no"]
[null,"64","Internal diameter not exceeding 1500mm.","no"]
[null,"65","Internal diameter exceeding 1500mm but not exceeding 2100mm.","no"]
[null,"66","Internal diameter exceeding 2100mm.","no"]
["c","","Cleaning; manholes; accessed from pavements, footways and/or paved areas requiring all-terrain vehicles; exceeding 3 number bit not exceeding 10 number;",""]
[null,"67","Rectangular or square chambers not exceeding 1000mm in length.","no"]
[null,"68","Internal diameter not exceeding 1500mm.","no"]
[null,"69","Internal diameter exceeding 1500mm but not exceeding 2100mm.","no"]
[null,"70","Internal diameter exceeding 2100mm.","no"]
["c","","Cleaning; manholes; accessed from pavements, footways and/or paved areas requiring all-terrain vehicles; exceeding 10 number;",""]
[null,"71","Rectangular or square chambers not exceeding 1000mm in length.","no"]
[null,"72","Internal diameter not exceeding 1500mm.","no"]
[null,"73","Internal diameter exceeding 1500mm but not exceeding 2100mm.","no"]
[null,"74","Internal diameter exceeding 2100mm.","no"]
["c","","Cleaning; gullies; all locations; not exceeding 20 number;",""]
[null,"75","All sizes.","no"]
["c","","Cleaning; gullies; all locations; exceeding 20 number but not exceeding 50 number;",""]
[null,"76","All sizes.","no"]
["c","","Cleaning; gullies; all locations; exceeding 50 number but not exceeding 100 number;",""]
[null,"77","All sizes.","no"]
["c","","Cleaning; gullies; all locations; exceeding 100 number;",""]
[null,"78","All sizes.","no"]
["c","","Cleaning; gully covers and aprons; all locations; not exceeding 20 number;",""]
[null,"79","All sizes.","no"]
["c","","Cleaning; gully covers and aprons; all locations; exceeding 20 number but not exceeding 50 number;",""]
[null,"80","All sizes.","no"]
["c","","Cleaning; gully covers and aprons; all locations; exceeding 50 number but not exceeding 100 number;",""]
[null,"81","All sizes.","no"]
["c","","Cleaning; gully covers and aprons; all locations; exceeding 100 number;",""]
[null,"82","All sizes.","no"]
["c","","Cleaning; Interceptors; all locations; not exceeding 20 number;",""]
[null,"83","All sizes.","no"]
["c","","Cleaning; Interceptors; all locations; exceeding 20 number but not exceeding 50 number;",""]
[null,"84","All sizes.","no"]
["c","","Cleaning; Interceptors; all locations; exceeding 50 number but not exceeding 100 number;",""]
[null,"85","All sizes.","no"]
["c","","Cleaning; Interceptors; all locations; exceeding 100 number;",""]
[null,"86","All sizes.","no"]
["c","","Cleaning; Soakaways; Priority soakaways; all locations;",""]
[null,"87","Volume not exceeding 50m3","m3"]
[null,"88","Volume exceeding 50m3 in steps of 50m3","m3"]
["c","","Cleaning; Soakaways; Non priority soakaways; all locations;",""]
[null,"89","Volume not exceeding 50m3","m3"]
[null,"90","Volume exceeding 50m3 in steps of 50m3","m3"]
[]
["c","","Drainage (repair defects, not resulting from an incident caused by a third party) and Disposal of Waste",""]
["c","","Drainage (repair defects, not resulting from an incident caused by a third party)",""]
[null,"161","Gully emptier including driver and operative.","hr"]
[null,"162","Vactor unit including driver and operative.","hr"]
[null,"163","CCTV unit including technician.","hr"]
["c","","Disposal of waste;",""]
[null,"164","Inert waste.","t"]
[null,"165","Wet waste gully emptying arisings.","t"]
[null,"166","Wet waste drainage arisings.","t"]
[null,"167","Green waste.","t"]
[]
[]
[null,null,"Note: Above rates are based on Mon to Fri 0700-1900hrs"]
[]
[null,null,"Out of Hours Uplift for Night Working (Mon to Fri 1900-0700hrs)","%"]
[null,null,"Out of Hours Uplift for Weekend Working (0700hrs on Sat to 0700 on Mon)","%"]