| # Wreck/Obstruction Report |

Feature Type: | Obstruction - 2113

### Field | ### Value
Spatial Type | Point
Horizontal Datum | EPSG:4326
gml parent id | fme-gen-91784790-6dd7-4ea6-b514-8f95dd00b0db
Wreck Number | 2113
Position | 57 49.882 N,3 37.487 W
Classification |
Obstruction Category | foul ground
Position Method |
General Depth | 22
Vertical Datum | Approximate Lowest Astronomical Tide
Depth Method |
Depth Quality | depth unknown
Conspic Visual | not visually conspicuous
Conspic Radar | not radar conspicuous
Last Amended | 20031118
Name | ROLYN
Type | fishing vessel
Flag | GB
Length | 7.6
Tonnage Type |
Date Sunk | 19841227
Scour Length |
Circumstances Of Loss | REPORTED TAKING IN WATER. LATER WAS ABANDONED, WHEN ENGINE STOPPED, AND SANK.
Surveying Details | H1270/85 13.2.85 SANK IN 574954N, 033724W. (MORAY CG, TLX DTD 28.12.84). NCA. 18.11.03 INS AS FOUL. BR STD.

| # Wreck/Obstruction Report |

Feature Type: | Obstruction - 76540

### Field | ### Value
Spatial Type | Point
Horizontal Datum | EPSG:4326
gml parent id | fme-gen-91784790-6dd7-4ea6-b514-8f95dd00b0db
Wreck Number | 76540
Position | 57 35.546 N,4 3.206 W
Classification |
Obstruction Category |
Position Method | Differential Global Positioning System
Depth | -2.9
General Depth | -1
Vertical Datum | Approximate Lowest Astronomical Tide
Depth Method |
Depth Quality | least depth known
Conspic Visual | not visually conspicuous
Conspic Radar | not radar conspicuous
Last Amended | 20100920
Type |
Tonnage Type |
Sonar Length | 24
Sonar width | 7
Orientation | 170
Scour Length |
General Comments | MINOR AREA OF DRYING DEBRIS
Circumstances Of Loss |
Surveying Details | HH091/336/01 20.9.10 EXAM'D 20.6.10 IN 5735.5463N, 0204.2062W [WGD] USING RTK GPS. LEAST DEPTH DRIES 2.87MTRS IN GEN DEPTH DRIES 1.07MTRS. LENGTH 24MTRS, WIDTH 7MTRS. LIES 170/350 DEGS. FRAMES INDICATE WK IS UPRIGHT, CABIN/WHEELHOUSE LIES ON ITS SIDE TO THE EAST. EXPOSED AFTER HALF-TIDE. (MMT, HI 1336). AREA OF DEBRIS. INS AS OBSTN DRIES 2.9MTRS. BR STD.

| # Wreck/Obstruction Report |

Feature Type: | Obstruction - 2078

### Field | ### Value
Spatial Type | Point
Horizontal Datum | EPSG:4326
gml parent id | fme-gen-91784790-6dd7-4ea6-b514-8f95dd00b0db
Wreck Number | 2078
Position | 57 43.482 N,3 39.687 W
Classification |
Obstruction Category |
Position Method |
General Depth | 52
Vertical Datum | Approximate Lowest Astronomical Tide
Depth Method |
Depth Quality | depth unknown
Conspic Visual | not visually conspicuous
Conspic Radar | not radar conspicuous
Last Amended | 20031117
Type | Equipment
Tonnage Type |
Scour Length |
Circumstances Of Loss |
Surveying Details | 11.5.71 POSSIBLE OBSTN AT A DEPTH OF 55MTRS. MARKED BY YELLOW BUOY FLG. (MV WHITETHORN 7 LL 11.5.71). NCA, POSN FOR FILING ONLY.

| # Wreck/Obstruction Report |

Feature Type: | Obstruction - 2107

### Field | ### Value
Spatial Type | Point
Horizontal Datum | EPSG:4326
gml parent id | fme-gen-91784790-6dd7-4ea6-b514-8f95dd00b0db
Wreck Number | 2107
Position | 57 41.183 N,3 41.986 W
Classification |
Obstruction Category | foul ground
Position Method | DECCA navigator
General Depth | 48
Vertical Datum | Approximate Lowest Astronomical Tide
Depth Method |
Depth Quality | depth unknown
Conspic Visual | not visually conspicuous
Conspic Radar | not radar conspicuous
Last Amended | 19950822
Name | BRIAR
Type | fishing vessel
Flag | GB
Tonnage Type |
Scour Length |
Circumstances Of Loss |
Surveying Details | H1310/84/40 14.11.84 REPORTED BY LOCAL FISHERMAN TO LIE IN 57412N, 034154W. POSN BY DECCA. NO HAZARD AS PRAWN NETS ARE DRAGGED OVER IT WITHOUT SNAGGING. (B GREIG). INS AS FOUL. BR STD.

| # Wreck/Obstruction Report |

Feature Type: | Obstruction - 2131

### Field | ### Value
Spatial Type | Point
Horizontal Datum | EPSG:4326
gml parent id | fme-gen-91784790-6dd7-4ea6-b514-8f95dd00b0db
Wreck Number | 2131
Position | 57 37.1 N,3 54.518 W
Classification |
Obstruction Category | foul ground
Position Method |
General Depth | 18
Vertical Datum | Approximate Lowest Astronomical Tide
Depth Method |
Depth Quality | depth unknown
Conspic Visual | not visually conspicuous
Conspic Radar | not radar conspicuous
Last Amended | 20031122
Type | Anchor
Tonnage Type |
Scour Length |
Circumstances Of Loss | LOST FROM 'PACIFIC HORIZON'. (MRCC ABERDEEN)
Surveying Details | HH266/420/03 27.11.97 ANCHOR LOST IN 573706.75N, 035425.95W [OGB]. (MRCC ABERDEEN, TLX DTD 21.11.97). CHART AS FOUL. BR STD. 22.11.03 EUT POSN: 5737.100N, 0354.518W. NE 1077.

| # Wreck/Obstruction Report |

Feature Type: | Obstruction - 64108

### Field | ### Value
Spatial Type | Point
Horizontal Datum | EPSG:4326
gml parent id | fme-gen-91784790-6dd7-4ea6-b514-8f95dd00b0db
Wreck Number | 64108
Position | 57 41.991 N,3 29.438 W
Classification |
Obstruction Category |
Position Method |
General Depth | -2
Vertical Datum | Approximate Lowest Astronomical Tide
Depth Method |
Depth Quality | depth unknown
Conspic Visual | not visually conspicuous
Conspic Radar | not radar conspicuous
Last Amended | 20040225
Type |
Tonnage Type |
Scour Length |
General Comments | SEE ALSO [2123]
Circumstances Of Loss |
Surveying Details | 15.11.90 OBS (DRIES) SHOWN IN 574201N, 032923W & 574200.5N, 032921W [OGB] ON PHOTOPLOT PG 199 - FC7 DTD 9.7.86. OBS APPEAR TO BE CONCRETE BLOCKS WASHED FROM THE WALL. THEY COULD EASILY HAVE MOVED SINCE PHOTO WAS TAKEN. NE 1462. HH266/410/07 13.2.04 OBSTNS STILL PRESENT. THEY ARE OLD TANK TRAPS FROM WW2. (K STRATTON, MORAY COUNCIL, LTR DTD 2.2.04). NCA. 25.2.04 EUT POSN: 5741.991N, 0329.438W. NE 1462.

| # Wreck/Obstruction Report |

Feature Type: | Obstruction - 2123

### Field | ### Value
Spatial Type | Point
Horizontal Datum | EPSG:4326
gml parent id | fme-gen-91784790-6dd7-4ea6-b514-8f95dd00b0db
Wreck Number | 2123
Position | 57 42.0 N,3 29.472 W
Classification |
Obstruction Category |
Position Method | Air photography
General Depth | -2
Vertical Datum | Approximate Lowest Astronomical Tide
Depth Method |
Depth Quality | depth unknown
Conspic Visual | not visually conspicuous
Conspic Radar | not radar conspicuous
Last Amended | 20040225
Type |
Tonnage Type |
Scour Length |
General Comments | SEE ALSO [64108]
Circumstances Of Loss |
Surveying Details | 15.11.90 OBS (DRIES) SHOWN IN 574201N, 032923W & 574200.5N, 032921W [OGB] ON PHOTOPLOT PG 199 - FC7 DTD 9.7.86. OBS APPEAR TO BE CONCRETE BLOCKS WASHED FROM THE WALL. THEY COULD EASILY HAVE MOVED SINCE PHOTO WAS TAKEN. NE 1462. HH266/410/07 13.2.04 OBSTNS STILL PRESENT. THEY ARE OLD TANK TRAPS FROM WW2. (K STRATTON, MORAY COUNCIL, LTR DTD 2.2.04). NCA. 25.2.04 EUT POSN: 5742.000N, 0329.472W. NE 1462.

| # Wreck/Obstruction Report |

Feature Type: | Obstruction - 70487

### Field | ### Value
Spatial Type | Point
Horizontal Datum | EPSG:4326
gml parent id | fme-gen-91784790-6dd7-4ea6-b514-8f95dd00b0db
Wreck Number | 70487
Position | 57 44.8 N,3 39.7 W
Classification |
Obstruction Category | foul ground
Position Method |
General Depth | 47
Vertical Datum | Approximate Lowest Astronomical Tide
Depth Method |
Depth Quality | depth unknown
Conspic Visual | not visually conspicuous
Conspic Radar | not radar conspicuous
Last Amended | 20070926
Type |
Tonnage Type |
Scour Length |
General Comments | ABANDONED FISHING GEAR
Circumstances Of Loss |
Surveying Details | SEP 2007/000069054 26.9.07 FISHING GEAR ABANDONED IN 5744.80N, 0339.70W [WGD]. UNMARKED & WILL NOT BE RECOVERED. (MRCC ABERDEEN, UKHO EMAIL DTD 22.9.07). INS AS FOUL. BR STD. SEP 2009/000031675 29.4.09 INS BY NM. - NM 2601/09.

| # Wreck/Obstruction Report |

Feature Type: | Obstruction - 2129

### Field | ### Value
Spatial Type | Point
Horizontal Datum | EPSG:4326
gml parent id | fme-gen-91784790-6dd7-4ea6-b514-8f95dd00b0db
Wreck Number | 2129
Position | 57 37.983 N,3 46.086 W
Classification |
Obstruction Category | foul ground
Position Method |
General Depth | 2
Vertical Datum | Approximate Lowest Astronomical Tide
Depth Method |
Depth Quality | depth unknown
Conspic Visual | not visually conspicuous
Conspic Radar | not radar conspicuous
Last Amended | 20020710
Name | LAUREL
Type | fishing vessel
Flag | GB
Length | 18.3
Tonnage Type |
Date Sunk | 19960418
Scour Length |
General Comments | WOODEN HULL
Circumstances Of Loss | CONVERTED WOODEN TRAWLER WENT AGROUND AFTER BECOMING ENTANGLED IN LOBSTER POTS. VESSEL BECAME HOLED. LATER BROKE UP.
Surveying Details | HH266/420/02 22.4.96 AGROUND IN 573800N, 034600W [OGB]. WILL BREAK UP OVERNIGHT. (MRCC ABERDEEN, TLX DTD 19.4.96). 22.4.96 STILL IN SAME POS'N. BREAKING UP QUICKLY. (MRCC ABERDEEN, TELECON 22.4.96). INS AS FOUL. BR STD.

| # Wreck/Obstruction Report |

Feature Type: | Wrecks - 2076

### Field | ### Value
Spatial Type | Point
Horizontal Datum | EPSG:4326
Wreck Number | 2076
Position | 57 42.466 N,3 39.037 W
Classification |
Wreck Category | non-dangerous wreck
Position Method | HI-FIX Parabolic or Hydrotrac
Depth | 53
General Depth | 54
Vertical Datum | Approximate Lowest Astronomical Tide
Depth Method | found by echo-sounder
Depth Quality | least depth known
Conspic Visual | not visually conspicuous
Conspic Radar | not radar conspicuous
Last Amended | 20031117
Name | GUIDING LIGHT
Type | fishing vessel
Flag | GB
Tonnage Type |
Scour Length |
Scour Width |
Scour Depth | 001.0
Scour Orientation |
Circumstances Of Loss |
Surveying Details | H4734/63 20.1.64 LIES IN 574449N, 033356W. POSN BY DECCA. (LT CDR J RALPH RNR). 1.12.70 INS AS NDW. LC 115. H454/67 10.8.76 EXAM'D 31.7.75 IN 574239N, 033857W [OGB] USING HIFIX [2 LOP]. LEAST E/S DEPTH 53 IN GEN DEPTH 54MTRS. SCOUR 55MTRS. (HMS ECHO, HI 80/75). BR STD. 21.12.84 THIS IS FV GUIDING LIGHT. (B GREIG, TELECON).

| # Wreck/Obstruction Report |

Feature Type: | Wrecks - 2104

### Field | ### Value
Spatial Type | Point
Horizontal Datum | EPSG:4326
Wreck Number | 2104
Position | 57 41.373 N,3 47.548 W
Classification |
Wreck Category | non-dangerous wreck
Position Method | Global Positioning System
Depth | 35
General Depth | 42
Vertical Datum | Approximate Lowest Astronomical Tide
Depth Method | found by echo-sounder
Depth Quality | least depth known
Conspic Visual | not visually conspicuous
Conspic Radar | not radar conspicuous
Last Amended | 20031118
Type | aircraft
Tonnage Type |
Shadow Height | 7
Scour Length |
Circumstances Of Loss | REPORTED AS A SUNDERLAND. PRESUMED TO HAVE CRASHED DURING WWII.
Surveying Details | H3060/79 29.9.81 LOCATED 6.8.81 IN 574125N, 034727W. DCS3 HT 7MTRS IN GEN DEPTH 42MTRS. BELIEVED TO BE AN AIRCRAFT. MANY SCOUR MARKS ON SEABED. (PALMER, EAE MARINE SURVEY, 25.8.81). INS AS WK 35MTRS. BR STD. H1310/84/40 15.11.84 LOCATED IN 574126N, 034720W USING DECCA. (B. GREIG). NCA. HH100/351/01 22.11.89 LOCATED IN CHARTED POSN AND DIVED ON. PART OF AIRCRAFT WING FOUND CONTAINING TWO ENGINE COWLINGS. THEREFORE CANNOT BE FROM A WELLINGTON BOMBER. (HMS CHALLENGER, 27.10.89). HH100/351/145 5.8.99 DIVED IN 5741.373, 0347.548W [WGD] USING GPS. FOUR ENGINE COWLINGS LOCATED TOGETHER WITH CIRCULAR WINDOWS. CONSIDERED TO BE THE WK OF SUNDERLAND AIRCRAFT. LARGE PIECES OF FUSELAGE REMAINING BUT THE WINGS HAVE BEEN WELL DAMAGED BY TRAWLERS. LIES ON TOP OF MUDDY SLOPE. MAX HT 5MTRS IN GEN DEPTH 51MTRS. (J LEIGH/B HUMBY, LTR DTD 24.7.99). NCA.

| # Wreck/Obstruction Report |

Feature Type: | Wrecks - 2070

### Field | ### Value
Spatial Type | Point
Horizontal Datum | EPSG:4326
Wreck Number | 2070
Position | 57 40.501 N,3 49.948 W
Classification |
Wreck Category | dangerous wreck
Position Method | Global Positioning System
Depth | 26.5
General Depth | 36
Vertical Datum | Approximate Lowest Astronomical Tide
Depth Method | swept by wire-drag
Depth Quality | least depth known
Conspic Visual | not visually conspicuous
Conspic Radar | not radar conspicuous
Last Amended | 20130515
Name | HMSM TANTIVY AND BARGE
Type | submarine
Flag | GB
Length | 77.4
Tonnage Type |
Date Sunk | 1951
Shadow Height | 11
Orientation | 0
Scour Length |
Scour Width |
Scour Depth | 002.0
Scour Orientation |
General Comments | UPRIGHT & INTACT, BARGE 50MTRS N, HT BY DIVER
Circumstances Of Loss | SCUTTLED FOR USE AS A SONAR TARGET.
Surveying Details | NO PREVIOUS RECORD. 17.6.75 NDW SHOWN IN 574033N, 034942W ON BA 3547. (AUTHORITY UNKNOWN). H454/67 30.7.75 LOCATED IN 574030N, 035000W. SWEPT CLEAR AT 26.6MTRS. LEAST E/S DEPTH 27.3MTRS. (SOISS, SIGNAL DTD 11.7.75). AMEND TO SW 14FMS. - NM 192/76. H454/67 9.8.76 EXAM'D 28.7.75 IN 574030N, 035000W [OGB] USING HIFIX [2 LOP]. SWEPT CLEAR AT 26.6, FOUL AT 27.6MTRS. LEAST E/S DEPTH 28.2 IN GEN DEPTH 36MTRS. SCOUR DEPTH 38MTRS. SEABED OF SAND & BROKEN SHELL. 137MTRS LONG, LYING N/S. (HMS ECHO, HI 80/75). AMEND TO SW 14FMS 3FT. BR STD. 11.5.78 AMEND TO SW 26.6MTRS. NC 223. 21.11.84 REPORTED TO BE WK OF A BARGE BY DIVER - MR SPITTAL. (NAVAL LAW, TELECON). 23.7.85 REPD TO BE WRECK OF HMS TANTIVY. LYING UPRIGHT & INTACT IN 574027N, 034942W. POSN BY DECCA. STANDS 30FT HIGH. (MR GRIEG, TELECON). 12.8.85 APPLICATION TO PURCHASE WK MADE BY A. HARDWICK. (NRE 31B/2695). HH100/351/01 28.8.89 TWO WKS DIVED ON IN THIS APPROX POSN. A) A BARGE, APPROX 150FT LONG & COVERED WITH OLD PRAWN FISHING NETS PREVENTING FURTHER EXAMINATION, IN 574018N, 034930W. POSN BY DECCA. ABOUT 50MTRS S IS B) WK OF SUBMARINE. LIES UPRIGHT & INTACT EXCEPT THAT BRIDGE APPEARS TO HAVE BEEN STRIPPED & TORPEDO TUBES REMOVED. (SGT J LEIGH, RAF KINLOSS, 10.8.89). AMEND TO SW WKS 26.5MTRS. BR STD. HH100/351/01 22.11.89 LOCATED IN CHARTED POSN. IN A GENERALLY GOOD CONDITION AND SITTING UPRIGHT, COVERED IN NETS. BARGE WAS NOT FOUND DESPITE EXTENSIVE DIVER, CAMERA AND SHORT RANGE HIGH DEFINITION SONAR SEARCH. (HMS CHALLENGER, 27.10.89). NCA. HH100/351/07 10.6.93 DIVED ON IN 574029N, 035002W [WGD] USING GPS. STANDS 11MTRS HIGH IN SCOUR 2MTRS DEEP. (J LEIGH, 27.4.93). NCA.

| # Wreck/Obstruction Report |

Feature Type: | Wrecks - 2036

### Field | ### Value
Spatial Type | Point
Horizontal Datum | EPSG:4326
Wreck Number | 2036
Position | 57 36.283 N,4 1.833 W
Classification |
Wreck Category | dangerous wreck
Position Method | Differential Global Positioning System
General Depth | 2
Vertical Datum | Approximate Lowest Astronomical Tide
Depth Method |
Depth Quality | depth unknown
Conspic Visual | not visually conspicuous
Conspic Radar | not radar conspicuous
Last Amended | 20100920
Name | CLAN MACDONALD
Type |
Tonnage Type |
Scour Length |
Circumstances Of Loss | NO RECORD OF VESSEL OF THIS NAME LOST IN THIS AREA IN ANY LOSS BOOKS HELD.
Surveying Details | H6025/23 WK IN 573618N, 040145W, 2.5M NE FORT GEORGE. H2671/76 10.3.76 SEARCHED FOR BY TRANSIT SONAR [MS47] NO CONTACTS OBTAINED. (HMS ENTERPRISE, JULY 1975, HI 82 & 83/75. ROS 31.1.76). FOR FILING ONLY. NCA. HH091/336/01 20.9.10 NOT LOCATED. (MMT, HI 1336). AMEND DEAD. NCA.

| # Wreck/Obstruction Report |

Feature Type: | Wrecks - 2066

### Field | ### Value
Spatial Type | Point
Horizontal Datum | EPSG:4326
Wreck Number | 2066
Position | 57 35.983 N,3 53.085 W
Classification |
Wreck Category | dangerous wreck
Position Method |
General Depth | 6
Vertical Datum | Approximate Lowest Astronomical Tide
Depth Method |
Depth Quality | depth unknown
Conspic Visual | not visually conspicuous
Conspic Radar | not radar conspicuous
Last Amended | 20031117
Name | ROBINA
Type | fishing vessel
Tonnage Type |
Date Sunk | 19571209
Scour Length |
General Comments | HULK
Circumstances Of Loss |
Surveying Details | H6703/57 3.1.58 DERELICT DRIFTED ASHORE ABOUT ONE MILE WEST OF NAIRN. (CROMARTY CG AND DISTRICT OFFICER PETERHEAD). NCA.

| # Wreck/Obstruction Report |

Feature Type: | Wrecks - 2074

### Field | ### Value
Spatial Type | Point
Horizontal Datum | EPSG:4326
Wreck Number | 2074
Position | 57 41.782 N,3 52.585 W
Classification |
Wreck Category | dangerous wreck
Position Method | HI-FIX Parabolic or Hydrotrac
Depth | 21.5
General Depth | 23
Vertical Datum | Approximate Lowest Astronomical Tide
Depth Method | found by echo-sounder
Depth Quality | least depth known
Conspic Visual | not visually conspicuous
Conspic Radar | not radar conspicuous
Last Amended | 20031117
Type |
Tonnage Type |
Sonar Length | 30
Scour Length |
Scour Width |
Scour Depth | 000.8
Scour Orientation |
Circumstances Of Loss |
Surveying Details | H454/67 9.8.76 EXAM'D 29.7.75 LOCATED IN 574148N, 035230W [OGB] USING HIFIX [2 LOP]. LEAST E/S DEPTH 21.8 IN GEN DEPTH 23.6MTRS. SEABED FINE SAND & BROKEN SHELL. LIES NE/SW. ABOUT 30MTRS LONG. (HMS ECHO, HI 80/75). INS AS WK 21.5MTRS. BR STD.

| # Wreck/Obstruction Report |

Feature Type: | Wrecks - 2105

### Field | ### Value
Spatial Type | Point
Horizontal Datum | EPSG:4326
Wreck Number | 2105
Position | 57 38.65 N,3 48.119 W
Classification |
Wreck Category | dangerous wreck
Position Method | DECCA navigator
General Depth | 24
Vertical Datum | Approximate Lowest Astronomical Tide
Depth Method |
Depth Quality | depth unknown
Conspic Visual | not visually conspicuous
Conspic Radar | not radar conspicuous
Last Amended | 19950822
Name | RONA
Type | fishing vessel
Flag | GB
Length | 15.2
Tonnage | 25
Tonnage Type | gross
Date Sunk | 19810929
Scour Length |
General Comments | INTACT, MAST STAND 18MTRS HIGH
Circumstances Of Loss | CAUGHT FIRE, WAS ABANDONED AND SANK. (LL).
Surveying Details | H3060/79 6.10.81 INVERGORDON LIFEBOAT LOST SIGHT OF RONA IN 573700N, 035100W, WHERE IT IS PRESUMED TO HAVE SUNK. (LL 30.9.81). INS AS DWPA. - NM 2503/81. H1310/84/40 14.11.84 DIVED IN 573840N, 034802W USNG DECCA. LIES IN SCOUR IN GEN DEPTH 24MTRS. HULL EXTENSIVELY DAMAGED BY FIRE, BUT REMAINS INTACT AND STANDS ABOUT 3MTRS ABOVE SEABED. MASTS STAND ABOUT 18MTRS HIGH. (B GRIEG). AMEND TO DW IN REVISED POSN. - NM 3279/84.

| # Wreck/Obstruction Report |

Feature Type: | Wrecks - 2124

### Field | ### Value
Spatial Type | Point
Horizontal Datum | EPSG:4326
Wreck Number | 2124
Position | 57 38.816 N,3 46.069 W
Classification |
Wreck Category | non-dangerous wreck
Position Method |
General Depth | 10
Vertical Datum | Approximate Lowest Astronomical Tide
Depth Method |
Depth Quality | depth unknown
Conspic Visual | not visually conspicuous
Conspic Radar | not radar conspicuous
Last Amended | 20140801
Name | RUBICON
Type | yacht
Flag | GB
Length | 10.4
Tonnage Type |
Date Sunk | 19901217
Scour Length |
General Comments | GRP HULL
Circumstances Of Loss | CAUGHT FIRE AND SANK.
Surveying Details | HH226/350/01 10.1.91 SANK IN 573850N, 034559W. (MRCC ABERDEEN, TLX DTD 17.12.90). INS AS NDW PA. BR STD.

| # Wreck/Obstruction Report |

Feature Type: | Wrecks - 2121

### Field | ### Value
Spatial Type | Point
Horizontal Datum | EPSG:4326
Wreck Number | 2121
Position | 57 41.649 N,3 30.588 W
Classification |
Wreck Category | dangerous wreck
Position Method |
General Depth | 4
Vertical Datum | Approximate Lowest Astronomical Tide
Depth Method |
Depth Quality | depth unknown
Conspic Visual | not visually conspicuous
Conspic Radar | not radar conspicuous
Last Amended | 20031118
Name | ESPIRANS
Type | fishing vessel
Flag | GB
Tonnage Type |
Scour Length |
General Comments | WOODEN HULL
Circumstances Of Loss | CAUGHT FIRE. ABANDONED BY CREW. FIRE EXTINGUISHED. VESSEL TOWED TO AND ANCHORED IN BURGHEAD BAY. LATER SANK, PRESUMABLY AT ANCHOR.
Surveying Details | HH268/350/01 8.2.90 ANCHORED IN BURGHEAD BAY WITHIN 0.25 MILES FROM THE BEACH AND 0.5 MILE FROM THE HARBOUR. (LL 25.10.89). SUNK IN BURGHEAD BAY. PURCHASED FROM INSURERS BY MR G ROBERTSON WHO ADVISED VESSEL IS TOO DEEP TO SALVAGE. (LL 18.1.90). NCA.

| # Wreck/Obstruction Report |

Feature Type: | Wrecks - 65359

### Field | ### Value
Spatial Type | Point
Horizontal Datum | EPSG:4326
Wreck Number | 65359
Position | 57 41.07 N,3 40.11 W
Classification |
Wreck Category | dangerous wreck
Position Method |
Depth | 11
General Depth | 16
Vertical Datum | Approximate Lowest Astronomical Tide
Depth Method |
Depth Quality | depth known
Conspic Visual | not visually conspicuous
Conspic Radar | not radar conspicuous
Last Amended | 20041216
Type | Vehicle
Tonnage Type |
Scour Length |
Circumstances Of Loss | LOST DURING REHEARSAL FOR NORMANDY 'D DAY' LANDINGS.
Surveying Details | HH310/590/03 16.12.04 VALENTINE TANK EXISTS IN 5741.07N, 0340.11W [WGD]. (MR JOHNSTON, FV RESTLESS WAVE, VIA FOSNI'S LTR DTD 9.12.04). INS AS WK 11MTRS. - NM 327/05.

| # Wreck/Obstruction Report |

Feature Type: | Wrecks - 65362

### Field | ### Value
Spatial Type | Point
Horizontal Datum | EPSG:4326
Wreck Number | 65362
Position | 57 40.68 N,3 39.644 W
Classification |
Wreck Category | dangerous wreck
Position Method |
Depth | 3
General Depth | 8
Vertical Datum | Approximate Lowest Astronomical Tide
Depth Method |
Depth Quality | depth known
Conspic Visual | not visually conspicuous
Conspic Radar | not radar conspicuous
Last Amended | 20041216
Type | Vehicle
Tonnage Type |
Scour Length |
Circumstances Of Loss | LOST DURING REHEARSAL FOR NORMANDY 'D DAY' LANDINGS.
Surveying Details | HH310/590/03 16.12.04 VALENTINE TANK TRAWLED IN 5740.68N, 0339.644W [WGD]. DAMAGE TO FISHING GEAR. (MR JOHNSTON, FV RESTLESS WAVE, VIA FOSNI'S LTR DTD 9.12.04). INS AS WK 3MTRS. - NM 327/05.

| # Wreck/Obstruction Report |

Feature Type: | Wrecks - 70371

### Field | ### Value
Spatial Type | Point
Horizontal Datum | EPSG:4326
Wreck Number | 70371
Position | 57 39.51 N,3 50.99 W
Classification |
Wreck Category | non-dangerous wreck
Position Method |
Depth | 25
General Depth | 32
Vertical Datum | Approximate Lowest Astronomical Tide
Depth Method |
Depth Quality | least depth unknown, safe clearance at value shown
Conspic Visual | not visually conspicuous
Conspic Radar | not radar conspicuous
Last Amended | 20081111
Name | ELLIE MAY
Type | fishing vessel
Flag | GB
Length | 9
Beam | 3
Tonnage Type |
Scour Length |
Circumstances Of Loss | 7.8.07 REPORTED OVERDUE 7.8.07. LATER LOCATED. CREW OF 1 LOST BUT BODY RECOVERED.
Surveying Details | SEP 2007/000061334 28.8.07 FV 'ELLIE MAY' REPORTED OVERDUE 7.8.07. RED HULL, WHITE WHEELHOUSE, STEEL HULL, LENGTH 9MTRS, BEAM 3MTRS. REPORT OF 17.8.07 FROM FV 'WESTERLY WARRIOR' REPORTED SNAGGED NETS & TRACES OF OIL IN 5739.5N, 0350.9W [WGD]. SUBSEQUENTLY FOLLOW BY CONFIRMATION FROM ECHO SOUNDER OF PREVIOUSLY UNKNOWN OBJECT. (ABERDEEN CG, FAX DTD 17.8.07). 28.8.07 EXCLUSION ZONE OF 250MTRS BEING ESTABLISHED AROUND POSN 5739.51N, 0350.99W [WGD]. (MAIB DIRECTION 1/07, E-MAIL DTD 24.8.07). WAIT FURTHER. FOR FILING ONLY. NCA. 19.9.07 LIES IN 5739.51N, 0350.99W [WGD]. LIES UPRIGHT. HT TO TOP OF VHE AERIAL ON FORMAST ESTIMATED AT 6MTRS. MARKED BY SMALL, FISHING MARKER BUOY AT THE STERN. LIGHT ROPES OVER WK THAT DO NOT REACH THE SURFACE. (M EVANS, MAIB, EMAIL DTD 18.9.07). COVERED BY NAV 1. NCA. 23.10.07 DECISION WHETHER TO SALVE WILL BE MADE BY RELATIVES IN THE NEXT FEW WEEKS. (M EVANS, MAIB, EMAIL DTD 22.10.07). NCA. 2.4.08 LIKELY TO BE RECOVERED MID-YEAR. (RNW HAVE CONSULTED WITH MAIB). NAV I (279/07) REMAINS IN FORCE. NCA. SEP 2008/000090583 10.11.08 OWNERS ESTIMATE VESSEL WILL BE RECOVERED MID 2009, IF AT ALL. (MAIB SOUTHAMPTON/RNW TELECON 10.11.08). INS AS WK USC 25MTRS. - NM 6704/08.

| # Wreck/Obstruction Report |

Feature Type: | Wrecks - 2126

### Field | ### Value
Spatial Type | Point
Horizontal Datum | EPSG:4326
Wreck Number | 2126
Position | 57 41.733 N,3 31.421 W
Classification |
Wreck Category | dangerous wreck
Position Method |
Depth | 4
General Depth | 7
Vertical Datum | Approximate Lowest Astronomical Tide
Depth Method | found by diver
Depth Quality | least depth known
Conspic Visual | not visually conspicuous
Conspic Radar | not radar conspicuous
Last Amended | 20031118
Type | Vehicle
Tonnage Type |
Shadow Height | 3
Scour Length |
General Comments | UPRIGHT, INTACT, HT BY DIVER
Circumstances Of Loss | LOST DURING REHEARSAL FOR NORMANDY 'D DAY' LANDINGS.
Surveying Details | HH100/351/07 10.6.93 WK OF ARMY VALENTINE TANK DIVED IN 574145N, 033120W. STANDS UPRIGHT ON FIRM SANDY BOTTOM AND STANDS 3MTRS CLEAR OF SEABED. (J LEIGH, 27.4.93). CHART AS WK 4MTRS. BR STD.

| # Wreck/Obstruction Report |

Feature Type: | Wrecks - 2114

### Field | ### Value
Spatial Type | Point
Horizontal Datum | EPSG:4326
Wreck Number | 2114
Position | 57 41.38 N,3 34.05 W
Classification |
Wreck Category | dangerous wreck
Position Method |
Depth | 6
General Depth | 8
Vertical Datum | Approximate Lowest Astronomical Tide
Depth Method | found by diver
Depth Quality | least depth known
Conspic Visual | not visually conspicuous
Conspic Radar | not radar conspicuous
Last Amended | 20041217
Type | Vehicle
Tonnage Type |
Shadow Height | 2
Scour Length |
General Comments | INTACT, HT BY DIVER
Circumstances Of Loss | LOST DURING REHEARSAL FOR NORMANDY 'D' DAY LANDINGS.
Surveying Details | H1310/85/39 11.11.85 LOCATED IN 574124N, 033406W IN GEN DEPTH 8 TO 9MTRS AT LW. STANDS APPROX 2MTRS HIGH AND IS FULL OF SILT. (SGT M R MARLE, 17.10.85). INS AS WK 6MTRS. BR STD. HH310/590/03 16.12.04 VALENTINE TANK EXISTS IN 5741.38N, 0334.05W [WGD]. (MR JOHNSTON, FV RESTLESS WAVE, VIA FOSNI'S LTR DTD 9.12.04). AMEND POSN. BR STD.

| # Wreck/Obstruction Report |

Feature Type: | Wrecks - 2108

### Field | ### Value
Spatial Type | Point
Horizontal Datum | EPSG:4326
Wreck Number | 2108
Position | 57 41.2 N,3 39.96 W
Classification |
Wreck Category | dangerous wreck
Position Method |
Depth | 12
General Depth | 16
Vertical Datum | Approximate Lowest Astronomical Tide
Depth Method | found by diver
Depth Quality | least depth known
Conspic Visual | not visually conspicuous
Conspic Radar | not radar conspicuous
Last Amended | 20041217
Type | Vehicle
Tonnage Type |
Date Sunk | 1944
Shadow Height | 3
Scour Length |
General Comments | INTACT, HT BY DIVER
Circumstances Of Loss | LOST BY ROYAL HUSSARS DURING REHEARSALS FOR NORMANDY LANDINGS.
Surveying Details | H1310/84/40 14.11.84 DIVED IN 574113N, 033952W [OGB] USING DECCA. TANK IS COMPLETE, STANDING ABOUT 3.5MTRS ABOVE SEABED. (B GREIG). INS AS NDW. BR STD. HH100/351/07 10.6.93 VALENTINE TANK DIVED ON IN 574113N, 033853W. STANDS 3MTRS CLEAR ABOVE SEABED OF FIRM HARD SAND AND SHELL. NO SCOUR. (J LEIGH, 27.4.93). AMEND TO WK 12MTRS. BR STD. HH310/590/03 16.12.04 VALENTINE TANK EXISTS IN 5741.20N, 0339.96W [WGD]. (MR JOHNSTON, FV RESTLESS WAVE, VIA FOSNI'S LTR DTD 9.12.04). AMEND POSN. BR STD.

| # Wreck/Obstruction Report |

Feature Type: | Wrecks - 2075

### Field | ### Value
Spatial Type | Point
Horizontal Datum | EPSG:4326
Wreck Number | 2075
Position | 57 41.989 N,3 51.14 W
Classification |
Wreck Category | dangerous wreck
Position Method | Differential Global Positioning System
Depth | 27
General Depth | 29
Vertical Datum | Approximate Lowest Astronomical Tide
Depth Method | found by echo-sounder
Depth Quality | least depth known
Conspic Visual | not visually conspicuous
Conspic Radar | not radar conspicuous
Last Amended | 20031117
Type | aircraft
Tonnage Type |
Sonar Length | 40
Shadow Height | 2
Scour Length |
Scour Width |
Scour Depth | 000.8
Scour Orientation |
General Comments | HT BY DIVER, OULINE OF AIRCRAFT STILL VISIBLE
Circumstances Of Loss |
Surveying Details | H454/67 9.8.76 NEW WRECK LOCATED 30.6.75 IN 574158N 035105W [OGB] USING HIFIX/6 [2 LOP]. LEAST E/S DEPTH 27.0MTRS IN GEN DEPTH 29.0MTRS. SCOUR 29.8MTRS. SEA BED BROKEN SHELL & FINE SAND. LENGTH 40MTRS. LIES E/W. (HMS ECHO, HI 80/75).INS AS WK 27MTRS. BR STD. HH100/351/14 5.8.99 DIVED IN 5741.989N, 0351.140W [WGD] USING GPS. CONFIRMED AS WK OF A SUNDERLAND AIRCRAFT. WELL BROKEN UP WITH MANY TRAWL NETS ON IT. STANDS 2MTRS PROUD OF FLAT SAND SEABED. THE OUTLINE IS STILL VISIBLE OF THE WINGS AND FUSELAGE. THE TAIL IS BROKEN OFF AND LIES ABOUT 30 FT AWAY. GEN DEPTH 35MTRS. (J LEIGH/B HUMBY, LTR DTD 24.7.99). NCA.

| # Wreck/Obstruction Report |

Feature Type: | Wrecks - 2130

### Field | ### Value
Spatial Type | Point
Horizontal Datum | EPSG:4326
Wreck Number | 2130
Position | 57 43.849 N,3 53.785 W
Classification |
Wreck Category | dangerous wreck
Position Method |
Depth | 8
General Depth | 10
Vertical Datum | Approximate Lowest Astronomical Tide
Depth Method |
Depth Quality | least depth unknown, safe clearance at value shown
Conspic Visual | not visually conspicuous
Conspic Radar | not radar conspicuous
Last Amended | 19970627
Name | LYNNE ANNE
Type | yacht
Flag | GB
Length | 6.7
Tonnage Type |
Date Sunk | 19970621
Scour Length |
Circumstances Of Loss | SANK. CREW OF 1 MADE SHORE SAFELY.
Surveying Details | HH266/420/03 27.6.97 VESSEL REPORTED TO HAVE SUNK IN PA 574418N, 035312W. (MRCC ABERDEEN, TLX DTD 22.6.97). HH266/420/03 27.6.97 LOCATED WHAT IS BELIEVED TO BE THE WK IN 574352N, 035342W. APPROX DEPTH OF WATER OVER WK WITH SONAR IS 9MTRS AT CHART DATUM. POSN IS WITHIN A SPOIL GROUND AND CLOSE TO THE THREE KINGS BUOY, NO INTENTION TO MARK WK. (COMMISSIONERS OF NORTHERN LIGHTS, FAX DTD 27.6.97). INS AS WK USC 8MTRS. - NM 2647/97.

| # Wreck/Obstruction Report |

Feature Type: | Wrecks - 2079

### Field | ### Value
Spatial Type | Point
Horizontal Datum | EPSG:4326
Wreck Number | 2079
Position | 57 44.332 N,3 45.753 W
Classification |
Wreck Category | non-dangerous wreck
Position Method | Global Positioning System
Depth | 29
General Depth | 33
Vertical Datum | Approximate Lowest Astronomical Tide
Depth Method | found by echo-sounder
Depth Quality | least depth known
Conspic Visual | not visually conspicuous
Conspic Radar | not radar conspicuous
Last Amended | 19990804
Type | aircraft
Tonnage Type |
Shadow Height | 1
Scour Length |
Scour Width |
Scour Depth | 001.0
Scour Orientation |
Circumstances Of Loss |
Surveying Details | H454/67 9.8.76 WK LOCATED 23.6.75 IN 574421N, 034540W [OGB] USING HIFIX/6 [2 LOP]. LEAST E/S DEPTH 29.2 IN GEN DEPTH 33MTRS. SCOUR DEPTH 34MTRS. DCS3 INDICATES SMALL WK LYING WITHIN ITS SCOUR. SEABED OF LIGHT GREY MUD. CONTACTED BY SONAR FROM ONE DIRECTION ONLY. (HMS ECHO, HI 80/75). CHART AS WK 29MTRS. BR STD. 12.9.91 TRAWLER REPORTED DAMAGING NETS AND TRAWLING UP PART OF AIRCRAFT IN 574426N, 034550W. (RAF KINLOSS, TELECON 12.9.91). HH100/351/06 7.6.93 DIVED IN 8.1990. WK OF SUNDERLAND FLYING BOAT. LEAST DEPTH 27MTRS. LARGE SECTION OF FUSELAGE WITH TOP DECK COCKPIT AND TAILPLANE MISSING. WINGS, FLOATS, ENGINE COWLINGS AND SUSPENSION FLAT TO SEABED. ENGINES MISSING. A FOULED FISHING NETS FLOATS UP TO 2MTRS FROM PORT WING, NEXT TO A LIVE MINE. (G WADSWORTH, 1.3.93). HH100/351/07 10.6.93 DIVED ON 574420.5N, 034546W [WGD] USING GPS. POSITIVELY IDENTIFIED AS SUNDERLAND A/C. STANDS 2MTRS HIGH. V SHALLOW SCOUR. (J LEIGH, 27.4.93). NCA. HH100/351/14 5.8.99 DIVED IN 5744.337N, 0345.771W [WGD] USING GPS. CONFIRMED AS SUNDERLAND. RISES MAX 1MTR ABOVE SEABED. (J LEIGH/B HUMBY, LTR DTD 24.7.99). NCA.

| # Wreck/Obstruction Report |

Feature Type: | Wrecks - 2127

### Field | ### Value
Spatial Type | Point
Horizontal Datum | EPSG:4326
Wreck Number | 2127
Position | 57 47.132 N,3 34.021 W
Classification |
Wreck Category | non-dangerous wreck
Position Method | DECCA navigator
General Depth | 35
Vertical Datum | Approximate Lowest Astronomical Tide
Depth Method |
Depth Quality | depth unknown
Conspic Visual | not visually conspicuous
Conspic Radar | not radar conspicuous
Last Amended | 20140801
Type | aircraft
Tonnage Type |
Scour Length |
Circumstances Of Loss |
Surveying Details | HH100/351/07 10.6.93 WRECKAGE, APPARENTLY FROM WELLINGTON BOMBER, REPORTED TRAWLED BY FISHERMEN IN 574709N, 033356W [OGB]. (J LEIGH, 27.4.93). NCA YET. 18.11.03 RECORD REVIEWED. INS AS NDW. BR STD. 18.3.04 EUT POSN: 5747.132N, 0334.021W. NE 223.

| # Wreck/Obstruction Report |

Feature Type: | Wrecks - 65378

### Field | ### Value
Spatial Type | Point
Horizontal Datum | EPSG:4326
Wreck Number | 65378
Position | 57 42.349 N,3 30.168 W
Classification |
Wreck Category | non-dangerous wreck
Position Method |
General Depth | 60
Vertical Datum | Approximate Lowest Astronomical Tide
Depth Method |
Depth Quality | depth unknown
Conspic Visual | not visually conspicuous
Conspic Radar | not radar conspicuous
Last Amended | 20140801
Name | MANXWOOD
Type | fishing vessel
Flag | GB
Tonnage Type |
Date Sunk | 19711216
Scour Length |
Circumstances Of Loss |
Surveying Details | SINKING POSN GIVEN AS 0.25 MILE NNW FROM BURGEHAD HR IN 574222N, 033008W, (LL 206 & SIGNAL, CG PETERHEAD). H2307/73 8.2.73 INS AS DW. - NM 448/73. 22.3.73 WK SALVAGED AND MOVED TO BURGHHEAD HARBOUR. AMEND LIFT. - NM 731/73.

| # Wreck/Obstruction Report |

Feature Type: | Wrecks - 2085

### Field | ### Value
Spatial Type | Point
Horizontal Datum | EPSG:4326
Wreck Number | 2085
Position | 57 49.015 N,3 36.854 W
Classification |
Wreck Category | dangerous wreck
Position Method | HI-FIX Parabolic or Hydrotrac
Depth | 26.5
General Depth | 29
Vertical Datum | Approximate Lowest Astronomical Tide
Depth Method | found by echo-sounder
Depth Quality | least depth known
Conspic Visual | not visually conspicuous
Conspic Radar | not radar conspicuous
Last Amended | 20031118
Type |
Tonnage Type |
Sonar Length | 125
Scour Length |
Circumstances Of Loss |
Surveying Details | H454/67 10.8.76 EXAM'D 30.7.75 IN 574902N, 033646W [OGB] USING HIFIX [2 LOP]. LEAST E/S DEPTH 26.9 I GEN DEPTH 29.6MTRS. NO SCOUR. SEABED SHELLS AND SMALL STONES. LENGTH APPROX 125MTRS. (HMS ECHO, HI 80/75). INS AS WK 26.5MTRS. BR STD.

| # Wreck/Obstruction Report |

Feature Type: | Wrecks - 2082

### Field | ### Value
Spatial Type | Point
Horizontal Datum | EPSG:4326
Wreck Number | 2082
Position | 57 46.549 N,3 45.619 W
Classification |
Wreck Category | dangerous wreck
Position Method | HI-FIX Parabolic or Hydrotrac
Depth | 19.1
General Depth | 31
Vertical Datum | Approximate Lowest Astronomical Tide
Depth Method | swept by wire-drag
Depth Quality | least depth known
Conspic Visual | not visually conspicuous
Conspic Radar | not radar conspicuous
Last Amended | 20041221
Name | SAN TIBURCIO
Type | tanker
Flag | GB
Length | 125.9
Beam | 16.2
Draught | 9.4
Tonnage | 5995
Tonnage Type | gross
Cargo | 503,523
Date Sunk | 19400504
Orientation | 22
Scour Length |
General Comments | IN TWO SECTIONS AT RT ANGLES. BREAKING UP
Circumstances Of Loss | MINED. BROKE IN TWO AND SANK WITHIN 45 MINUTES OF THE EXPLOSION. PASSAGE SCAPA FLOW FOR INVERGORDON. CREW OF 40 RECOVERED. (LL WW2).
Surveying Details | H0438/40 18.5.40 GREEN DAN BUOY LAID 500YDS NE OF WK. (AUTHORITY NOT KNOWN). INS AS DW. - FNM 1196/40. H0162/40 26.8.40 AMEND POSN. - FNM 2110/40. H0438/40 23.12.43 INS G CON BUOY, GP FL (3) G 15 SEC. - NM 2745/43. H0438/40 23.2.44 AMEND PERIOD OF LT TO 30 SEC. - NM 403/44. H4697/55 20.10.55 AMEND POSN OF LT BUOY. (HMS CALTON, HN). BR STD. H0438/40 3.1.58 AMEND TO WK 9FMS 2FT, WITH G CON LT BUOY GP FL (3) G, 30 SEC, CLOSE WSW IN 173 DEGS TARBET NESS LT 5.4 MILES. (DIVING SURVEY). - NM 3068/57. H0438/40 6.5.58 BUOY TO BE WITHDRAWN. AWAIT FURTHER NOTICE. (NLB NM 13/58). - NM 1418/58. H454/67 10.8.76 EXAM'D 29.5.75 IN 574634N, 034532W [OGB] USING HIFIX/6 [2 LOP]. SWEPT CLEAR AT 19.1, FOUL AT 19.8MTRS. LEAST E/S DEPTH 19.2 IN GEN DEPTH 30.7MTRS. 175MTRS LONG, LYING 022/202 DEG. EXCELLENT DCS3 TRACE SHOWS WK LYING IN TWO SECTIONS AT RIGHT ANGLES TO EACH. DIVER REPORTS WK IS ON ITS SIDE. SWEEPING ATTEMPT WAS INCONCLUSIVE DUE VERY WEAK TIDAL STREAM BUT CONSIDER CAN BE ACCEPTED WHEN E/S AND DIVING REPORT TAKEN INTO ACCOUNT. (HMS ECHO, HI 80/75). AMEND TO SW 19.1MTRS. BR STD. H1310/81/9 12.6.81 REPORTED TO BE A LARGE WK, BROKEN IN TWO JUST AFT OF MIDSHIPS. HEADING NNE. LEAST DEPTH FOUND WHILE DIVING 22MTRS (BELOW CD) IN GENERAL DEPTH 33MTRS. (H W WILLIAMS, 5.6.81). NCA. H1310/84/25 6.8.84 REGULARLY DIVED UPON. (T JONES, 27.7.84). NOW BELONGS TO PETERHEAD WASTE METAL CO. 1.11.84 HIGHEST PART OF WK STANDS 16MTRS ABOVE SEABED. (TELECON T JONES). 21.12.84 LIES UPRIGHT IN 3 PARTS, WITH ABOUT 60YDS BETWEEN EACH SECTION. DIVERS REPORT THAT OIL TANKS ARE STILL FULL. (B GREIG, TELECON). H1310/85/39 11.11.85 WK HAS STARTED TO BREAK UP OVER PAST YEAR. STILL UPRIGHT AND IN 2 PIECES. (M R MARLE, 17.10.85). HH100/351/01 28.8.89 LIES IN TWO SEPARATE SECTIONS UPRIGHT ON SEABED. BOW SECTION ABOUT 160FT LONG LIES N/S WITH BOW S AND STERN SECTION IS ALMOST AT RIGHT ANGLES TO BOW, ABOUT 30MTRS AWAY. WK IS DECAYING FAIRLY RAPIDLY. RN TEAM RECENTLY REMOVED GUN USING EXPLOSIVES AND THIS LEAD TO A LARGE AMOUNT OF OIL LEAKING FROM STERN SECTION PRESUMABLY FROM ENGINE FUEL TANKS AS CARGO TANKS ARE EMPTY. OIL TANK HATCHES IN FOR'D SECTION ALSO BLOWN OFF AND THESE TANKS NOW EMPTY. A FAIR NUMBER OF SHELL HEADS/PROJECTILES, AT LEAST 20 SEEN, REMAIN IN VICINITY OF GUN MOUNTING AND THESE CONSIDERED BY ORDNANCE DISPOSAL EXPERT TO BE VERY DANGEROUS IF REMOVED FROM THE WATER. (SGT J LEIGH, RAF KINLOSS, 10.8.89). HH100351/07 10.6.93 HWK IS NOW STARTING TO COLLAPSE. BOW SECTION SUPERSTRUCTURE IS RAPIDLY FALLING IN AND HULL PLATES ARE FALLING OFF. CENTRE OF WK IS IN 574632.5N, 034535W [WGD] USING GPS. SMALL AMOUNT OF OIL STILL LEAKING. (J LEIGH, 27.4.93). NCA.

| # Wreck/Obstruction Report |

Feature Type: | Wrecks - 2080

### Field | ### Value
Spatial Type | Point
Horizontal Datum | EPSG:4326
Wreck Number | 2080
Position | 57 45.515 N,3 40.503 W
Classification |
Wreck Category | dangerous wreck
Position Method | HI-FIX Parabolic or Hydrotrac
Depth | 26
General Depth | 26
Vertical Datum | Approximate Lowest Astronomical Tide
Depth Method | found by echo-sounder
Depth Quality | least depth known
Conspic Visual | not visually conspicuous
Conspic Radar | not radar conspicuous
Last Amended | 20031117
Type |
Tonnage Type |
Scour Length |
General Comments | SMALL WK
Circumstances Of Loss |
Surveying Details | H454/67 10.8.76 H454/67 10.8.76 EXAM'D 31.7.75 IN 574532N, 034025W [OGB] USING HIFIX [2 LOP]. LEAST E/S DEPTH 26.0 IN GEN DEPTH 26.5MTRS. SEABED SAND. THOUGHT TO BE VERY SMALL WRECK. (HMS ECHO, HI 80/75). BR STD.